**mbed-mkit\_\_FirstStepsV00\_20141111PR.docx**

|  |
| --- |
| 1. Ensure the Nordic nRF51822-mkit has latest firmware, see: **(mbed\_bl.htm == Connect with RESET Pressed)** |
| 1. Plug in the mkit, USB drive loads, open: mbed.htm **(mbed.htm == Connect without RESET Pressed)**    1. Opens: [ <https://developer.mbed.org/platforms/Nordic-nRF51822/> ] == [ <http://mbed.org/device/?code=107002161FE6E019E20F0F91> ]    2. Follow Link to FOTA: [by following this link](http://developer.mbed.org/platforms/Nordic-nRF51822-FOTA/). [ <http://developer.mbed.org/platforms/Nordic-nRF51822-FOTA/> ]    3. Load the initial FOTA image hex by copying near mbed.htm on mkit USB drive    4. If get “insufficient space then was incorrectly connected with reset pressed like step 1) |