BlueUSB
       Now get a bunch of usb or bluetooth things and plug them in
USB INIT (Controller is 1396 bytes)
HubStatusChange Hub:0 Port:1 00010101
ResetPort Hub:0 Port:1
HubStatusChange Hub:0 Port:1 00100103
Connect Hub:0 Port:1 full

Class E0 found 0A12:0001
AddEndpoint D:01 A:00 T:00 P:0040 I:00
AddEndpoint D:01 A:81 T:03 P:0010 I:01
AddEndpoint D:01 A:02 T:02 P:0040 I:01
AddEndpoint D:01 A:82 T:02 P:0040 I:01
LoadDevice 1 E0:01:01
Bluetooth inserted of 1
Local Address: 00:1B:DC:02:40:1B
CALLBACK_READY
HIDBluetooth 112
Scanning...
Status HCI_OP_ACCEPT_CONN_REQ OK
Connected on 002B
ConnectionComplete 00:26:43:64:BF:5A10000794 100003ec
listen return code ctrl socket = 0
listen return code data socket = 0
OPEN DEVICE CLASS 3: 08 05 00
From address 00:26:43:64:BF:5A : L2CAP_CONN_REQ Result 8005
Connection request scid = 197 psm = 17
Call to BTDevice Create
Connection accepted
L2CP send:  20: 2B 20 10 00 0C 00 01 00 03 01 08 00 40 00 C5 00 00 00 00 00
L2CP send:  20: 2B 20 10 00 0C 00 01 00 04 00 08 00 C5 00 00 00 01 02 A0 02
Call to BTDevice Send
L2CP send:  14: 2B 20 0A 00 06 00 C5 00 53 F4 42 03 00 00
From address 00:26:43:64:BF:5A : L2CAP_CONF_REQ Result 39349
Config request dcid = 40 flags = 00
L2CP send:  18: 2B 20 0E 00 0A 00 01 00 05 02 06 00 C5 00 00 00 00 00
From address 00:26:43:64:BF:5A : L2CAP_CONF_RSP Result 0
From address 00:26:43:64:BF:5A : L2CAP_CONN_REQ Result 38759
Connection request scid = 198 psm = 19
Call to BTDevice Create
Connection accepted
L2CP send:  20: 2B 20 10 00 0C 00 01 00 03 03 08 00 41 00 C6 00 00 00 00 00
L2CP send:  20: 2B 20 10 00 0C 00 01 00 04 01 08 00 C6 00 00 00 01 02 A0 02
OnAcceptDataSocket: Data Socket accept here
OnAcceptDataSocket: Data Socket number = 2
From address 00:26:43:64:BF:5A : L2CAP_CONF_REQ Result 5635
Config request dcid = 41 flags = 00
L2CP send:  18: 2B 20 0E 00 0A 00 01 00 05 04 06 00 C6 00 00 00 00 00
From address 00:26:43:64:BF:5A : L2CAP_CONF_RSP Result 0
Ps3Hid led 0
Call to BTDevice Send
L2CP send:  45: 2B 20 29 00 25 00 C5 00 52 01 00 00 00 00 00 00 00 00 00 02 FF 27 10 00 32 FF 27 10 00 32
 FF 27 10 00 32 FF 27 10 00 32 00 00 00 00 00
Ps3Hid rumble
Call to BTDevice Send
L2CP send:  45: 2B 20 29 00 25 00 C5 00 52 01 00 20 FF 20 FF 00 00 00 00 02 FF 27 10 00 32 FF 27 10 00 32
 FF 27 10 00 32 FF 27 10 00 32 00 00 00 00 00
124 129 130 128   0   0   0   0   0   0   0   0   0   0   0   0  534  270  114 26885
124 129 130 128   0   0   0   0   0   0   0   0   0   0   0   0  536  271  107 27141
124 129 130 128   0   0   0   0   0   0   0   0   0   0   0   0  534  271  103 17669