START

SEND XBEE OCCUPIED

ULTRASONICSONIC OCCUPIED

SEND XBEE VACANT

YES

NO

ULTRASONIC VACANT

SEND XBEE OCCUPIED

CHECK ULTRASONIC SENSOR

TRIGGER PIR SENSOR

VACANT

OCCUPIED