Back to Release page
# Release Notes for STM32L4xx HAL Drivers Copyright 2017 STMicroelectronics
## Update History ### V1.7.1 / 21-April-2017 Main Changes Maintenance Release of HAL and Low Layer drivers HAL Drivers changes HAL generic driver Add HAL_GetUIDw0(), HAL_GetUIDw1() and HAL_GetUIDw2() APIs HAL DAC driver Fix Sample & Hold configuration in case of multi-channel HAL HASH driver Fix to ensure proper DMA-based HASH processing suspension/resumption HAL PCD driver Fix USB PCD lock/unlock and flush TX fifo during device reset HAL RTC driver Add wait for synchronization in HAL_RTC_Init() to insure RTC time initialization LL Drivers changes LL ADC Fix legacy APIs LL_ADC_REG_SetTrigSource() and LL_ADC_INJ_SetTrigSource() LL DMA Write only operation on IFCR register ### V1.7.0 / 17-February-2017 Main Changes Release of HAL and Low Layer drivers to add support of STM32L496xx/STM32L4A6xx devices New DCMI, DMA2D, HASH peripherals supported in new HAL DCMI, HAL & LL DMA2D and HAL HASH drivers New CAN2 instance supported in HAL CAN Superset features device STM32L4A6xx API User Manual available (STM32L4A6xx_User_Manual.chm) HAL Drivers changes HAL DCMI driver (NEW): stm32l4xx_hal_dcmi.h/.c files HAL DMA2D driver (NEW): stm32l4xx_hal_dma2d.h/.c files HAL HASH driver (NEW): stm32l4xx_hal_hash.h/.c and extension stm32l4xx_hal_hash_ex.h/.c files The following changes done on the HAL drivers require an update on the application code based on older HAL versions HAL SD update Overall rework of the driver for a more efficient implementation Modify initialization API and structures Modify Read / Write sequences: separate transfer process and SD Cards state management Adding interrupt mode for Read / Write operations Update the HAL_SD_IRQHandler function by optimizing the management of interrupt errors Refer to the following examples in STM32CubeL4 firmware package V1.7.0 to identify the changes: BSP example and USB_Device/MSC_Standalone application HAL generic update stm32l4xx_hal_conf_template.h updated for new HAL DCMI, HAL DMA2D and HAL HASH #define HAL_DCMI_MODULE_ENABLED #define HAL_DMA2D_MODULE_ENABLED HAL_HASH_MODULE_ENABLED HAL_Delay() updated to guarantee minimum delay HAL CAN driver Add support of CAN2 instance HAL GPIO driver Add support of GPIOI port and STM32L496xx/STM32L4A6xx alternate functions HAL PWR driver Add support of GPIOI port pull-up/pull-down state in Standby and Shutdown modes HAL QSPI driver Fix QSPI_HandleTypeDef structure to handle data size as uint32_t HAL RCC driver Add new macros for new peripherals clock and reset for CAN2, DCMI, DMA2D, GPIOI and HASH Fix HAL_RCCEx_GetPeriphCLKFreq() to compute peripheral frequencies from MSI frequency Fix HAL_RCCEx_GetPeriphCLKFreq() to compute DFSDM1 frequency from PCLK2 frequency Rename some peripheral clock sources to specify the corresponding APB clock: RCC_DFSDM1CLKSOURCE_PCLK to RCC_DFSDM1CLKSOURCE_PCLK2 RCC_SWPMI1CLKSOURCE_PCLK to RCC_SWPMI1CLKSOURCE_PCLK1 RCC_LPTIMxCLKSOURCE_PCLK to RCC_LPTIMxCLKSOURCE_PCLK1 HAL RTC driver Fix wrong clear of time and date registers in HAL_RTCEx_TamperTimeStampIRQHandler() HAL SPI driver Add internal timeout to exit HAL_SPI_Abort() and HAL_SPI_Abort_IT() HAL TIM driver Fix wrong MOE disable conditions with new macro __HAL_TIM_MOE_DISABLE_UNCONDITIONALLY() HAL SWPMI driver Fix peripheral clock management sequence in HAL_SWPMI_Init() LL Drivers changes LL DMA2D driver (NEW) LL BUS Add management of new peripherals: CAN2, DCMI, DMA2D, GPIOI and HASH LL PWR For compatibility purpose accross STM32 series, rename LL_PWR_IsActiveFlag_VOSF() to LL_PWR_IsActiveFlag_VOS() LL RCC Fix LL_RCC_GetDFSDMClockFreq() to compute frequency from PCLK2 frequency LL SDMMC Add new internal functions after HAL SD rework LL TIM Fix definition of TIM break input polarity (fix values LL_TIM_BKIN_POLARITY_LOW / LL_TIM_BKIN_POLARITY_HIGH) ### V1.6.0 / 28-October-2016 Main Changes Release of HAL and Low Layer drivers to add support of STM32L451xx/STM32L452xx/STM32L462xx devices Superset features device STM32L462xx API User Manual available (STM32L462xx_User_Manual.chm) HAL Drivers changes HAL CRYP driver HAL CRYP exported macros alignment with other STM32 series to use CRYP handle address as parameter in: __HAL_CRYP_ENABLE(), __HAL_CRYP_DISABLE(), __HAL_CRYP_SET_OPERATINGMODE(), __HAL_CRYP_SET_CHAININGMODE(), __HAL_CRYP_GET_FLAG(), __HAL_CRYP_CLEAR_FLAG(), __HAL_CRYP_GET_IT_SOURCE(), __HAL_CRYP_GET_IT(), __HAL_CRYP_CLEAR_IT(), __HAL_CRYP_ENABLE_IT() and __HAL_CRYP_DISABLE_IT() HAL FLASH driver Temporary data cache deactivation on Flash programming in HAL_FLASH_Program() and HAL_FLASH_Program_IT() Flash erase in HAL_FLASHEx_Erase() and HAL_FLASHEx_Erase_IT() To insure LSB/MSB address order in C compiler assembly output, split 64-bit programming in 2 double-word write operations HAL I2C driver Fix to reset HAL I2C handle LISTEN state option in transfer direction change with HAL_I2C_Slave_Sequential_Transmit_IT() and HAL_I2C_Slave_Sequential_Receive_IT() HAL SMBUS driver Add support of Zone read/write feature thanks to new XferOptions parameter values SMBUS_OTHER_FRAME_NO_PEC, SMBUS_OTHER_FRAME_WITH_PEC, SMBUS_OTHER_AND_LAST_FRAME_NO_PEC and SMBUS_OTHER_AND_LAST_FRAME_WITH_PEC that may be used in HAL_SMBUS_Master_Transmit_IT(), HAL_SMBUS_Master_Receive_IT(), HAL_SMBUS_Slave_Transmit_IT() and HAL_SMBUS_Slave_Receive_IT() HAL RTC driver Fix race conditions on EXTI flags clearing in HAL_RTC_AlarmIRQHandler(), HAL_RTCEx_TamperTimeStampIRQHandler() and HAL_RTCEx_WakeUpTimerIRQHandler() Fix CodeSonar warnings in HAL ADC, HAL CRC, HAL CRYP, HAL I2C, HAL IRDA, HAL SMARTCARD, HAL SMBUS, HAL OPAMP, HAL RTC, HAL UART, HAL USART LL Drivers changes LL I2C driver Add I2C4 management in LL_I2C_DeInit() LL SYSTEM driver Application shall be responsible to write the correct key sequence in SYSCFG_SKR register prior to call LL_SYSCFG_EnableSRAM2Erase() LL TIM driver New APIs to insure BDTR register initialization in a single write operation LL_TIM_BDTR_StructInit() LL_TIM_BDTR_Init() LL UTILS driver Fix LL_RCC_PLLSOURCE_HSE in LL_PLL_ConfigSystemClock_HSE() ### V1.5.2 / 12-September-2016 HAL Drivers changes HAL ADC driver No need to configure number of discontinuous conversions if discontinuous mode is not enabled HAL_ADCEx_MultiModeConfigChannel() returns HAL_ERROR if no Slave instance defined HAL DAC driver Fix calibration with correct handling of DAC_SR_CAL_FLAGx bits in HAL_DACEx_SelfCalibrate() HAL FLASH driver Change in HAL_FLASHEx_OBGetConfig() to not return PCROP and/or WRP data if their respective areas are not defined Fix error management in HAL_FLASH_IRQHandler() to simply call HAL_FLASH_OperationErrorCallback() instead of calling both HAL_FLASH_EndOfOperationCallback() and HAL_FLASH_OperationErrorCallback() HAL I2C driver Fix wrong state check in HAL_I2C_Master_Sequential_Transmit_IT() Add new option I2C_FIRST_AND_NEXT_FRAME to manage a sequencewith start condition, address and data to transfer without a final stop condition allowing successive calls to HAL_I2C_Master_Sequential_Transmit_IT() HAL IRDA driver Add transfer abort functions and associated callbacks in interrupt mode HAL_IRDA_Abort(), HAL_IRDA_AbortTransmit(), HAL_IRDA_AbortReceive() HAL_IRDA_Abort_IT(), HAL_IRDA_AbortTransmit_IT(), HAL_IRDA_AbortReceive_IT() HAL_IRDA_AbortCpltCallback(), HAL_IRDA_AbortTransmit CpltCallback(), HAL_IRDA_AbortReceive CpltCallback() IRQ Handler + DMA model optimizations HAL RTC driver Fix missing wakeup flag clear in HAL_RTCEx_SetWakeUpTimer_IT() HAL SMARTCARD driver Add transfer abort functions and associated callbacks in interrupt mode HAL_SMARTCARD_Abort(), HAL_SMARTCARD_AbortTransmit(), HAL_SMARTCARD_AbortReceive() HAL_SMARTCARD_Abort_IT(), HAL_SMARTCARD_AbortTransmit_IT(), HAL_SMARTCARD_AbortReceive_IT() HAL_SMARTCARD_AbortCpltCallback(), HAL_SMARTCARD_AbortTransmit CpltCallback(), HAL_SMARTCARD_AbortReceive CpltCallback() IRQ Handler + DMA model optimizations HAL SMBUS driver Fix issue on last data reception in host or device modes HAL SPI driver USE_SPI_CRC compilation define added to provide the mean to optimize the HAL SPI driver when CRC feature is not used (when CRC is used, application must be changed to set USE_SPI_CRC in stm32l4xx_hal_conf.h (see Inc\stm32l4xx_hal_conf_template.h)) Add transfer abort functions and associated callbacks in interrupt mode HAL_SPI_Abort() HAL_SPI_Abort_IT() HAL_SPI_AbortCpltCallback() HAL SWPMI driver Fix SWPMI peripheral errors management in DMA (resort to HAL_DMA_Abort_IT() and DMA XferAbortCallback in HAL_SWPMI_IRQHandler()) HAL UART driver New APIs to abort UART tranfer with associated callbacks added HAL_UART_Abort(), HAL_UART_AbortTransmit(), HAL_UART_AbortReceive(), HAL_UART_Abort_IT(), HAL_UART_AbortTransmit_IT(), HAL_UART_AbortReceive_IT(), HAL_UART_AbortCpltCallback(), HAL_UART_AbortTransmitCpltCallback() and HAL_UART_AbortReceiveCpltCallback() HAL USART driver New APIs to abort USART tranfer with associated callbacks added HAL_USART_Abort(), HAL_USART_Abort_IT() and HAL_USART_AbortCpltCallback() LL Drivers changes LL COMP driver Fix LL_COMP_INPUT_PLUS_IO3 definition ### V1.5.1 / 31-May-2016 HAL Drivers changes HAL ADC driver Bypass multimode assert_param macro calls depending on configuration HAL CRC driver HAL_CRC_DeInit() resets CRC_IDR register to reset value LL Drivers changes LL BUS driver LL_APB1_GRP1_PERIPH_USBFS renamed to LL_APB1_GRP1_PERIPH_USB LL SYSTEM driver Fix typo on LL_DBGMCU_APB1_xxx and LL_DBGMCU_APB2_xxx ### V1.5.0 / 29-April-2016 Main Changes Maintenance Release of HAL and Low Layer drivers HAL Drivers changes Enhance HAL delay and timebase implementation Add new driver stm32l4xx_hal_timebase_tim_template.c which overrides the native HAL time base functions (defined as weak) to use the TIM peripheral as time base tick source. For more details about the usage of this driver, please refer to HAL\HAL_TimeBase example and FreeRTOS-based applications The following changes done on the HAL drivers require an update on the application code based on HAL V1.4.0 HAL RCC driver To use PLLSAI1 and PLLSAI2 indidependently from main system PLL, PLLSAI1 & PLLSAI2 initialization enriched to add PLL entry clock source and divider M RCC_PLLSAI1InitTypeDef includes PLLSAI1Source and PLLSAI1M new fields RCC_PLLSAI2InitTypeDef includes PLLSAI2Source and PLLSAI2M new fields Add missing RTC clock source definition RCC_RTCCLKSOURCE_NO_CLK DFSDM renaming to DFSDM1 (previous definitions preserved for legacy compatibility) All macros __HAL_RCC_DFSDM_xxx() renamed to __HAL_RCC_DFSDM1_xxx() DfsdmClockSelection field of RCC_PeriphCLKInitTypeDef renamed to Dfsdm1ClockSelection RCC_PERIPHCLK_DFSDM renamed to RCC_PERIPHCLK_DFSDM1 RCC_DFSDMCLKSOURCE_PCLK renamed to RCC_DFSDM1CLKSOURCE_PCLK RCC_DFSDMCLKSOURCE_SYSCLK renamed to RCC_DFSDM1CLKSOURCE_SYSCLK __HAL_RCC_DFSDM_CONFIG() renamed to __HAL_RCC_DFSDM1_CONFIG() __HAL_RCC_GET_DFSDM_SOURCE() renamed to __HAL_RCC_GET_DFSDM1_SOURCE() Add missing RTC clock source definition RCC_RTCCLKSOURCE_NO_CLK HAL I2C driver Update to avoid waiting on STOPF/BTF/AF flag under DMA ISR by using the PPP end of transfer interrupt in the DMA transfer process. This requires the following updates on user application: Configure and enable the I2Cx IRQ in HAL_I2C_MspInit() function In stm32l4xx_it.c file, I2Cx_IRQHandler() function: add a call to HAL_I2C_IRQHandler() function HAL UART/USART drivers IRQ Handler global optimization Add error management in case of DMA transfer through HAL_DMA_Abort_IT() and DMA XferAbortCallback() Polling management update: The user Timeout value must be estimated for the overall process duration HAL IRDA/SMARTCARD drivers Polling management update: The user Timeout value must be estimated for the overall process duration HAL SPI driver Add SPI error management during DMA process: this requires the following updates in the user application: Configure and enable the SPIx IRQ in HAL_SPI_MspInit() function In stm32l4xx_it.c file, SPIx_IRQHandler() function: add a call to HAL_SPI_IRQHandler() function Add and customize the Error Callback API: HAL_SPI_ErrorCallback() HAL QSPI driver Add QSPI error management during DMA process Improve the DMA transmit process by using QSPI TC interrupt instead of waiting on TC flag under DMA ISR. These two improvements require the following updates on user application: Configure and enable the QSPI IRQ in HAL_QSPI_MspInit() function In stm32l4xx_it.c file, QSPI_IRQHandler() function: add a call to HAL_QSPI_IRQHandler() function Add and customize the Error Callback API: HAL_QSPI_ErrorCallback() Add the management of non-blocking transfer abort service: HAL_QSPI_Abort_IT(). In this case the user must: Add new callback HAL_QSPI_AbortCpltCallback() to inform user at the end of abort process A new value of State in the HAL_QSPI_StateTypeDef provides the current state during the abort phase Polling management update: The user Timeout value must be estimated for the overall process duration Fix wrong data size management in HAL_QSPI_Receive_DMA() New API HAL_QSPI_SetFifoThreshold() and HAL_QSPI_GetFifoThreshold() HAL IWDG driver New simplified HAL IWDG driver: r emove HAL_IWDG_Start(), HAL_IWDG_MspInit() and HAL_IWDG_GetState() APIs API functions are: HAL_IWDG_Init(): this function insures the configuration and the start of the IWDG counter HAL_IWDG_Refresh(): this function insures the reload of the IWDG counter Refer to the following example to identify the changes: IWDG_Example HAL WWDG driver New simplified HAL WWDG driver: remove HAL_WWDG_Start(), HAL_WWDG_Start_IT(), HAL_WWDG_MspDeInit() and HAL_WWDG_GetState() APIs Update HAL_WWDG_Refresh() API to remove counter parameter New field EWIMode in WWDG_InitTypeDef to specify need for Early Wakeup Interrupt API functions are: HAL_WWDG_Init(), HAL_WWDG_MspInit(), HAL_WWDG_Refresh(), HAL_WWDG_IRQHandler() and HAL_WWDG_EarlyWakeupCallback() HAL DMA driver Global driver code optimization to reduce memory footprint New APIs HAL_DMA_RegisterCallback() and HAL_DMA_UnRegisterCallback() to register/unregister the different possible callbacks identified by enum typedef HAL_DMA_CallbackIDTypeDef New API HAL_DMA_Abort_IT() to abort DMA transfer in non-blocking mode for interrupt context The new registered Abort callback is called when DMA transfer abortion is completed Add new Error Codes: HAL_DMA_ERROR_NO_XFER and HAL_DMA_ERROR_NOT_SUPPORTED Add __HAL_DMA_GET_COUNTER() macro HAL COMP driver EXTI configuration done in HAL_COMP_Init() based on TriggerMode field of COMP_InitTypeDef structure; HAL_COMP_Start()/HAL_COMP_Stop() APIs are sufficient to start and stop comparators (HAL_COMP_Start_IT() and HAL_COMP_Stop_IT() are preserved for legacy compatibility) Add comparator startup time and scaler bridge stabilization time in HAL_COMP_Init() Fix to call HAL_COMP_TriggerCallback() only once when the 2 comparators are configured in window mode Inverting & Non-inverting inputs renaming (previous definitions preserved for legacy compatibility) COMP_INVERTING_xxx definitions renamed to COMP_INPUT_MINUS_xxx COMP_NONINVERTING_xxx definitions renamed to COMP_INPUT_PLUS_xxx Blanking sources renaming to highlight Comparator & Timer instances connections (previous definitions preserved for legacy compatibility) COMP_BLANKINGSRCE_TIM1OC5 renamed to COMP_BLANKINGSRC_TIM1_OC5_COMP1 COMP_BLANKINGSRCE_TIM2OC3 renamed to COMP_BLANKINGSRC_TIM2_OC3_COMP1 COMP_BLANKINGSRCE_TIM3OC3 renamed to COMP_BLANKINGSRC_TIM3_OC3_COMP1 COMP_BLANKINGSRCE_TIM3OC4 renamed to COMP_BLANKINGSRC_TIM3_OC4_COMP2 COMP_BLANKINGSRCE_TIM8OC5 renamed to COMP_BLANKINGSRC_TIM8_OC5_COMP2 COMP_BLANKINGSRCE_TIM15OC1 renamed to COMP_BLANKINGSRC_TIM15_OC1_COMP2 COMP_BLANKINGSRCE_NONE renamed to COMP_BLANKINGSRC_NONE HAL CRYP driver Software workaround for AES issue on GCM encryption with payload length not a multiple of 128 bits Add support of payload length not multiple of 32 bits HAL GPIO driver Add missing GPIO_AF6_COMP1 for STM32L431xx/STM32L432xx/STM32L433xx/STM32L442xx/STM32L443xx DFSDM renaming to DFSDM1 (previous definitions preserved for legacy compatibility) GPIO_AF6_DFSDM renamed to GPIO_AF6_DFSDM1 HAL HCD driver Clear NACK flag before re-enabling the channel for new IN request HAL PCD driver Host mode Use HCLK frequency to set TRDT value Device mode Force suspend and low-power mode before going to L1 state Unmask Start Of Frame interrupt HAL TIM driver DFSDM renaming to DFSDM1 (previous definitions preserved for legacy compatibility) TIM_BREAKINPUTSOURCE_DFSDM renamed to TIM_BREAKINPUTSOURCE_DFSDM1 HAL SAI driver Update HAL_SAI_IRQHandler: Add error management in case of DMA transfer through HAL_DMA_Abort_IT() and DMA XferAbortCallback() HAL SWPMI driver Update initialization sequence in voltage class B LL Drivers changes LL ADC driver Fix injected conversion configuration with SW start in LL_ADC_INJ_ConfigQueueContext() LL BUS driver DFSDM renaming to DFSDM1 (previous definitions preserved for legacy compatibility) LL_APB2_GRP1_PERIPH_DFSDM renamed to LL_APB2_GRP1_PERIPH_DFSDM1 LL COMP driver Window mode renaming to highlight Comparator instances connection (previous definitions preserved for legacy compatibility) LL_COMP_WINDOWMODE_ENABLE renamed to LL_COMP_WINDOWMODE_COMP1_INPUT_PLUS_COMMON Blanking sources renaming to highlight Comparator & Timer instances connections (previous definitions preserved for legacy compatibility) LL_COMP_BLANKINGSRCE_TIM1OC5 renamed to LL_COMP_BLANKINGSRC_TIM1_OC5_COMP1 LL_COMP_BLANKINGSRCE_TIM2OC3 renamed to LL_COMP_BLANKINGSRC_TIM2_OC3_COMP1 LL_COMP_BLANKINGSRCE_TIM3OC3 renamed to LL_COMP_BLANKINGSRC_TIM3_OC3_COMP1 LL_COMP_BLANKINGSRCE_TIM3OC4 renamed to LL_COMP_BLANKINGSRC_TIM3_OC4_COMP2 LL_COMP_BLANKINGSRCE_TIM8OC5 renamed to LL_COMP_BLANKINGSRC_TIM8_OC5_COMP2 LL_COMP_BLANKINGSRCE_TIM15OC1 renamed to LL_COMP_BLANKINGSRC_TIM15_OC1_COMP2 LL I2C driver Add SMBus feature support LL_I2C_InitTypeDef structure enriched with new PeripheralMode field to indicate I2C or SMBus modes New APIs LL_I2C_EnableSMBusAlert(), LL_I2C_DisableSMBusAlert(), LL_I2C_IsEnabledSMBusAlert(), LL_I2C_EnableSMBusPEC(), LL_I2C_DisableSMBusPEC(), LL_I2C_IsEnabledSMBusPEC(), LL_I2C_ConfigSMBusTimeout(), LL_I2C_EnableSMBusTimeout(), LL_I2C_DisableSMBusTimeout(), LL_I2C_IsEnabledSMBusTimeout(), LL_I2C_SetSMBusTimeoutA(), LL_I2C_GetSMBusTimeoutA(), LL_I2C_SetSMBusTimeoutAMode(), LL_I2C_GetSMBusTimeoutAMode(), LL_I2C_SetSMBusTimeoutB(), LL_I2C_GetSMBusTimeoutB(), LL_I2C_SetSMBusTimeoutBMode(), LL_I2C_GetSMBusTimeoutBMode(), LL_I2C_IsActiveSMBusFlag_PECERR(), LL_I2C_IsActiveSMBusFlag_TIMEOUT(), LL_I2C_IsActiveSMBusFlag_ALERT(), LL_I2C_ClearSMBusFlag_PECERR(), LL_I2C_ClearSMBusFlag_TIMEOUT(), LL_I2C_ClearSMBusFlag_ALERT(), LL_I2C_EnableSMBusPECCompare(), LL_I2C_IsEnabledSMBusPECCompare() and LL_I2C_GetSMBusPEC() New APIs LL_I2C_SetMode() and LL_I2C_GetMode() New APIs LL_I2C_EnableAutoEndMode(), LL_I2C_DisableAutoEndMode() and LL_I2C_IsEnabledAutoEndMode() New APIs LL_I2C_EnableReloadMode(), LL_I2C_DisableReloadMode() and LL_I2C_IsEnabledReloadMode() New APIs LL_I2C_EnableSlaveByteControl(), LL_I2C_DisableSlaveByteControl() and LL_I2C_IsEnabledSlaveByteControl() New APIs LL_I2C_SetTransferRequest(), LL_I2C_GetTransferRequest(), LL_I2C_SetSlaveAddr() and LL_I2C_GetSlaveAdd() New APIs LL_I2C_SetTransferSize() and LL_I2C_GetTransferSize() New APIs LL_I2C_GenerateStopCondition(), LL_I2C_GenerateStartCondition() New APIs LL_I2C_EnableAuto10BitRead(), LL_I2C_DisableAuto10BitRead() and LL_I2C_IsEnabledAuto10BitRead() LL PWR driver New APIs LL_PWR_EnterLowPowerRunMode() and LL_PWR_ExitLowPowerRunMode() LL RCC driver DFSDM renaming to DFSDM1 (previous definitions preserved for legacy compatibility) LL_RCC_DFSDM_CLKSOURCE renamed to LL_RCC_DFSDM1_CLKSOURCE LL_RCC_DFSDM_CLKSOURCE_PCLK renamed to LL_RCC_DFSDM1_CLKSOURCE_PCLK LL_RCC_DFSDM_CLKSOURCE_SYSCLK renamed to LL_RCC_DFSDM1_CLKSOURCE_SYSCLK LL SYSTEM driver New API LL_FLASH_IsPrefetchEnabled() LL TIM driver DFSDM renaming to DFSDM1 (previous definitions preserved for legacy compatibility) LL_TIM_BKIN_SOURCE_DFBK renamed to LL_TIM_BKIN_SOURCE_DF1BK New OCRef clear input selection definitions LL_TIM_OCREF_CLR_INT_NC and LL_TIM_OCREF_CLR_INT_ETR New OCRef clear API LL_TIM_SetOCRefClearInputSource() ### V1.4.0 / 26-February-2016 Main Changes Release of HAL and Low Layer drivers to add support of STM32L431xx/STM32L432xx/STM32L433xx/STM32L442xx/ STM32L443xx devices Low Layer driver initialization/de-initialization APIs applicable to all STM32L4xx devices CRS peripheral implemented as an extension of HAL RCC (HAL_RCCEx_CRS_xxxx() APIs) Superset features device STM32L443xx API User Manual available (STM32L443xx_User_Manual.chm) HAL Drivers changes HAL generic update Add default HSI48_VALUE in stm32l4xx_hal_conf_template HAL CRYP update New error code HAL_CRYP_BUSY_ERROR to reject new request while ongoing processing HAL IRDA/SMARTCARD/UART/USART update Improvement of baud rate computation at initialization LL Drivers changes New C files requiring to use USE_FULL_LL_DRIVER compilation switch in user project to benefit from new APIs stm32l4xx_ll_crs.c LL BUS update Add read-back register on clock enable functions to take into account any delay on bus LL ADC update Trigger sources renaming: LL_ADC_REG_TRIG_SW_START renamed to LL_ADC_REG_TRIG_SOFTWARE LL_ADC_REG_TRIG_EXT_TIMx_CCy renamed to LL_ADC_REG_TRIG_EXT_TIMx_CHy LL_ADC_INJ_TRIG_SW_START renamed to LL_ADC_INJ_TRIG_SOFTWARE LL_ADC_INJ_TRIG_EXT_TIMx_CCy renamed to LL_ADC_INJ_TRIG_EXT_TIMx_CHy Oversamping data shift renaming: LL_ADC_OVS_DATA_SHIFT_NONE renamed to LL_ADC_OVS_SHIFT_NONE LL_ADC_OVS_DATA_SHIFT_xxx renamed to LL_ADC_OVS_SHIFT_xxx LL DAC update Trigger sources renaming: LL_DAC_TRIGGER_SOFTWARE renamed to LL_DAC_TRIG_SOFTWARE LL_DAC_TRIGGER_TIMx_TRGO renamed to LL_DAC_TRIG_EXT_TIMx_TRGO LL_DAC_TRIGGER_EXT_IT9 renamed to LL_DAC_TRIG_EXT_EXTI_LINE9 LL LPUART update Improvement of LPUARTDIV value in baud rate computation in __LL_LPUART_DIV() macro LL USART update Improvement of USARTDIV value in baud rate computation in __LL_USART_DIV_SAMPLING8() and __LL_USART_DIV_SAMPLING16() macros ### V1.3.0 / 29-January-2016 Main Changes New Low Layer driver initialization/de-initialization APIs Naming rule is LL_PPP_Init(), LL_PPP_StructInit(), LL_PPP_DeInit() and more initialization APIs when applicable for peripheral PPP: ADC, COMP, CRC, DAC, DMA, EXTI, GPIO, I2C, LPTIM, LPUART, OPAMP, PWR, RCC, RNG, RTC, SPI, SWPMI, TIM and USART. New C files requiring to use USE_FULL_LL_DRIVER compilation switch in user project to benefit from new APIs stm32l4xx_ll_adc.c, stm32l4xx_ll_comp.c, stm32l4xx_ll_crc.c, stm32l4xx_ll_dac.c, stm32l4xx_ll_dma.c, stm32l4xx_ll_exti.c, stm32l4xx_ll_gpio.c, stm32l4xx_ll_i2c.c, stm32l4xx_ll_lptim.c, stm32l4xx_ll_lpuart.c, stm32l4xx_ll_opamp.c, stm32l4xx_ll_pwr.c, stm32l4xx_ll_rcc.c, stm32l4xx_ll_rng.c, stm32l4xx_ll_rtc.c, stm32l4xx_ll_spi.c, stm32l4xx_ll_swpmi.c, stm32l4xx_ll_tim.c and stm32l4xx_ll_usart.c stm32l4xx_ll_utils.c contains some Low Layer utilities for SysTick, Flash latency and clock configuration. Fix "parameter unused" GCC compilation warnings on __weak functions HAL Drivers changes HAL generic update Declare uwTick as global variable to allow weak HAL_IncTick() API updates in user application Add new API HAL_SYSCFG_EnableIOAnalogSwitchBooster() and HAL_SYSCFG_DisableIOAnalogSwitchBooster() HAL COMP update Allow comparator lock from the reset state with HAL_COMP_Lock() HAL CRYP update Fix state issue to resume AES calculations HAL DMA update Fix state issue after DMA transfer error HAL FLASH update Fix __HAL_FLASH_INSTRUCTION_CACHE_RESET() and __HAL_FLASH_DATA_CACHE_RESET() to allow multiple resets HAL I2C update Add support of repeated start feature with the following new APIs HAL_I2C_Master_Sequential_Transmit_IT(), HAL_I2C_Master_Sequential_Receive_IT() and HAL_I2C_Master_Abort_IT(), HAL_I2C_Slave_Sequential_Transmit_IT() and HAL_I2C_Slave_Sequential_Receive_IT() HAL_I2C_EnableListen_IT() and HAL_I2C_DisableListen_IT() New user callbacks HAL_I2C_ListenCpltCallback() and HAL_I2C_AddrCallback() Fix acknowledge failure error management (STOP being automatically generated) Review state machine and provide new API HAL_I2C_GetMode() to return HAL_I2C_MODE_MASTER, HAL_I2C_MODE_SLAVE or HAL_I2C_MODE_NONE HAL IRDA update Add missing IRDA_CLEAR_IDLEF definition for IDLE flag clear with __HAL_IRDA_CLEAR_FLAG() HAL SD update Fix SD card capacity calculation for cards with capacity over 4GB in HAL_SD_Get_CardInfo() HAL SMARTCARD update Add missing SMARTCARD_STOPBITS_0_5 definition for frame with 0.5 stop bit HAL SMARTCARD guardtime correction to not expect a minimum of 12 etu HAL UART update Add missing UART_STOPBITS_0_5 definition for frame with 0.5 stop bit RX Buffer flush request should not be called at each RXNE processing Fix wrong macro used in assert_param in HAL_LIN_SendBreak() HAL USART update Add missing USART_STOPBITS_0_5 definition for frame with 0.5 stop bit LL Drivers changes LL UTILS update (user code impacted !) Move the following functions declaration from stm32l4xx_ll_utils.h to stm32l4xx_ll_utils.c file LL_mDelay(), LL_Init1msTick() and LL_SetSystemCoreClock() LL ADC update FLAG & IT definition name change LL COMP update Rename InputInverting and InputNonInverting APIs LL_COMP_Set{/Get}InputNonInverting() renamed to LL_COMP_Set{/Get}InputMinus LL_COMP_Set{/Get}InputInverting() renamed to LL_COMP_Set{/Get}InputPlus Remove LL_COMP_SetWindowMode() and LL_COMP_GetWindowMode() LL DMA update Add helper macro __LL_DMA_GET_CHANNEL_INSTANCE() LL GPIO update Fix definition LL_GPIO_OUTPUT_OPENDRAIN Add the explicit possible values in the API description of LL_GPIO_GetPinMode(), LL_GPIO_GetPinOutputType(), LL_GPIO_GetPinSpeed(), LL_GPIO_GetPinPull(), LL_GPIO_GetAFPin_0_7() and LL_GPIO_GetAFPin_8_15() Add GPIO speed definitions LL_GPIO_SPEED_FREQ_LOW, LL_GPIO_SPEED_FREQ_MEDIUM, LL_GPIO_SPEED_FREQ_HIGH and LL_GPIO_SPEED_FREQ_VERY_HIGH to align with HAL GPIO LL I2C update Add missing function LL_I2C_ConfigFilters() to configure noise filters LL LPTIM update Add missing functions LL_LPTIM_IsEnabled() LL_LPTIM_SetWaveform() LL_LPTIM_SetPolarity() LL OPAMP update Rename power range APIs LL_OPAMP_Get{/Set}PowerRange() renamed to LL_OPAMP_Get{/Set}CommonPowerRange() LL SPI update Fix LL_SPI_IsEnabled(), LL_SPI_IsEnabledCRC() and LL_SPI_IsEnabledNSSPulse() Remove LL_SPI_Set{/Get}HalfDuplexDirection() functions: this is managed with TransferDirection parameter in LL_SPI_Set{/Get}TransferDirection() LL SWPMI update Add missing function LL_SWPMI_IsActivated() LL TIM update Add missing functions LL_TIM_CC_IsEnabledChannel() LL_TIM_OC_IsEnabledFast(), LL_TIM_OC_IsEnabledPreload() and LL_TIM_OC_IsEnabledClear() LL_TIM_IsEnabledMasterSlaveMode() LL_TIM_EnableExternalClock(), LL_TIM_DisableExternalClock() and LL_TIM_IsEnabledExternalClock() LL USART update Add LL_USART_STOPBITS_0_5 definition for usage in LL_USART_Set{/Get}StopBitsLength() and LL_USART_ConfigCharacter() ### V1.2.0 / 25-November-2015 Main Changes HAL generic update Reduce default HSE startup timeout value to 100ms in Inc\stm32l4xx_hal_conf_template.h file HAL PWR update (User application code impacted) Stop 1 with main regulator renamed into Stop 0, to be aligned with latest version of Reference Manual Change HAL_PWREx_EnterSTOP1Mode(uint32_t Regulator, uint8_t STOPEntry) into HAL_PWREx_EnterSTOP1Mode(uint8_t STOPEntry) Application code using HAL_PWREx_EnterSTOP1Mode(PWR_LOWPOWERREGULATOR_ON, STOPEntry) must be updated to use HAL_PWREx_EnterSTOP1Mode(STOPEntry) Add new API HAL_PWREx_EnterSTOP0Mode(uint8_t STOPEntry) Application code using HAL_PWREx_EnterSTOP1Mode(PWR_MAINREGULATOR_ON, STOPEntry) must be updated to use HAL_PWREx_EnterSTOP0Mode(STOPEntry) HAL OPAMP update Provide capability to run calibration despite PGA mode by switching temporary to standalone mode HAL SAI update Update SAI block synchronization selection (User application code impacted) Replace uncomplete SAI_SYNCHRONOUS_EXT value for with SAI_SYNCHRONOUS_EXT_SAI1 and SAI_SYNCHRONOUS_EXT_SAI2 Update external synchronization input selection (User application code impacted) Remove useless SAI_SYNCEXT_IN_ENABLE value for SynchroExt field in SAI_InitTypeDef structure Add support of 24bits configuration in PCM protocol Add codec not ready interrupt management Fix computation of data size, frame length, active frame length, slot size and first bit offset in I2S protocol Fix mute counter setting in HAL_SAI_EnableRxMuteMode() Fix ambiguous clock strobing values: fix HAL_SAI_Init() to set correct CKSTR bits in SAI_xCR1 according to ClockStrobing and AudioMode parameters Fill in the Fifo before enable interrupt in HAL_SAI_Transmit_IT() Fix assert on active slot selection in HAL_SAI_Init() Fix companding mode management in HAL_SAI_Init() HAL TSC update Improve IODefault state management HAL NOR/HAL SRAM/FMC update WriteFifo field of FMC_NORSRAM_InitTypeDef structure is not applicable on STM32L47x/STM32L48x devices LL PWR update (User application code impacted) LL PWR API change to add new Stop 0 mode and update Stop 1 mode definition Change LL_PWR_SetPowerMode(uint32_t LowPowerMode) possible LowPowerMode values update LL_PWR_MODE_STOP1_LP_REGU renamed into LL_PWR_MODE_STOP1 Application code using LL_PWR_SetPowerMode(LL_PWR_MODE_STOP1_LP_REGU) must be updated to use LL_PWR_SetPowerMode(LL_PWR_MODE_STOP1) LL_PWR_MODE_STOP1_MAIN_REGU renamed into LL_PWR_MODE_STOP0 Application code using LL_PWR_SetPowerMode(LL_PWR_MODE_STOP1_MAIN_REGU) must be updated to use LL_PWR_SetPowerMode(LL_PWR_MODE_STOP0) ### V1.1.1 / 16-October-2015 Main Changes HAL generic update Fine tuning of Inc\stm32l4xx_hal_conf_template.h file to keep Flash prefetch off as default system configuration (PREFETCH_ENABLE set to 0) HAL TIM update Removed useless assert_param() macro check on input parameters in HAL_TIM_OC_ConfigChannel(), HAL_TIM_PWM_ConfigChannel() and HAL_TIM_ConfigClockSource(), LL ADC update Fix LL_ADC_GetAnalogWDMonitChannels() for AWD2 and AWD3 LL RCC update Add new API LL_RCC_LSE_DisableCSS() LL UTILS update Fix LL_GetPackageType() ### V1.1.0 / 16-September-2015 Main Changes Add Low Layer drivers allowing performance and footprint optimization Low Layer drivers APIs provide register level programming: they require deep knowledge of peripherals described in STM32L4x6 Reference Manual Low Layer drivers are available for: ADC, COMP, Cortex, CRC, DAC, DMA, EXTI, GPIO, I2C, IWDG, LPYIM, LPUART, OPAMP, PWR, RCC, RNG, RTC, SPI, SWPMI, TIM, USART, WWDG peripherals and additionnal Low Level Bus, System and Utilities APIs. Low Layer drivers APIs are implemented as static inline function in new Inc/stm32l4xx_ll_ppp.h files for PPP peripherals, there is no configuration file and each stm32l4xx_ll_ppp.h file must be included in user code. HAL ADC update Channel 5 is not usable for ADC3 HAL CAN update Update HAL_CAN_IRQHandler() to clear ERRI bit prior to call HAL_CAN_ErrorCallback() HAL COMP update Update HAL_COMP_Init() for low power optimization in case of COMP_INVERTINGINPUT_VREFINT HAL CRC update Add new API HAL_CRYPEx_ProcessSuspend() HAL DMA update Update HAL_DMA_IRQHandler() to set HAL_DMA_ERROR_TE error bit in handle ErrorCode field HAL FLASH update Add option byte OB_USER_nRST_SHDW to be used with HAL_FLASHEx_OBProgram() HAL GPIO update Rename GPIO speed definitions to GPIO_SPEED_FREQ_LOW, GPIO_SPEED_FREQ_MEDIUM, GPIO_SPEED_FREQ_HIGH and GPIO_SPEED_FREQ_VERY_HIGH Fix macro __HAL_GPIO_EXTI_GENERATE_SWIT() HAL PWR update Fix HAL_PWR_DisableWakeUpPin() to clear only appropriate bits in PWR CR3 register Combination of GPIO pins possible in HAL_PWREx_EnableGPIOPullUp(), HAL_PWREx_DisableGPIOPullUp(), HAL_PWREx_EnableGPIOPullDown() and HAL_PWREx_DisableGPIOPullDown() HAL RCC update Add LSE Clock Security System (CSS) management with new APIs: HAL_RCCEx_EnableLSECSS_IT(), HAL_RCCEx_LSECSS_IRQHandler() and HAL_RCCEx_LSECSS_Callback() Add RCC_MCO1SOURCE_NOCLOCK to provide capability to disable MCO output in HAL_RCC_MCOConfig() Update HAL_RCC_OscConfig() and HAL_RCCEx_PeriphCLKConfig() to keep backup domain enabled when configuring respectively LSE and RTC clock source Update HAL_RCCEx_DisablePLLSAI1() and HAL_RCCEx_DisablePLLSAI2() to disable respectively PLLSAI1 and PLLSAI2 clock outputs Update HAL_RCCEx_GetPeriphCLKFreq() to return the frequency in Hz applied to peripherals via HAL_RCCEx_PeriphCLKConfig() Update HAL_RCC_DeInit() to set default MSI range Remove old workaround on LSE drive medium configuration values HAL SPI update Fix issue to receive CRC in RX 2 lines mode 8-bit dataSize and even buffer size. HAL TIM update Fix macro __HAL_TIM_SET_COMPARE() HAL UART update Remove enable of Error interrupt in HAL_UART_Transmit_IT() ### V1.0.0 / 26-June-2015 Main Changes First official release of STM32L4xx HAL Drivers for STM32L471xx/STM32L475xx/ STM32L476xx/ STM32L485xx and STM32L486xx devices. ## License Redistribution and use in source and binary forms, with or without modification, are permitted provided that the following conditions are met: Redistributions of source code must retain the above copyright notice, this list of conditions and the following disclaimer. Redistributions in binary form must reproduce the above copyright notice, this list of conditions and the following disclaimer in the documentation and/or other materials provided with the distribution. Neither the name of STMicroelectronics nor the names of its contributors may be used to endorse or promote products derived from this software without specific prior written permission. THIS SOFTWARE IS PROVIDED BY THE COPYRIGHT HOLDERS AND CONTRIBUTORS "AS IS" AND ANY EXPRESS OR IMPLIED WARRANTIES, INCLUDING, BUT NOT LIMITED TO, THE IMPLIED WARRANTIES OF MERCHANTABILITY AND FITNESS FOR A PARTICULAR PURPOSE ARE DISCLAIMED. IN NO EVENT SHALL THE COPYRIGHT HOLDER OR CONTRIBUTORS BE LIABLE FOR ANY DIRECT, INDIRECT, INCIDENTAL, SPECIAL, EXEMPLARY, OR CONSEQUENTIAL DAMAGES (INCLUDING, BUT NOT LIMITED TO, PROCUREMENT OF SUBSTITUTE GOODS OR SERVICES; LOSS OF USE, DATA, OR PROFITS; OR BUSINESS INTERRUPTION) HOWEVER CAUSED AND ON ANY THEORY OF LIABILITY, WHETHER IN CONTRACT, STRICT LIABILITY, OR TORT (INCLUDING NEGLIGENCE OR OTHERWISE) ARISING IN ANY WAY OUT OF THE USE OF THIS SOFTWARE, EVEN IF ADVISED OF THE POSSIBILITY OF SUCH DAMAGE. For complete documentation on STM32 Microcontrollers visit www.st.com/STM32