----------------
Date: 2015-08-14
Author: Sonny Jeon
Subject: Individual control pin invert compile-option.

- Control pins may be individually inverted through a
CONTROL_INVERT_MASK macro. This mask is define in the cpu_map.h file.


----------------
Date: 2015-07-17
Author: Sonny Jeon
Subject: Version bump to v0.9j

- Version bump requested by OEMs to easily determine whether the
firmware supports the new EEPROM reset feature. Other than that, no
significant changes.
