PAL A Platform Abstraction Layer connects the mbed-client with the underlying platform.

- Main Page
- Data Structures
- Files

- Data Structures
- Data Structure Index
- Data Fields

- All
- Variables

Here is a list of all struct and union fields with links to the structures/unions they belong to:

- address : palNetInterfaceInfo
- addressData : palSocketAddress
- addressSize : palNetInterfaceInfo
- addressType : palSocketAddress
- arg1 : threadsArgument
- arg2 : threadsArgument
- arg3 : threadsArgument
- arg4 : threadsArgument
- arg5 : threadsArgument
- arg6 : threadsArgument
- arg7 : threadsArgument
- buffer : _palBuffer_t , _palConstBuffer_t
- bufferLength : _palBuffer_t , _palConstBuffer_t
- interfaceName : palNetInterfaceInfo
- maxBufferLength : _palBuffer_t , _palConstBuffer_t
- pal_tv_sec : pal_timeVal
- pal_tv_usec : pal_timeVal
- storeData : pal_threadLocalStore
- ticksBeforeTimer : timerArgument
- ticksInFunc1 : timerArgument
- ticksInFunc2 : timerArgument