PAL A Platform Abstraction Layer connects the mbed-client with the underlying platform.

- Main Page
- Data Structures
- Files

- File List
- Globals

Macros | Functions
pal_socket_test_main_FreeRTOS.c File Reference
`#include "fsl_device_registers.h"`
`#include "fsl_debug_console.h"`
`#include "board.h"`
`#include "pin_mux.h"`
`#include "clock_config.h"`
`#include "unity.c"`
`#include "FreeRTOS.h"`
`#include "task.h"`

## Macros
#define | APP_DEBUG_UART_BAUDRATE 9600 /* Debug console baud rate. */
#define | APP_DEBUG_UART_CLKSRC_NAME kCLOCK_CoreSysClk /* System clock. */

## Functions
int | UnityMain (int argc, const char *argv[], void(*runAllTests)(void))
void | TEST_pal_socket_GROUP_RUNNER (void)
int | main (void)
| Main function. More...
void | unity_output_char (int c)

## Macro Definition Documentation

#define APP_DEBUG_UART_BAUDRATE 9600 /* Debug console baud rate. */

#define APP_DEBUG_UART_CLKSRC_NAME kCLOCK_CoreSysClk /* System clock. */

## Function Documentation

int main | ( | void |  | ) |

Main function.

void TEST_pal_socket_GROUP_RUNNER | ( | void |  | ) |

void unity_output_char | ( | int | c | ) |

int UnityMain | ( | int | argc,
|  | const char * | argv[],
|  | void(*)(void) | runAllTests
| ) |  |