PAL A Platform Abstraction Layer connects the mbed-client with the underlying platform.

- Main Page
- Data Structures
- Files

- Data Structures
- Data Structure Index
- Data Fields

Data Fields
palNetInterfaceInfo Struct Reference

`#include <pal_network.h>`

## Data Fields
char | interfaceName [16]
palSocketAddress_t | address
uint32_t | addressSize

## Detailed Description

address data structure with enough room to support IPV4 and IPV6

## Field Documentation

palSocketAddress_t palNetInterfaceInfo::address

uint32_t palNetInterfaceInfo::addressSize

char palNetInterfaceInfo::interfaceName[16]

The documentation for this struct was generated from the following file:

- C:/work/PAL/zolFull/mbed-client-pal/Source/PAL-Impl/Services-API/pal_network.h