{
    "Target": {
        "core": null,
        "default_toolchain": "ARM",
        "supported_toolchains": null,
        "extra_labels": [],
        "is_disk_virtual": false,
        "macros": [],
        "device_has": [],
        "features": [],
        "detect_code": [],
        "public": false,
        "default_lib": "std",
        "bootloader_supported": false,
        "config": {
            "console-uart-flow-control": {
                "help": "Console hardware flow control. Options: null, RTS, CTS, RTSCTS.",
                "value": null
            },
            "network-default-interface-type": {
                "help": "Default network interface type. Typical options: null, ETHERNET, WIFI, CELLULAR, MESH",
                "value": null
            }
        }
    },
    "CM4_UARM": {
        "inherits": ["Target"],
        "core": "Cortex-M4",
        "default_toolchain": "uARM",
        "public": false,
        "supported_toolchains": ["uARM"],
        "default_lib": "small"
    },
    "CM4_ARM": {
        "inherits": ["Target"],
        "core": "Cortex-M4",
        "public": false,
        "supported_toolchains": ["ARM"]
    },
    "CM4F_UARM": {
        "inherits": ["Target"],
        "core": "Cortex-M4F",
        "default_toolchain": "uARM",
        "public": false,
        "supported_toolchains": ["uARM"],
        "default_lib": "small"
    },
    "CM4F_ARM": {
        "inherits": ["Target"],
        "core": "Cortex-M4F",
        "public": false,
        "supported_toolchains": ["ARM"]
    },
    "LPCTarget": {
        "inherits": ["Target"],
        "post_binary_hook": {"function": "LPCTargetCode.lpc_patch"},
        "public": false
    },
    "LPC11C24": {
        "inherits": ["LPCTarget"],
        "core": "Cortex-M0",
        "extra_labels": ["NXP", "LPC11XX_11CXX", "LPC11CXX"],
        "OUTPUT_EXT": "hex",
        "macros": ["CMSIS_VECTAB_VIRTUAL", "CMSIS_VECTAB_VIRTUAL_HEADER_FILE=\"cmsis_nvic.h\""],
        "supported_toolchains": ["ARM", "uARM", "GCC_ARM", "IAR"],
        "device_has": ["ANALOGIN", "CAN", "I2C", "I2CSLAVE", "INTERRUPTIN", "PORTIN", "PORTINOUT", "PORTOUT", "PWMOUT", "SERIAL", "SLEEP", "SPI", "SPISLAVE", "STDIO_MESSAGES"],
        "device_name": "LPC11C24FBD48/301"
    },
    "LPC1114": {
        "inherits": ["LPCTarget"],
        "core": "Cortex-M0",
        "default_toolchain": "uARM",
        "extra_labels": ["NXP", "LPC11XX_11CXX", "LPC11XX"],
        "macros": ["CMSIS_VECTAB_VIRTUAL", "CMSIS_VECTAB_VIRTUAL_HEADER_FILE=\"cmsis_nvic.h\""],
        "supported_toolchains": ["ARM", "uARM", "GCC_ARM", "IAR"],
        "device_has": ["ANALOGIN", "I2C", "I2CSLAVE", "INTERRUPTIN", "PORTIN", "PORTINOUT", "PORTOUT", "PWMOUT", "SERIAL", "SLEEP", "SPI", "SPISLAVE", "STDIO_MESSAGES"],
        "default_lib": "small",
        "release_versions": ["2"],
        "device_name": "LPC1114FN28/102"
    },
    "LPC11U24": {
        "inherits": ["LPCTarget"],
        "core": "Cortex-M0",
        "default_toolchain": "uARM",
        "extra_labels": ["NXP", "LPC11UXX", "LPC11U24_401"],
        "macros": ["CMSIS_VECTAB_VIRTUAL", "CMSIS_VECTAB_VIRTUAL_HEADER_FILE=\"cmsis_nvic.h\""],
        "supported_toolchains": ["ARM", "uARM", "GCC_ARM", "IAR"],
        "detect_code": ["1040"],
        "device_has": ["ANALOGIN", "I2C", "I2CSLAVE", "INTERRUPTIN", "LOCALFILESYSTEM", "PORTIN", "PORTINOUT", "PORTOUT", "PWMOUT", "SEMIHOST", "SERIAL", "SLEEP", "SPI", "SPISLAVE", "STDIO_MESSAGES"],
        "default_lib": "small",
        "release_versions": ["2"],
        "device_name": "LPC11U24FBD48/401"
    },
    "OC_MBUINO": {
        "inherits": ["LPC11U24"],
        "macros": ["TARGET_LPC11U24", "CMSIS_VECTAB_VIRTUAL", "CMSIS_VECTAB_VIRTUAL_HEADER_FILE=\"cmsis_nvic.h\""],
        "extra_labels": ["NXP", "LPC11UXX"],
        "device_has": ["ANALOGIN", "I2C", "I2CSLAVE", "INTERRUPTIN", "PORTIN", "PORTINOUT", "PORTOUT", "PWMOUT", "SERIAL", "SLEEP", "SPI", "SPISLAVE", "STDIO_MESSAGES"],
        "release_versions": ["2"]
    },
    "LPC11U24_301": {
        "inherits": ["LPCTarget"],
        "core": "Cortex-M0",
        "extra_labels": ["NXP", "LPC11UXX"],
        "macros": ["CMSIS_VECTAB_VIRTUAL", "CMSIS_VECTAB_VIRTUAL_HEADER_FILE=\"cmsis_nvic.h\""],
        "supported_toolchains": ["ARM", "uARM", "GCC_ARM", "IAR"],
        "device_has": ["ANALOGIN", "I2C", "I2CSLAVE", "INTERRUPTIN", "LOCALFILESYSTEM", "PORTIN", "PORTINOUT", "PORTOUT", "PWMOUT", "SEMIHOST", "SERIAL", "SLEEP", "SPI", "SPISLAVE", "STDIO_MESSAGES"],
        "device_name": "LPC11U24FHI33/301"
    },
    "LPC11U34_421": {
        "inherits": ["LPCTarget"],
        "core": "Cortex-M0",
        "default_toolchain": "uARM",
        "extra_labels": ["NXP", "LPC11UXX"],
        "macros": ["CMSIS_VECTAB_VIRTUAL", "CMSIS_VECTAB_VIRTUAL_HEADER_FILE=\"cmsis_nvic.h\""],
        "supported_toolchains": ["ARM", "uARM", "GCC_ARM"],
        "device_has": ["ANALOGIN", "I2C", "I2CSLAVE", "INTERRUPTIN", "PORTIN", "PORTINOUT", "PORTOUT", "PWMOUT", "SERIAL", "SLEEP", "SPI", "SPISLAVE"],
        "default_lib": "small",
        "device_name": "LPC11U34FBD48/311"
    },
    "MICRONFCBOARD": {
        "inherits": ["LPC11U34_421"],
        "macros_add": ["LPC11U34_421", "APPNEARME_MICRONFCBOARD"],
        "extra_labels_add": ["APPNEARME_MICRONFCBOARD"],
        "release_versions": ["2"],
        "device_name": "LPC11U34FBD48/311"
    },
    "LPC11U35_401": {
        "inherits": ["LPCTarget"],
        "core": "Cortex-M0",
        "default_toolchain": "uARM",
        "extra_labels": ["NXP", "LPC11UXX"],
        "macros": ["CMSIS_VECTAB_VIRTUAL", "CMSIS_VECTAB_VIRTUAL_HEADER_FILE=\"cmsis_nvic.h\""],
        "supported_toolchains": ["ARM", "uARM", "GCC_ARM", "IAR"],
        "device_has": ["ANALOGIN", "I2C", "I2CSLAVE", "INTERRUPTIN", "PORTIN", "PORTINOUT", "PORTOUT", "PWMOUT", "SERIAL", "SLEEP", "SPI", "SPISLAVE"],
        "default_lib": "small",
        "release_versions": ["2"],
        "device_name": "LPC11U35FBD48/401"
    },
    "LPC11U35_501": {
        "inherits": ["LPCTarget"],
        "core": "Cortex-M0",
        "default_toolchain": "uARM",
        "extra_labels": ["NXP", "LPC11UXX", "MCU_LPC11U35_501"],
        "macros": ["CMSIS_VECTAB_VIRTUAL", "CMSIS_VECTAB_VIRTUAL_HEADER_FILE=\"cmsis_nvic.h\""],
        "supported_toolchains": ["ARM", "uARM", "GCC_ARM", "IAR"],
        "device_has": ["ANALOGIN", "I2C", "I2CSLAVE", "INTERRUPTIN", "PORTIN", "PORTINOUT", "PORTOUT", "PWMOUT", "SERIAL", "SLEEP", "SPI", "SPISLAVE"],
        "default_lib": "small",
        "release_versions": ["2"],
        "device_name": "LPC11U35FHI33/501"
    },
    "LPC11U35_501_IBDAP": {
        "inherits": ["LPCTarget"],
        "core": "Cortex-M0",
        "default_toolchain": "uARM",
        "extra_labels": ["NXP", "LPC11UXX", "MCU_LPC11U35_501"],
        "macros": ["CMSIS_VECTAB_VIRTUAL", "CMSIS_VECTAB_VIRTUAL_HEADER_FILE=\"cmsis_nvic.h\""],
        "supported_toolchains": ["ARM", "uARM", "GCC_ARM", "IAR"],
        "device_has": ["ANALOGIN", "I2C", "I2CSLAVE", "INTERRUPTIN", "PORTIN", "PORTINOUT", "PORTOUT", "PWMOUT", "SERIAL", "SLEEP", "SPI", "SPISLAVE"],
        "default_lib": "small",
        "device_name": "LPC11U35FHI33/501"
    },
    "XADOW_M0": {
        "inherits": ["LPC11U35_501"]
    },
    "LPC11U35_Y5_MBUG": {
        "inherits": ["LPCTarget"],
        "core": "Cortex-M0",
        "default_toolchain": "uARM",
        "extra_labels": ["NXP", "LPC11UXX", "MCU_LPC11U35_501"],
        "macros": ["CMSIS_VECTAB_VIRTUAL", "CMSIS_VECTAB_VIRTUAL_HEADER_FILE=\"cmsis_nvic.h\""],
        "supported_toolchains": ["ARM", "uARM", "GCC_ARM", "IAR"],
        "device_has": ["ANALOGIN", "I2C", "I2CSLAVE", "INTERRUPTIN", "PORTIN", "PORTINOUT", "PORTOUT", "PWMOUT", "SERIAL", "SLEEP", "SPI", "SPISLAVE"],
        "default_lib": "small",
        "device_name": "LPC11U35FHI33/501"
    },
    "LPC11U37_501": {
        "inherits": ["LPCTarget"],
        "core": "Cortex-M0",
        "default_toolchain": "uARM",
        "extra_labels": ["NXP", "LPC11UXX"],
        "macros": ["CMSIS_VECTAB_VIRTUAL", "CMSIS_VECTAB_VIRTUAL_HEADER_FILE=\"cmsis_nvic.h\""],
        "supported_toolchains": ["ARM", "uARM", "GCC_ARM", "IAR"],
        "default_lib": "small",
        "device_name": "LPC11U37FBD64/501"
    },
    "LPCCAPPUCCINO": {
        "inherits": ["LPC11U37_501"],
        "device_has": ["ANALOGIN", "I2C", "I2CSLAVE", "INTERRUPTIN", "PORTIN", "PORTINOUT", "PORTOUT", "PWMOUT", "SERIAL", "SLEEP", "SPI", "SPISLAVE"],
        "device_name": "LPC11U37FBD64/501"
    },
    "ARCH_GPRS": {
        "supported_form_factors": ["ARDUINO"],
        "core": "Cortex-M0",
        "default_toolchain": "uARM",
        "extra_labels": ["NXP", "LPC11UXX", "LPC11U37_501"],
        "macros": ["CMSIS_VECTAB_VIRTUAL", "CMSIS_VECTAB_VIRTUAL_HEADER_FILE=\"cmsis_nvic.h\""],
        "supported_toolchains": ["ARM", "uARM", "GCC_ARM", "IAR"],
        "inherits": ["LPCTarget"],
        "device_has": ["ANALOGIN", "I2C", "I2CSLAVE", "INTERRUPTIN", "PORTIN", "PORTINOUT", "PORTOUT", "PWMOUT", "SERIAL", "SLEEP", "SPI", "SPISLAVE"],
        "default_lib": "small",
        "release_versions": ["2"],
        "device_name": "LPC11U37FBD64/501"
    },
    "LPC11U68": {
        "supported_form_factors": ["ARDUINO"],
        "core": "Cortex-M0+",
        "default_toolchain": "uARM",
        "extra_labels": ["NXP", "LPC11U6X"],
        "supported_toolchains": ["ARM", "uARM", "GCC_ARM", "IAR"],
        "inherits": ["LPCTarget"],
        "detect_code": ["1168"],
        "device_has": ["ANALOGIN", "I2C", "I2CSLAVE", "INTERRUPTIN", "PWMOUT", "SERIAL", "SLEEP", "SPI"],
        "default_lib": "small",
        "release_versions": ["2"],
        "device_name": "LPC11U68JBD100"
    },
    "LPC1347": {
        "inherits": ["LPCTarget"],
        "core": "Cortex-M3",
        "extra_labels": ["NXP", "LPC13XX"],
        "supported_toolchains": ["ARM", "GCC_ARM", "IAR"],
        "device_has": ["ANALOGIN", "I2C", "I2CSLAVE", "INTERRUPTIN", "PORTIN", "PORTINOUT", "PORTOUT", "PWMOUT", "SERIAL", "SLEEP", "SPI", "SPISLAVE", "STDIO_MESSAGES"],
        "release_versions": ["2"],
        "device_name": "LPC1347FBD48"
    },
    "LPC1549": {
        "supported_form_factors": ["ARDUINO"],
        "core": "Cortex-M3",
        "default_toolchain": "uARM",
        "extra_labels": ["NXP", "LPC15XX"],
        "supported_toolchains": ["uARM", "GCC_ARM", "IAR"],
        "inherits": ["LPCTarget"],
        "detect_code": ["1549"],
        "device_has": ["ANALOGIN", "ANALOGOUT", "CAN", "I2C", "INTERRUPTIN", "PWMOUT", "SERIAL", "SERIAL_FC", "SPI", "SPISLAVE"],
        "default_lib": "small",
        "release_versions": ["2"],
        "device_name": "LPC1549JBD64"
    },
    "LPC1768": {
        "inherits": ["LPCTarget"],
        "core": "Cortex-M3",
        "extra_labels": ["NXP", "LPC176X", "MBED_LPC1768", "NXP_EMAC"],
        "supported_toolchains": ["ARM", "uARM", "GCC_ARM", "IAR"],
        "detect_code": ["1010"],
        "device_has": ["RTC", "USTICKER", "ANALOGIN", "ANALOGOUT", "CAN", "DEBUG_AWARENESS", "EMAC", "ETHERNET", "I2C", "I2CSLAVE", "INTERRUPTIN", "LOCALFILESYSTEM", "PORTIN", "PORTINOUT", "PORTOUT", "PWMOUT", "SEMIHOST", "SERIAL", "SERIAL_FC", "SLEEP", "SPI", "SPISLAVE", "STDIO_MESSAGES", "FLASH"],
        "release_versions": ["2", "5"],
        "device_name": "LPC1768",
        "bootloader_supported": true,
        "config": {
            "us-ticker-timer": {
                "help": "Chooses which timer (0-3) to use for us_ticker.c",
                "value": 3
            }
        },
        "overrides": {
            "network-default-interface-type": "ETHERNET"
        }
    },
    "LPC1769": {
        "inherits": ["LPC1768"],
        "device_name": "LPC1769"
    },
    "ARCH_PRO": {
        "supported_form_factors": ["ARDUINO"],
        "core": "Cortex-M3",
        "supported_toolchains": ["ARM", "uARM", "GCC_ARM", "IAR"],
        "extra_labels": ["NXP", "LPC176X", "NXP_EMAC"],
        "macros": ["TARGET_LPC1768"],
        "inherits": ["LPCTarget"],
        "device_has": ["ANALOGIN", "ANALOGOUT", "CAN", "DEBUG_AWARENESS", "EMAC", "ETHERNET", "I2C", "I2CSLAVE", "INTERRUPTIN", "PORTIN", "PORTINOUT", "PORTOUT", "PWMOUT", "SERIAL", "SERIAL_FC", "SLEEP", "SPI", "SPISLAVE", "STDIO_MESSAGES", "FLASH"],
        "release_versions": ["2", "5"],
        "device_name": "LPC1768",
        "bootloader_supported": true,
        "overrides": {
            "network-default-interface-type": "ETHERNET"
        }
    },
    "UBLOX_C027": {
        "supported_form_factors": ["ARDUINO"],
        "core": "Cortex-M3",
        "supported_toolchains": ["ARM", "uARM", "GCC_ARM", "IAR"],
        "extra_labels": ["NXP", "LPC176X", "NXP_EMAC"],
        "config": {
            "modem_is_on_board": {
                "help": "Value: Tells the build system that the modem is on-board as oppose to a plug-in shield/module.",
                "value": 1,
                "macro_name": "MODEM_ON_BOARD"
            },
            "modem_data_connection_type": {
                "help": "Value: Defines how the modem is wired up to the MCU, e.g., data connection can be a UART or USB and so forth.",
                "value": 1,
                "macro_name": "MODEM_ON_BOARD_UART"
            }
        },
        "macros": ["TARGET_LPC1768"],
        "inherits": ["LPCTarget"],
        "device_has": ["USTICKER", "ANALOGIN", "ANALOGOUT", "CAN", "DEBUG_AWARENESS", "EMAC", "ETHERNET", "I2C", "I2CSLAVE", "INTERRUPTIN", "PORTIN", "PORTINOUT", "PORTOUT", "PWMOUT", "SERIAL", "SERIAL_FC", "SLEEP", "SPI", "SPISLAVE", "STDIO_MESSAGES", "FLASH"],
        "release_versions": ["2", "5"],
        "device_name": "LPC1768",
        "bootloader_supported": true,
        "overrides": {
            "network-default-interface-type": "CELLULAR"
        }
    },
    "XBED_LPC1768": {
        "inherits": ["LPCTarget"],
        "core": "Cortex-M3",
        "supported_toolchains": ["ARM", "uARM", "GCC_ARM", "IAR"],
        "extra_labels": ["NXP", "LPC176X", "XBED_LPC1768"],
        "macros": ["TARGET_LPC1768"],
        "detect_code": ["1010"],
        "device_has": ["ANALOGIN", "ANALOGOUT", "CAN", "DEBUG_AWARENESS", "ETHERNET", "I2C", "I2CSLAVE", "INTERRUPTIN", "LOCALFILESYSTEM", "PORTIN", "PORTINOUT", "PORTOUT", "PWMOUT", "SEMIHOST", "SERIAL", "SERIAL_FC", "SLEEP", "SPI", "SPISLAVE", "STDIO_MESSAGES", "FLASH"],
        "device_name": "LPC1768"
    },
    "LPC810": {
        "inherits": ["LPCTarget"],
        "core": "Cortex-M0+",
        "default_toolchain": "uARM",
        "extra_labels": ["NXP", "LPC81X"],
        "is_disk_virtual": true,
        "supported_toolchains": ["uARM", "IAR", "GCC_ARM"],
        "device_has": ["I2C", "I2CSLAVE", "INTERRUPTIN", "PWMOUT", "SERIAL", "SERIAL_FC", "SLEEP", "SPI", "SPISLAVE"],
        "default_lib": "small",
        "device_name": "LPC810M021FN8"
    },
    "LPC812": {
        "supported_form_factors": ["ARDUINO"],
        "core": "Cortex-M0+",
        "default_toolchain": "uARM",
        "extra_labels": ["NXP", "LPC81X"],
        "is_disk_virtual": true,
        "supported_toolchains": ["uARM", "IAR", "GCC_ARM"],
        "inherits": ["LPCTarget"],
        "detect_code": ["1050"],
        "device_has": ["I2C", "I2CSLAVE", "INTERRUPTIN", "PWMOUT", "SERIAL", "SERIAL_FC", "SLEEP", "SPI", "SPISLAVE"],
        "default_lib": "small",
        "release_versions": ["2"],
        "device_name": "LPC812M101JDH20"
    },
    "LPC824": {
        "supported_form_factors": ["ARDUINO"],
        "core": "Cortex-M0+",
        "default_toolchain": "uARM",
        "extra_labels": ["NXP", "LPC82X"],
        "is_disk_virtual": true,
        "supported_toolchains": ["uARM", "GCC_ARM", "IAR"],
        "inherits": ["LPCTarget"],
        "device_has": ["ANALOGIN", "I2C", "I2CSLAVE", "INTERRUPTIN", "PWMOUT", "SERIAL", "SLEEP", "SPI", "SPISLAVE"],
        "default_lib": "small",
        "release_versions": ["2"],
        "device_name": "LPC824M201JDH20"
    },
    "SSCI824": {
        "inherits": ["LPCTarget"],
        "core": "Cortex-M0+",
        "default_toolchain": "uARM",
        "extra_labels": ["NXP", "LPC82X"],
        "is_disk_virtual": true,
        "supported_toolchains": ["uARM", "GCC_ARM"],
        "device_has": ["ANALOGIN", "I2C", "I2CSLAVE", "INTERRUPTIN", "PWMOUT", "SERIAL", "SLEEP", "SPI", "SPISLAVE"],
        "default_lib": "small",
        "release_versions": ["2"]
    },
    "MCU_LPC4088": {
        "inherits": ["LPCTarget"],
        "core": "Cortex-M4F",
        "extra_labels": ["NXP", "LPC408X", "NXP_EMAC"],
        "is_disk_virtual": true,
        "supported_toolchains": ["ARM", "GCC_ARM", "IAR"],
        "post_binary_hook": {
            "function": "LPC4088Code.binary_hook"
        },
        "device_has": ["ANALOGIN", "ANALOGOUT", "CAN", "DEBUG_AWARENESS", "EMAC", "ETHERNET", "I2C", "I2CSLAVE", "INTERRUPTIN", "PORTIN", "PORTINOUT", "PORTOUT", "PWMOUT", "SERIAL", "SLEEP", "SPI", "SPISLAVE", "STDIO_MESSAGES"],
        "device_name": "LPC4088FBD144",
        "overrides": {
            "network-default-interface-type": "ETHERNET"
        }
    },
    "LPC4088": {
        "inherits": ["MCU_LPC4088"],
        "release_versions": ["2", "5"]
    },
    "LPC4088_DM": {
        "inherits": ["MCU_LPC4088"],
        "release_versions": ["2", "5"]
    },
    "LPC4330_M4": {
        "inherits": ["LPCTarget"],
        "core": "Cortex-M4F",
        "extra_labels": ["NXP", "LPC43XX", "LPC4330"],
        "supported_toolchains": ["ARM", "IAR", "GCC_ARM"],
        "device_has": ["ANALOGIN", "ANALOGOUT", "DEBUG_AWARENESS", "ETHERNET", "I2C", "I2CSLAVE", "INTERRUPTIN", "PORTIN", "PORTINOUT", "PORTOUT", "PWMOUT", "SERIAL", "SLEEP", "SPI", "SPISLAVE", "STDIO_MESSAGES"],
        "device_name": "LPC4330"
    },
    "LPC4330_M0": {
        "inherits": ["LPCTarget"],
        "core": "Cortex-M0",
        "extra_labels": ["NXP", "LPC43XX", "LPC4330"],
        "supported_toolchains": ["ARM", "IAR"],
        "device_has": ["ANALOGIN", "ANALOGOUT", "DEBUG_AWARENESS", "ETHERNET", "I2C", "I2CSLAVE", "INTERRUPTIN", "PORTIN", "PORTINOUT", "PORTOUT", "PWMOUT", "SERIAL", "SLEEP", "SPI", "SPISLAVE", "STDIO_MESSAGES"]
    },
    "LPC4337": {
        "inherits": ["LPCTarget"],
        "core": "Cortex-M4F",
        "extra_labels": ["NXP", "LPC43XX", "LPC4337"],
        "supported_toolchains": ["ARM"],
        "device_has": ["ANALOGIN", "ANALOGOUT", "DEBUG_AWARENESS", "ETHERNET", "I2C", "I2CSLAVE", "INTERRUPTIN", "PORTIN", "PORTINOUT", "PORTOUT", "PWMOUT", "SERIAL", "SLEEP", "SPI", "SPISLAVE", "STDIO_MESSAGES"],
        "release_versions": ["2"],
        "device_name": "LPC4337"
    },
    "LPC1800": {
        "inherits": ["LPCTarget"],
        "core": "Cortex-M3",
        "extra_labels": ["NXP", "LPC43XX"],
        "public": false,
        "supported_toolchains": ["ARM", "IAR"]
    },
    "LPC11U37H_401": {
        "supported_form_factors": ["ARDUINO"],
        "core": "Cortex-M0",
        "default_toolchain": "uARM",
        "extra_labels": ["NXP", "LPC11UXX"],
        "macros": ["CMSIS_VECTAB_VIRTUAL", "CMSIS_VECTAB_VIRTUAL_HEADER_FILE=\"cmsis_nvic.h\""],
        "supported_toolchains": ["ARM", "uARM", "GCC_ARM"],
        "inherits": ["LPCTarget"],
        "device_has": ["ANALOGIN", "I2C", "I2CSLAVE", "INTERRUPTIN", "PORTIN", "PORTINOUT", "PORTOUT", "PWMOUT", "SERIAL", "SLEEP", "SPI", "SPISLAVE"],
        "default_lib": "small",
        "release_versions": ["2"],
        "device_name": "LPC11U37HFBD64/401"
    },
    "ELEKTOR_COCORICO": {
        "core": "Cortex-M0+",
        "default_toolchain": "uARM",
        "extra_labels": ["NXP", "LPC81X"],
        "supported_toolchains": ["uARM", "GCC_ARM", "IAR"],
        "inherits": ["LPCTarget"],
        "is_disk_virtual": true,
        "detect_code": ["C000"],
        "default_lib": "small",
        "device_name": "LPC812M101JDH16"
    },
    "KL05Z": {
        "supported_form_factors": ["ARDUINO"],
        "core": "Cortex-M0+",
        "default_toolchain": "uARM",
        "extra_labels": ["Freescale", "KLXX"],
        "is_disk_virtual": true,
        "supported_toolchains": ["ARM", "uARM", "GCC_ARM", "IAR"],
        "inherits": ["Target"],
        "device_has": ["USTICKER", "ANALOGIN", "ANALOGOUT", "I2C", "I2CSLAVE", "INTERRUPTIN", "PORTIN", "PORTINOUT", "PORTOUT", "PWMOUT", "SEMIHOST", "SERIAL", "SLEEP", "SPI", "SPISLAVE", "STDIO_MESSAGES"],
        "default_lib": "small",
        "release_versions": ["2"],
        "device_name": "MKL05Z32xxx4"
    },
    "KL25Z": {
        "supported_form_factors": ["ARDUINO"],
        "core": "Cortex-M0+",
        "extra_labels": ["Freescale", "KLXX"],
        "is_disk_virtual": true,
        "supported_toolchains": ["ARM", "GCC_ARM", "IAR"],
        "inherits": ["Target"],
        "detect_code": ["0200"],
        "device_has": ["USTICKER", "ANALOGIN", "ANALOGOUT", "I2C", "I2CSLAVE", "INTERRUPTIN", "PORTIN", "PORTINOUT", "PORTOUT", "PWMOUT", "SEMIHOST", "SERIAL", "SLEEP", "SPI", "SPISLAVE", "STDIO_MESSAGES"],
        "release_versions": ["2", "5"],
        "device_name": "MKL25Z128xxx4"
    },
    "KL26Z": {
        "supported_form_factors": ["ARDUINO"],
        "core": "Cortex-M0+",
        "extra_labels": ["Freescale", "KLXX"],
        "is_disk_virtual": true,
        "supported_toolchains": ["ARM", "GCC_ARM", "IAR"],
        "inherits": ["Target"],
        "device_has": ["USTICKER", "ANALOGIN", "ANALOGOUT", "I2C", "I2CSLAVE", "INTERRUPTIN", "PORTIN", "PORTINOUT", "PORTOUT", "PWMOUT", "SEMIHOST", "SERIAL", "SLEEP", "SPI", "SPISLAVE", "STDIO_MESSAGES"],
        "device_name": "MKL26Z128xxx4"
    },
    "KL46Z": {
        "supported_form_factors": ["ARDUINO"],
        "core": "Cortex-M0+",
        "extra_labels": ["Freescale", "KLXX", "FLASH_CMSIS_ALGO"],
        "is_disk_virtual": true,
        "supported_toolchains": ["GCC_ARM", "ARM", "IAR"],
        "inherits": ["Target"],
        "detect_code": ["0220"],
        "device_has": ["USTICKER", "ANALOGIN", "ANALOGOUT", "I2C", "I2CSLAVE", "INTERRUPTIN", "PORTIN", "PORTINOUT", "PORTOUT", "PWMOUT", "SEMIHOST", "SERIAL", "SLEEP", "SPI", "SPISLAVE", "STDIO_MESSAGES", "FLASH"],
        "release_versions": ["2", "5"],
        "device_name": "MKL46Z256xxx4",
        "bootloader_supported": true
    },
    "K20D50M": {
        "inherits": ["Target"],
        "core": "Cortex-M4",
        "extra_labels": ["Freescale", "K20XX"],
        "is_disk_virtual": true,
        "supported_toolchains": ["GCC_ARM", "ARM", "IAR"],
        "detect_code": ["0230"],
        "device_has": ["ANALOGIN", "I2C", "I2CSLAVE", "INTERRUPTIN", "PORTIN", "PORTINOUT", "PORTOUT", "PWMOUT", "SEMIHOST", "SERIAL", "SLEEP", "SPI", "SPISLAVE", "STDIO_MESSAGES"],
        "release_versions": ["2"],
        "device_name": "MK20DX128xxx5"
    },
    "TEENSY3_1": {
        "inherits": ["Target"],
        "core": "Cortex-M4",
        "extra_labels": ["Freescale", "K20XX", "K20DX256"],
        "OUTPUT_EXT": "hex",
        "is_disk_virtual": true,
        "supported_toolchains": ["GCC_ARM", "ARM"],
        "post_binary_hook": {
            "function": "TEENSY3_1Code.binary_hook",
            "toolchains": ["ARM_STD", "ARM_MICRO", "GCC_ARM"]
        },
        "detect_code": ["0230"],
        "device_has": ["ANALOGIN", "ANALOGOUT", "I2C", "I2CSLAVE", "INTERRUPTIN", "PORTIN", "PORTINOUT", "PORTOUT", "PWMOUT", "SEMIHOST", "SERIAL", "SLEEP", "SPI", "SPISLAVE", "STDIO_MESSAGES"],
        "release_versions": ["2"],
        "device_name": "MK20DX256xxx7"
    },
    "MCU_K22F512": {
        "core": "Cortex-M4F",
        "supported_toolchains": ["ARM", "GCC_ARM", "IAR"],
        "extra_labels": ["Freescale", "MCUXpresso_MCUS", "KSDK2_MCUS", "MCU_K22F", "MCU_K22F512", "FRDM", "KPSDK_MCUS", "KPSDK_CODE"],
        "is_disk_virtual": true,
        "public": false,
        "macros": ["CPU_MK22FN512VLH12", "FSL_RTOS_MBED"],
        "inherits": ["Target"],
        "detect_code": ["0231"],
        "device_has": ["USTICKER", "LPTICKER", "RTC", "ANALOGIN", "ANALOGOUT", "I2C", "I2CSLAVE", "INTERRUPTIN", "PORTIN", "PORTINOUT", "PORTOUT", "PWMOUT", "SERIAL", "SLEEP", "SPI", "SPISLAVE", "STDIO_MESSAGES", "TRNG", "FLASH"],
        "device_name": "MK22DN512xxx5"
    },
    "K22F": {
        "supported_form_factors": ["ARDUINO"],
        "inherits": ["MCU_K22F512"],
        "release_versions": ["2", "5"],
        "extra_labels_add": ["FRDM"]
    },
    "KL27Z": {
        "inherits": ["Target"],
        "core": "Cortex-M0+",
        "extra_labels": ["Freescale", "MCUXpresso_MCUS", "KSDK2_MCUS", "FRDM"],
        "macros": ["CPU_MKL27Z64VLH4", "FSL_RTOS_MBED"],
        "supported_toolchains": ["ARM", "GCC_ARM", "IAR"],
        "supported_form_factors": ["ARDUINO"],
        "is_disk_virtual": true,
        "default_toolchain": "ARM",
        "detect_code": ["0261"],
        "device_has": ["USTICKER", "LPTICKER", "RTC", "ANALOGIN", "I2C", "I2CSLAVE", "INTERRUPTIN", "PORTIN", "PORTOUT", "PWMOUT", "SERIAL", "SLEEP", "SPI", "SPISLAVE", "STDIO_MESSAGES"],
        "default_lib": "std",
        "release_versions": ["2"],
        "device_name": "MKL27Z64xxx4"
    },
    "KL43Z": {
        "supported_form_factors": ["ARDUINO"],
        "core": "Cortex-M0+",
        "supported_toolchains": ["GCC_ARM", "ARM", "IAR"],
        "extra_labels": ["Freescale", "MCUXpresso_MCUS", "KSDK2_MCUS", "FRDM"],
        "macros": ["CPU_MKL43Z256VLH4", "FSL_RTOS_MBED"],
        "is_disk_virtual": true,
        "inherits": ["Target"],
        "detect_code": ["0262"],
        "device_has": ["USTICKER", "LPTICKER", "RTC", "ANALOGIN", "ANALOGOUT", "I2C", "I2CSLAVE", "INTERRUPTIN", "PORTIN", "PORTINOUT", "PORTOUT", "PWMOUT", "SEMIHOST", "SERIAL", "SLEEP", "SPI", "SPISLAVE", "STDIO_MESSAGES", "FLASH"],
        "release_versions": ["2", "5"],
        "device_name": "MKL43Z256xxx4"
    },
    "KL82Z": {
        "supported_form_factors": ["ARDUINO"],
        "core": "Cortex-M0+",
        "supported_toolchains": ["GCC_ARM", "ARM", "IAR"],
        "extra_labels": ["Freescale", "MCUXpresso_MCUS", "KSDK2_MCUS", "FRDM"],
        "macros": ["CPU_MKL82Z128VLK7", "FSL_RTOS_MBED"],
        "is_disk_virtual": true,
        "inherits": ["Target"],
        "detect_code": ["0218"],
        "device_has": ["USTICKER", "LPTICKER", "RTC", "ANALOGIN", "ANALOGOUT", "I2C", "I2CSLAVE", "INTERRUPTIN", "PORTIN", "PORTINOUT", "PORTOUT", "PWMOUT", "SEMIHOST", "SERIAL", "SLEEP", "SPI", "SPISLAVE", "STDIO_MESSAGES", "TRNG", "FLASH", "QSPI"],
        "release_versions": ["2", "5"],
        "device_name": "MKL82Z128xxx7"
    },
    "USENSE": {
        "inherits": ["KL82Z"],
        "extra_labels_remove": ["FRDM"],
        "device_has_remove": ["QSPI"],
        "supported_form_factors": []
    },
    "KW24D": {
        "supported_form_factors": ["ARDUINO"],
        "core": "Cortex-M4",
        "supported_toolchains": ["ARM", "GCC_ARM", "IAR"],
        "extra_labels": ["Freescale", "MCUXpresso_MCUS", "KSDK2_MCUS", "FRDM"],
        "is_disk_virtual": true,
        "macros": ["CPU_MKW24D512VHA5", "FSL_RTOS_MBED"],
        "inherits": ["Target"],
        "detect_code": ["0250"],
        "device_has": ["USTICKER", "LPTICKER", "RTC", "ANALOGIN", "I2C", "I2CSLAVE", "INTERRUPTIN", "PORTIN", "PORTINOUT", "PORTOUT", "PWMOUT", "SERIAL", "SERIAL_FC", "SLEEP", "SPI", "SPISLAVE", "STDIO_MESSAGES", "TRNG", "FLASH", "802_15_4_PHY"],
        "release_versions": ["2", "5"],
        "device_name": "MKW24D512xxx5",
        "bootloader_supported": true,
        "overrides": {
            "network-default-interface-type": "MESH"
        }
    },
    "KW41Z": {
        "supported_form_factors": ["ARDUINO"],
        "core": "Cortex-M0+",
        "supported_toolchains": ["ARM", "GCC_ARM", "IAR"],
        "extra_labels": ["Freescale", "MCUXpresso_MCUS", "KSDK2_MCUS", "FRDM"],
        "is_disk_virtual": true,
        "macros": ["CPU_MKW41Z512VHT4", "FSL_RTOS_MBED"],
        "inherits": ["Target"],
        "detect_code": ["0201"],
        "device_has": ["USTICKER", "LPTICKER", "RTC", "ANALOGIN", "ANALOGOUT", "I2C", "I2CSLAVE", "INTERRUPTIN", "PORTIN", "PORTINOUT", "PORTOUT", "PWMOUT", "SERIAL", "SLEEP", "SPI", "SPISLAVE", "TRNG", "STDIO_MESSAGES", "FLASH"],
        "release_versions": ["2", "5"],
        "device_name": "MKW41Z512xxx4"
    },
    "MCU_K24F1M": {
        "core": "Cortex-M4F",
        "supported_toolchains": ["ARM", "GCC_ARM", "IAR"],
        "extra_labels": ["Freescale", "MCUXpresso_MCUS", "KSDK2_MCUS", "MCU_K24F", "KPSDK_MCUS", "KPSDK_CODE"],
        "is_disk_virtual": true,
        "public": false,
        "macros": ["CPU_MK24FN1M0VDC12", "FSL_RTOS_MBED"],
        "inherits": ["Target"],
        "device_has": ["USTICKER", "LPTICKER", "RTC", "ANALOGIN", "ANALOGOUT", "I2C", "I2CSLAVE", "INTERRUPTIN", "PORTIN", "PORTINOUT", "PORTOUT", "PWMOUT", "SERIAL", "SERIAL_FC", "SERIAL_ASYNCH", "SLEEP", "SPI", "SPI_ASYNCH", "SPISLAVE", "STDIO_MESSAGES", "TRNG", "FLASH"],
        "device_name": "MK24FN1M0xxx12"
    },
    "RO359B": {
        "supported_form_factors": ["ARDUINO"],
        "inherits": ["MCU_K24F1M"],
        "detect_code": ["1022"],
        "release_versions": ["2", "5"]
    },
    "K64F": {
        "supported_form_factors": ["ARDUINO"],
        "components": ["SD"],
        "core": "Cortex-M4F",
        "supported_toolchains": ["ARM", "GCC_ARM", "IAR"],
        "extra_labels": ["Freescale", "MCUXpresso_MCUS", "KSDK2_MCUS", "FRDM", "KPSDK_MCUS", "KPSDK_CODE", "MCU_K64F", "Freescale_EMAC"],
        "is_disk_virtual": true,
        "macros": ["CPU_MK64FN1M0VMD12", "FSL_RTOS_MBED"],
        "inherits": ["Target"],
        "detect_code": ["0240"],
        "device_has": ["USTICKER", "LPTICKER", "RTC", "CRC", "ANALOGIN", "ANALOGOUT", "EMAC", "I2C", "I2CSLAVE", "INTERRUPTIN", "PORTIN", "PORTINOUT", "PORTOUT", "PWMOUT", "SERIAL", "SERIAL_FC", "SERIAL_ASYNCH", "SLEEP", "SPI", "SPI_ASYNCH", "SPISLAVE", "STDIO_MESSAGES", "STORAGE", "TRNG", "FLASH"],
        "features": ["STORAGE"],
        "release_versions": ["2", "5"],
        "device_name": "MK64FN1M0xxx12",
        "bootloader_supported": true,
        "overrides": {
            "network-default-interface-type": "ETHERNET"
        }
    },
    "SDT64B": {
        "inherits": ["K64F"],
        "extra_labels_add": ["K64F"],
        "extra_labels_remove": ["FRDM"],
        "components_remove": ["SD"],
        "supported_form_factors": [],
        "detect_code": ["3105"]
    },
    "EV_COG_AD4050LZ": {
        "inherits": ["Target"],
        "core": "Cortex-M4F",
        "supported_toolchains": ["ARM", "GCC_ARM", "IAR"],
        "macros": ["__ADUCM4050__", "EV_COG_AD4050LZ"],
        "extra_labels": ["Analog_Devices", "ADUCM4X50", "ADUCM4050", "EV_COG_AD4050LZ", "FLASH_CMSIS_ALGO"],
        "device_has": ["FLASH", "USTICKER", "RTC", "SERIAL", "STDIO_MESSAGES", "TRNG", "SLEEP", "INTERRUPTIN", "SPI", "I2C", "ANALOGIN"],
        "device_name": "ADuCM4050",
        "detect_code": ["0603"],
        "release_versions": ["5"],
        "bootloader_supported": true
    },
    "EV_COG_AD3029LZ": {
        "inherits": ["Target"],
        "core": "Cortex-M3",
        "supported_toolchains": ["ARM", "GCC_ARM", "IAR"],
        "macros": ["__ADUCM3029__", "EV_COG_AD3029LZ"],
        "extra_labels": ["Analog_Devices", "ADUCM302X", "ADUCM3029", "EV_COG_AD3029LZ", "FLASH_CMSIS_ALGO"],
        "device_has": ["FLASH", "USTICKER", "RTC", "SERIAL", "STDIO_MESSAGES", "TRNG", "SLEEP", "INTERRUPTIN", "SPI", "I2C", "ANALOGIN"],
        "device_name": "ADuCM3029",
        "detect_code": ["0602"],
        "release_versions": ["5"],
        "bootloader_supported": true
    },
    "MTS_GAMBIT": {
        "inherits": ["Target"],
        "core": "Cortex-M4F",
        "supported_toolchains": ["ARM", "GCC_ARM"],
        "extra_labels": ["Freescale", "MCUXpresso_MCUS", "KSDK2_MCUS", "KPSDK_MCUS", "KPSDK_CODE", "MCU_K64F"],
        "is_disk_virtual": true,
        "macros": ["CPU_MK64FN1M0VMD12", "FSL_RTOS_MBED", "TARGET_K64F"],
        "device_has": ["USTICKER", "LPTICKER", "RTC", "I2C", "I2CSLAVE", "INTERRUPTIN", "PORTIN", "PORTINOUT", "PORTOUT", "SERIAL", "SERIAL_ASYNCH", "SLEEP", "SPI", "SPI_ASYNCH", "SPISLAVE", "STDIO_MESSAGES", "FLASH"],
        "device_name": "MK64FN1M0xxx12"
    },
    "HEXIWEAR": {
        "inherits": ["Target"],
        "core": "Cortex-M4F",
        "extra_labels": ["Freescale", "MCUXpresso_MCUS", "KSDK2_MCUS", "MCU_K64F"],
        "supported_toolchains": ["ARM", "GCC_ARM", "IAR"],
        "macros": ["CPU_MK64FN1M0VMD12", "FSL_RTOS_MBED", "TARGET_K64F"],
        "is_disk_virtual": true,
        "default_toolchain": "ARM",
        "detect_code": ["0214"],
        "device_has": ["USTICKER", "LPTICKER", "RTC", "ANALOGIN", "ANALOGOUT", "I2C", "I2CSLAVE", "INTERRUPTIN", "PORTIN", "PORTINOUT", "PORTOUT", "PWMOUT", "SERIAL", "SERIAL_ASYNCH", "SERIAL_FC", "SLEEP", "SPI", "SPI_ASYNCH", "SPISLAVE", "STDIO_MESSAGES", "TRNG", "FLASH"],
        "default_lib": "std",
        "release_versions": ["2", "5"],
        "device_name": "MK64FN1M0xxx12",
        "bootloader_supported": true
    },
    "RAPIDIOT": {
        "inherits": ["Target"],
        "public": false,
        "core": "null",
        "supported_toolchains": ["ARM", "GCC_ARM", "IAR"],
        "macros": ["FSL_RTOS_MBED", "USE_EXTERNAL_RTC"],
        "default_toolchain": "ARM",
        "default_lib": "std",
        "release_versions": ["2", "5"]
    },
    "RAPIDIOT_K64F": {
        "inherits": ["RAPIDIOT"],
        "core": "Cortex-M4F",
        "extra_labels": ["Freescale", "MCUXpresso_MCUS", "KSDK2_MCUS", "MCU_K64F"],
        "macros_add": ["CPU_MK64FN1M0VMD12", "TARGET_K64F"],
        "is_disk_virtual": true,
        "mbed_rom_start": "0x00014000",
        "mbed_rom_size": "0xEC000",
        "detect_code": ["0228"],
        "device_has": ["USTICKER", "LPTICKER", "ANALOGIN", "ANALOGOUT", "I2C", "I2CSLAVE", "INTERRUPTIN", "PORTIN", "PORTINOUT", "PORTOUT", "PWMOUT", "SERIAL", "SERIAL_ASYNCH", "SERIAL_FC", "SLEEP", "SPI", "SPI_ASYNCH", "SPISLAVE", "STDIO_MESSAGES", "TRNG", "FLASH"],
        "forced_reset_timeout": 7,
        "device_name": "MK64FN1M0xxx12",
        "bootloader_supported": true
    },
    "K66F": {
        "supported_form_factors": ["ARDUINO"],
        "components": ["SD"],
        "core": "Cortex-M4F",
        "supported_toolchains": ["ARM", "GCC_ARM", "IAR"],
        "extra_labels": ["Freescale", "MCUXpresso_MCUS", "KSDK2_MCUS", "FRDM", "Freescale_EMAC"],
        "is_disk_virtual": true,
        "macros": ["CPU_MK66FN2M0VMD18", "FSL_RTOS_MBED"],
        "inherits": ["Target"],
        "detect_code": ["0311"],
        "device_has": ["USTICKER", "LPTICKER", "RTC", "ANALOGIN", "ANALOGOUT", "EMAC", "I2C", "I2CSLAVE", "INTERRUPTIN", "PORTIN", "PORTINOUT", "PORTOUT", "PWMOUT", "SERIAL", "SERIAL_FC", "SLEEP", "SPI", "SPISLAVE", "STDIO_MESSAGES", "TRNG", "FLASH"],
        "release_versions": ["2", "5"],
        "device_name": "MK66FN2M0xxx18",
        "bootloader_supported": true,
        "overrides": {
            "network-default-interface-type": "ETHERNET"
        }
    },
    "K82F": {
        "supported_form_factors": ["ARDUINO"],
        "components": ["SPIF"],
        "core": "Cortex-M4F",
        "supported_toolchains": ["ARM", "GCC_ARM", "IAR"],
        "extra_labels": ["Freescale", "MCUXpresso_MCUS", "KSDK2_MCUS", "FRDM"],
        "is_disk_virtual": true,
        "macros": ["CPU_MK82FN256VDC15", "FSL_RTOS_MBED"],
        "inherits": ["Target"],
        "detect_code": ["0217"],
        "device_has": ["USTICKER", "LPTICKER", "RTC", "ANALOGIN", "ANALOGOUT", "I2C", "I2CSLAVE", "INTERRUPTIN", "PORTIN", "PORTINOUT", "PORTOUT", "PWMOUT", "SERIAL", "SLEEP", "SPI", "SPISLAVE", "STDIO_MESSAGES", "TRNG", "FLASH", "QSPI"],
        "release_versions": ["2", "5"],
        "device_name": "MK82FN256xxx15"
    },
    "UBRIDGE": {
        "inherits": ["K82F"],
        "extra_labels_remove": ["FRDM"],
        "components_remove": ["SPIF"],
        "device_has_remove": ["QSPI"],
        "supported_form_factors": []
    },
    "FAMILY_STM32": {
        "inherits": ["Target"],
        "public": false,
        "extra_labels": ["STM"],
        "supported_toolchains": ["ARM", "uARM", "IAR", "GCC_ARM"],
        "macros": ["TRANSACTION_QUEUE_SIZE_SPI=2"],
        "config": {
            "lse_available": {
                "help": "Define if a Low Speed External xtal (LSE) is available on the board (0 = No, 1 = Yes). If Yes, the LSE will be used to clock the RTC, LPUART, ... otherwise the Low Speed Internal clock (LSI) will be used",
                "value": "1"
            },
            "lpuart_clock_source": {
                "help": "Define the LPUART clock source. Mask values: USE_LPUART_CLK_LSE, USE_LPUART_CLK_PCLK1, USE_LPUART_CLK_HSI",
                "value": "USE_LPUART_CLK_LSE|USE_LPUART_CLK_PCLK1"
            },
            "stdio_uart_tx": {
                "help": "default TX STDIO pins is defined in PinNames.h file, but it can be overridden"
            },
            "stdio_uart_rx": {
                "help": "default RX STDIO pins is defined in PinNames.h file, but it can be overridden"
            },
            "lpticker_delay_ticks": {
                "help": "https://os.mbed.com/docs/latest/porting/low-power-ticker.html",
                "value": 1,
                "macro_name": "LPTICKER_DELAY_TICKS"
             }
        },
        "device_has": ["USTICKER", "LPTICKER", "RTC", "ANALOGIN", "I2C", "I2CSLAVE", "I2C_ASYNCH", "INTERRUPTIN", "PORTIN", "PORTINOUT", "PORTOUT", "PWMOUT", "SERIAL", "SLEEP", "SPI", "SPISLAVE", "SPI_ASYNCH", "STDIO_MESSAGES"]
    },
    "MIMXRT1050_EVK": {
        "supported_form_factors": ["ARDUINO"],
        "core": "Cortex-M7FD",
        "supported_toolchains": ["ARM", "GCC_ARM", "IAR"],
        "extra_labels": ["NXP", "MCUXpresso_MCUS", "EVK", "MIMXRT1050", "IMX"],
        "is_disk_virtual": true,
        "macros": ["CPU_MIMXRT1052DVL6B", "FSL_RTOS_MBED", "XIP_BOOT_HEADER_ENABLE=1", "XIP_EXTERNAL_FLASH=1", "XIP_BOOT_HEADER_DCD_ENABLE=1", "SKIP_SYSCLK_INIT"],
        "inherits": ["Target"],
        "detect_code": ["0227"],
        "device_has": ["RTC", "SLEEP", "USTICKER", "LPTICKER", "ANALOGIN", "I2C", "I2CSLAVE", "ERROR_RED", "INTERRUPTIN", "PORTIN", "PORTINOUT", "PORTOUT", "PWMOUT", "SERIAL", "SPI", "SPISLAVE", "STDIO_MESSAGES"],
        "release_versions": ["2", "5"],
        "device_name": "MIMXRT1052"
    },
    "LPC54114": {
        "supported_form_factors": ["ARDUINO"],
        "core": "Cortex-M4F",
        "supported_toolchains": ["ARM", "IAR", "GCC_ARM"],
        "extra_labels": ["NXP", "MCUXpresso_MCUS", "LPC54114_M4", "LPCXpresso", "LPC"],
        "is_disk_virtual": true,
        "macros": ["CPU_LPC54114J256BD64_cm4", "FSL_RTOS_MBED"],
        "inherits": ["Target"],
        "detect_code": ["1054"],
        "device_has": ["USTICKER", "RTC", "ANALOGIN", "I2C", "I2CSLAVE", "INTERRUPTIN", "PORTIN", "PORTINOUT", "PORTOUT", "SERIAL", "SLEEP", "SPI", "SPISLAVE", "STDIO_MESSAGES", "FLASH"],
        "release_versions": ["2", "5"],
        "post_binary_hook": {"function": "LPCTargetCode.lpc_patch"},
        "device_name" : "LPC54114J256BD64"
    },
    "MCU_LPC546XX": {
        "core": "Cortex-M4F",
        "supported_toolchains": ["ARM", "IAR", "GCC_ARM"],
        "extra_labels": ["NXP", "MCUXpresso_MCUS", "LPCXpresso", "LPC", "LPC546XX", "NXP_EMAC"],
        "is_disk_virtual": true,
        "macros": ["CPU_LPC54628J512ET180", "FSL_RTOS_MBED"],
        "inherits": ["Target"],
        "device_has": ["USTICKER", "RTC", "ANALOGIN", "EMAC", "I2C", "I2CSLAVE", "INTERRUPTIN", "PORTIN", "PORTINOUT", "PORTOUT", "SERIAL", "SLEEP", "SPI", "SPISLAVE", "STDIO_MESSAGES", "FLASH", "TRNG"],
        "device_name" : "LPC54628J512ET180",
        "post_binary_hook": {"function": "LPCTargetCode.lpc_patch"},
        "overrides": {
            "network-default-interface-type": "ETHERNET"
        }
    },
    "LPC546XX": {
        "supported_form_factors": ["ARDUINO"],
        "inherits": ["MCU_LPC546XX"],
        "detect_code": ["1056"],
        "release_versions": ["2", "5"]
    },
    "FF_LPC546XX": {
        "inherits": ["MCU_LPC546XX"],
        "extra_labels_remove" : ["LPCXpresso"],
        "detect_code": ["8081"],
        "release_versions": ["2", "5"]
    },
    "NUCLEO_F030R8": {
        "inherits": ["FAMILY_STM32"],
        "supported_form_factors": ["ARDUINO", "MORPHO"],
        "core": "Cortex-M0",
        "extra_labels_add": ["STM32F0", "STM32F030R8"],
        "config": {
            "clock_source": {
                "help": "Mask value : USE_PLL_HSE_EXTC | USE_PLL_HSE_XTAL (need HW patch) | USE_PLL_HSI",
                "value": "USE_PLL_HSE_EXTC|USE_PLL_HSI",
                "macro_name": "CLOCK_SOURCE"
            }
        },
        "detect_code": ["0725"],
        "macros_add": ["CMSIS_VECTAB_VIRTUAL", "CMSIS_VECTAB_VIRTUAL_HEADER_FILE=\"cmsis_nvic.h\""],
        "device_has_add": ["CRC", "SERIAL_FC"],
        "device_has_remove": ["LPTICKER"],
        "default_lib": "small",
        "release_versions": ["2"],
        "device_name": "STM32F030R8"
    },
    "NUCLEO_F031K6": {
        "inherits": ["FAMILY_STM32"],
        "supported_form_factors": ["ARDUINO"],
        "core": "Cortex-M0",
        "default_toolchain": "uARM",
        "extra_labels_add": ["STM32F0", "STM32F031K6"],
        "config": {
            "clock_source": {
                "help": "Mask value : USE_PLL_HSE_EXTC (need HW patch) | USE_PLL_HSE_XTAL (need HW patch) | USE_PLL_HSI",
                "value": "USE_PLL_HSI",
                "macro_name": "CLOCK_SOURCE"
            }
        },
        "detect_code": ["0791"],
        "overrides": {"lse_available": 0},
        "macros_add": ["CMSIS_VECTAB_VIRTUAL", "CMSIS_VECTAB_VIRTUAL_HEADER_FILE=\"cmsis_nvic.h\""],
        "device_has_add": ["CRC", "SERIAL_FC"],
        "device_has_remove": ["LPTICKER"],
        "default_lib": "small",
        "release_versions": ["2"],
        "device_name": "STM32F031K6"
    },
    "NUCLEO_F042K6": {
        "inherits": ["FAMILY_STM32"],
        "supported_form_factors": ["ARDUINO"],
        "core": "Cortex-M0",
        "default_toolchain": "uARM",
        "extra_labels_add": ["STM32F0", "STM32F042K6"],
        "config": {
            "clock_source": {
                "help": "Mask value : USE_PLL_HSE_EXTC (need HW patch) | USE_PLL_HSE_XTAL (need HW patch) | USE_PLL_HSI",
                "value": "USE_PLL_HSI",
                "macro_name": "CLOCK_SOURCE"
            }
        },
        "detect_code": ["0785"],
        "overrides": {"lse_available": 0},
        "macros_add": ["CMSIS_VECTAB_VIRTUAL", "CMSIS_VECTAB_VIRTUAL_HEADER_FILE=\"cmsis_nvic.h\""],
        "device_has_add": ["CAN", "CRC", "SERIAL_FC"],
        "device_has_remove": ["LPTICKER"],
        "default_lib": "small",
        "release_versions": ["2"],
        "device_name": "STM32F042K6"
    },
    "NUCLEO_F070RB": {
        "inherits": ["FAMILY_STM32"],
        "supported_form_factors": ["ARDUINO", "MORPHO"],
        "core": "Cortex-M0",
        "extra_labels_add": ["STM32F0", "STM32F070RB"],
        "config": {
            "clock_source": {
                "help": "Mask value : USE_PLL_HSE_EXTC | USE_PLL_HSE_XTAL (need HW patch) | USE_PLL_HSI",
                "value": "USE_PLL_HSE_EXTC|USE_PLL_HSI",
                "macro_name": "CLOCK_SOURCE"
            }
        },
        "detect_code": ["0755"],
        "macros_add": ["CMSIS_VECTAB_VIRTUAL", "CMSIS_VECTAB_VIRTUAL_HEADER_FILE=\"cmsis_nvic.h\""],
        "device_has_add": ["CRC", "SERIAL_FC", "SERIAL_ASYNCH", "FLASH"],
        "release_versions": ["2", "5"],
        "device_name": "STM32F070RB"
    },
    "NUCLEO_F072RB": {
        "inherits": ["FAMILY_STM32"],
        "supported_form_factors": ["ARDUINO", "MORPHO"],
        "core": "Cortex-M0",
        "extra_labels_add": ["STM32F0", "STM32F072RB"],
        "config": {
            "clock_source": {
                "help": "Mask value : USE_PLL_HSE_EXTC | USE_PLL_HSE_XTAL (need HW patch) | USE_PLL_HSI",
                "value": "USE_PLL_HSE_EXTC|USE_PLL_HSI",
                "macro_name": "CLOCK_SOURCE"
            }
        },
        "detect_code": ["0730"],
        "macros_add": ["CMSIS_VECTAB_VIRTUAL", "CMSIS_VECTAB_VIRTUAL_HEADER_FILE=\"cmsis_nvic.h\""],
        "device_has_add": ["ANALOGOUT", "CAN", "CRC", "SERIAL_FC", "SERIAL_ASYNCH", "FLASH"],
        "release_versions": ["2", "5"],
        "device_name": "STM32F072RB"
    },
    "NUCLEO_F091RC": {
        "inherits": ["FAMILY_STM32"],
        "supported_form_factors": ["ARDUINO", "MORPHO"],
        "core": "Cortex-M0",
        "extra_labels_add": ["STM32F0", "STM32F091RC"],
        "config": {
            "clock_source": {
                "help": "Mask value : USE_PLL_HSE_EXTC | USE_PLL_HSE_XTAL (need HW patch) | USE_PLL_HSI",
                "value": "USE_PLL_HSE_EXTC|USE_PLL_HSI",
                "macro_name": "CLOCK_SOURCE"
            }
        },
        "detect_code": ["0750"],
        "macros_add": ["CMSIS_VECTAB_VIRTUAL", "CMSIS_VECTAB_VIRTUAL_HEADER_FILE=\"cmsis_nvic.h\""],
        "device_has_add": ["ANALOGOUT", "CAN", "CRC", "SERIAL_FC", "SERIAL_ASYNCH", "FLASH"],
        "release_versions": ["2", "5"],
        "device_name": "STM32F091RC"
    },
    "NUCLEO_F103RB": {
        "inherits": ["FAMILY_STM32"],
        "supported_form_factors": ["ARDUINO", "MORPHO"],
        "core": "Cortex-M3",
        "extra_labels_add": ["STM32F1", "STM32F103RB"],
        "config": {
            "clock_source": {
                "help": "Mask value : USE_PLL_HSE_EXTC (SYSCLK=72 MHz) | USE_PLL_HSE_XTAL (need HW patch) | USE_PLL_HSI (SYSCLK=64 MHz)",
                "value": "USE_PLL_HSE_EXTC|USE_PLL_HSI",
                "macro_name": "CLOCK_SOURCE"
            },
            "clock_source_usb": {
                "help": "In case of HSI clock source, to get 48 Mhz USB, SYSCLK has to be reduced from 64 to 48 MHz (set 0 for the max SYSCLK value)",
                "value": "0",
                "macro_name": "CLOCK_SOURCE_USB"
            }
        },
        "detect_code": ["0700"],
        "device_has_add": ["CAN", "SERIAL_FC", "SERIAL_ASYNCH", "FLASH"],
        "device_has_remove": ["LPTICKER"],
        "release_versions": ["2", "5"],
        "device_name": "STM32F103RB"
    },
    "NUCLEO_F207ZG": {
        "inherits": ["FAMILY_STM32"],
        "supported_form_factors": ["ARDUINO", "MORPHO"],
        "core": "Cortex-M3",
        "extra_labels_add": ["STM32F2", "STM32F207ZG", "STM_EMAC"],
        "config": {
            "d11_configuration": {
                "help": "Value: PA_7 for the default board configuration, PB_5 in case of solder bridge update (SB121 off/ SB122 on)",
                "value": "PA_7",
                "macro_name": "STM32_D11_SPI_ETHERNET_PIN"
            },
            "clock_source": {
                "help": "Mask value : USE_PLL_HSE_EXTC | USE_PLL_HSE_XTAL (need HW patch) | USE_PLL_HSI",
                "value": "USE_PLL_HSE_EXTC|USE_PLL_HSI",
                "macro_name": "CLOCK_SOURCE"
            }
        },
        "detect_code": ["0835"],
        "macros_add": ["USBHOST_OTHER"],
        "device_has_add": ["ANALOGOUT", "CAN", "EMAC", "SERIAL_ASYNCH", "SERIAL_FC", "FLASH"],
        "device_has_remove": ["LPTICKER"],
        "release_versions": ["2", "5"],
        "device_name": "STM32F207ZG",
        "bootloader_supported": true,
        "overrides": {
            "network-default-interface-type": "ETHERNET"
        }
    },
    "NUCLEO_F302R8": {
        "inherits": ["FAMILY_STM32"],
        "supported_form_factors": ["ARDUINO", "MORPHO"],
        "core": "Cortex-M4F",
        "extra_labels_add": ["STM32F3", "STM32F302x8", "STM32F302R8"],
        "config": {
            "clock_source": {
                "help": "Mask value : USE_PLL_HSE_EXTC | USE_PLL_HSE_XTAL (need HW patch) | USE_PLL_HSI",
                "value": "USE_PLL_HSE_EXTC|USE_PLL_HSI",
                "macro_name": "CLOCK_SOURCE"
            }
        },
        "detect_code": ["0705"],
        "device_has_add": ["ANALOGOUT", "CAN",  "CRC", "SERIAL_ASYNCH", "SERIAL_FC"],
        "default_lib": "small",
        "release_versions": ["2"],
        "device_name": "STM32F302R8"
    },
    "NUCLEO_F303K8": {
        "inherits": ["FAMILY_STM32"],
        "supported_form_factors": ["ARDUINO"],
        "core": "Cortex-M4F",
        "extra_labels_add": ["STM32F3", "STM32F303x8", "STM32F303K8"],
        "config": {
            "clock_source": {
                "help": "Mask value : USE_PLL_HSE_EXTC | USE_PLL_HSE_XTAL (need HW patch) | USE_PLL_HSI",
                "value": "USE_PLL_HSI",
                "macro_name": "CLOCK_SOURCE"
            }
        },
        "overrides": {"lse_available": 0},
        "detect_code": ["0775"],
        "default_lib": "small",
        "device_has_add": ["ANALOGOUT", "CAN", "CRC", "SERIAL_FC"],
        "release_versions": ["2"],
        "device_name": "STM32F303K8"
    },
    "NUCLEO_F303RE": {
        "inherits": ["FAMILY_STM32"],
        "supported_form_factors": ["ARDUINO", "MORPHO"],
        "core": "Cortex-M4F",
        "extra_labels_add": ["STM32F3", "STM32F303xE", "STM32F303RE"],
        "config": {
            "clock_source": {
                "help": "Mask value : USE_PLL_HSE_EXTC | USE_PLL_HSE_XTAL (need HW patch) | USE_PLL_HSI",
                "value": "USE_PLL_HSE_EXTC|USE_PLL_HSI",
                "macro_name": "CLOCK_SOURCE"
            }
        },
        "detect_code": ["0745"],
        "device_has_add": ["ANALOGOUT", "CAN", "CRC", "SERIAL_ASYNCH", "SERIAL_FC", "FLASH"],
        "release_versions": ["2", "5"],
        "bootloader_supported": true,
        "device_name": "STM32F303RE"
    },
    "NUCLEO_F303ZE": {
        "inherits": ["FAMILY_STM32"],
        "supported_form_factors": ["ARDUINO", "MORPHO"],
        "core": "Cortex-M4F",
        "extra_labels_add": ["STM32F3", "STM32F303xE", "STM32F303ZE"],
        "config": {
            "clock_source": {
                "help": "Mask value : USE_PLL_HSE_EXTC | USE_PLL_HSE_XTAL (need HW patch) | USE_PLL_HSI",
                "value": "USE_PLL_HSE_EXTC|USE_PLL_HSI",
                "macro_name": "CLOCK_SOURCE"
            }
        },
        "detect_code": ["0747"],
        "device_has_add": ["ANALOGOUT", "CAN", "CRC", "FLASH"],
        "release_versions": ["2", "5"],
        "device_name": "STM32F303ZE"
    },
    "NUCLEO_F334R8": {
        "inherits": ["FAMILY_STM32"],
        "supported_form_factors": ["ARDUINO", "MORPHO"],
        "core": "Cortex-M4F",
        "extra_labels_add": ["STM32F3", "STM32F334x8", "STM32F334R8"],
        "config": {
            "clock_source": {
                "help": "Mask value : USE_PLL_HSE_EXTC | USE_PLL_HSE_XTAL (need HW patch) | USE_PLL_HSI",
                "value": "USE_PLL_HSE_EXTC|USE_PLL_HSI",
                "macro_name": "CLOCK_SOURCE"
            }
        },
        "detect_code": ["0735"],
        "device_has_add": ["ANALOGOUT", "CAN", "CRC", "SERIAL_ASYNCH", "SERIAL_FC"],
        "default_lib": "small",
        "release_versions": ["2"],
        "device_name": "STM32F334R8"
    },
    "NUCLEO_F401RE": {
        "inherits": ["FAMILY_STM32"],
        "supported_form_factors": ["ARDUINO", "MORPHO"],
        "core": "Cortex-M4F",
        "extra_labels_add": ["STM32F4", "STM32F401xE", "STM32F401RE"],
        "config": {
            "clock_source": {
                "help": "Mask value : USE_PLL_HSE_EXTC | USE_PLL_HSE_XTAL (need HW patch) | USE_PLL_HSI",
                "value": "USE_PLL_HSE_EXTC|USE_PLL_HSI",
                "macro_name": "CLOCK_SOURCE"
            }
        },
        "detect_code": ["0720"],
        "macros_add": ["USB_STM_HAL", "USBHOST_OTHER"],
        "device_has_add": ["SERIAL_ASYNCH", "SERIAL_FC", "FLASH"],
        "release_versions": ["2", "5"],
        "device_name": "STM32F401RE"
    },
    "STEVAL_3DP001V1": {
        "inherits": ["FAMILY_STM32"],
        "core": "Cortex-M4F",
        "extra_labels_add": ["STM32F4", "STM32F401xE", "STM32F401VE"],
        "config": {
            "clock_source": {
                "help": "Mask value : USE_PLL_HSE_EXTC | USE_PLL_HSE_XTAL | USE_PLL_HSI",
                "value": "USE_PLL_HSE_XTAL|USE_PLL_HSI",
                "macro_name": "CLOCK_SOURCE"
            }
        },
        "macros_add": ["USB_STM_HAL", "USBHOST_OTHER", "HSE_VALUE=25000000"],
        "device_has_add": ["SERIAL_ASYNCH", "SERIAL_FC", "FLASH"],
        "overrides": {"lse_available": 0},
        "release_versions": ["2", "5"],
        "device_name": "STM32F401VE"
    },
    "NUCLEO_F410RB": {
        "inherits": ["FAMILY_STM32"],
        "supported_form_factors": ["ARDUINO", "MORPHO"],
        "core": "Cortex-M4F",
        "extra_labels_add": ["STM32F4", "STM32F410RB","STM32F410xB", "STM32F410Rx"],
        "config": {
            "clock_source": {
                "help": "Mask value : USE_PLL_HSE_EXTC | USE_PLL_HSE_XTAL (need HW patch) | USE_PLL_HSI",
                "value": "USE_PLL_HSE_EXTC|USE_PLL_HSI",
                "macro_name": "CLOCK_SOURCE"
            },
            "lpticker_lptim": {
                "help": "This target supports LPTIM. Set value 1 to use LPTIM for LPTICKER, or 0 to use RTC wakeup timer",
                "value": 1
            }
        },
        "detect_code": ["0744"],
        "device_has_add": ["ANALOGOUT", "SERIAL_ASYNCH", "SERIAL_FC", "TRNG", "FLASH"],
        "release_versions": ["2", "5"],
        "device_name": "STM32F410RB"
    },
    "NUCLEO_F411RE": {
        "inherits": ["FAMILY_STM32"],
        "supported_form_factors": ["ARDUINO", "MORPHO"],
        "core": "Cortex-M4F",
        "extra_labels_add": ["STM32F4", "STM32F411xE", "STM32F411RE"],
        "detect_code": ["0740"],
        "config": {
            "clock_source": {
                "help": "Mask value : USE_PLL_HSE_EXTC | USE_PLL_HSE_XTAL (need HW patch) | USE_PLL_HSI",
                "value": "USE_PLL_HSE_EXTC|USE_PLL_HSI",
                "macro_name": "CLOCK_SOURCE"
            },
            "clock_source_usb": {
                "help": "As 48 Mhz clock is configured for USB, SYSCLK has to be reduced from 100 to 96 MHz (set 0 for the max SYSCLK value)",
                "value": "0",
                "macro_name": "CLOCK_SOURCE_USB"
            }
        },
        "macros_add": ["USB_STM_HAL", "USBHOST_OTHER"],
        "device_has_add": ["SERIAL_ASYNCH", "SERIAL_FC", "FLASH"],
        "release_versions": ["2", "5"],
        "device_name": "STM32F411RE",
        "bootloader_supported": true
    },
    "NUCLEO_F412ZG": {
        "inherits": ["FAMILY_STM32"],
        "supported_form_factors": ["ARDUINO", "MORPHO"],
        "core": "Cortex-M4F",
        "extra_labels_add": ["STM32F4", "STM32F412xG", "STM32F412ZG"],
        "config": {
            "clock_source": {
                "help": "Mask value : USE_PLL_HSE_EXTC | USE_PLL_HSE_XTAL (need HW patch) | USE_PLL_HSI",
                "value": "USE_PLL_HSE_EXTC|USE_PLL_HSI",
                "macro_name": "CLOCK_SOURCE"
            }
        },
        "detect_code": ["0826"],
        "macros_add": ["USB_STM_HAL", "USBHOST_OTHER"],
        "device_has_add": ["CAN", "SERIAL_ASYNCH", "SERIAL_FC", "TRNG", "FLASH"],
        "release_versions": ["2", "5"],
        "device_name": "STM32F412ZG",
        "bootloader_supported": true
    },
    "MTB_MXCHIP_EMW3166": {
        "inherits": ["FAMILY_STM32"],
        "core": "Cortex-M4F",
        "extra_labels_add": ["STM32F4", "STM32F412xG", "STM32F412ZG", "WICED", "CYW43362"],
        "macros_add": ["USB_STM_HAL", "USBHOST_OTHER"],
        "device_has_add": ["CAN", "SERIAL_ASYNCH", "SERIAL_FC", "TRNG", "FLASH"],
        "release_versions": ["5"],
        "device_name": "STM32F412ZG",
        "bootloader_supported": true,
        "config": {
            "clock_source": {
                "help": "Mask value : USE_PLL_HSE_EXTC | USE_PLL_HSE_XTAL (need HW patch) | USE_PLL_HSI",
                "value": "USE_PLL_HSI",
                "macro_name": "CLOCK_SOURCE"
            }
        },
        "overrides": {
            "network-default-interface-type": "WIFI"
        }
    },
    "USI_WM_BN_BM_22": {
        "inherits": ["FAMILY_STM32"],
        "components": ["SPIF"],
        "core": "Cortex-M4F",
        "extra_labels_add": ["STM32F4", "STM32F412xG", "STM32F412ZG", "WICED", "CYW4343X", "CORDIO"],
        "features": ["BLE", "STORAGE"],
        "macros_add": ["USB_STM_HAL", "USBHOST_OTHER"],
        "device_has_add": ["SERIAL_ASYNCH", "SERIAL_FC", "TRNG", "FLASH"],
        "release_versions": ["5"],
        "device_name": "STM32F412ZG",
        "bootloader_supported": true,
        "public": false,
        "config": {
            "clock_source": {
                "help": "Mask value : USE_PLL_HSE_EXTC | USE_PLL_HSE_XTAL (need HW patch) | USE_PLL_HSI",
                "value": "USE_PLL_HSI",
                "macro_name": "CLOCK_SOURCE"
            }
        },
        "overrides": {
            "network-default-interface-type": "WIFI"
        }
    },
    "MTB_USI_WM_BN_BM_22": {
        "overrides": {
            "lse_available": 0
        },
        "inherits": ["USI_WM_BN_BM_22"]
    },
    "MTB_ADV_WISE_1530": {
        "inherits": ["USI_WM_BN_BM_22"],
        "config": {
            "led1": "PA_4",
            "led2": "PC_12",
            "led3": "NC"
            },
        "overrides": {
            "stdio_uart_tx": "PB_10",
            "stdio_uart_rx": "PC_11"
        }
    },
    "DISCO_F413ZH": {
        "inherits": ["FAMILY_STM32"],
        "supported_form_factors": ["ARDUINO"],
        "core": "Cortex-M4F",
        "extra_labels_add": ["STM32F4", "STM32F413xx", "STM32F413ZH", "STM32F413xH"],
        "config": {
            "clock_source": {
                "help": "Mask value : USE_PLL_HSE_EXTC | USE_PLL_HSE_XTAL (need HW patch) | USE_PLL_HSI",
                "value": "USE_PLL_HSE_EXTC|USE_PLL_HSI",
                "macro_name": "CLOCK_SOURCE"
            },
            "lpticker_lptim": {
                "help": "This target supports LPTIM. Set value 1 to use LPTIM for LPTICKER, or 0 to use RTC wakeup timer",
                "value": 1
            }
        },
        "detect_code": ["0743"],
        "macros_add": ["USB_STM_HAL", "USBHOST_OTHER"],
        "device_has_add": ["ANALOGOUT", "CAN", "SERIAL_ASYNCH", "SERIAL_FC", "TRNG", "FLASH", "QSPI"],
        "bootloader_supported": true,
        "release_versions": ["2", "5"],
        "device_name": "STM32F413ZH"
    },
    "NUCLEO_F413ZH": {
        "inherits": ["FAMILY_STM32"],
        "supported_form_factors": ["ARDUINO"],
        "core": "Cortex-M4F",
        "extra_labels_add": ["STM32F4", "STM32F413xx", "STM32F413ZH", "STM32F413xH"],
        "config": {
            "clock_source": {
                "help": "Mask value : USE_PLL_HSE_EXTC | USE_PLL_HSE_XTAL (need HW patch) | USE_PLL_HSI",
                "value": "USE_PLL_HSE_EXTC|USE_PLL_HSI",
                "macro_name": "CLOCK_SOURCE"
            },
            "lpticker_lptim": {
                "help": "This target supports LPTIM. Set value 1 to use LPTIM for LPTICKER, or 0 to use RTC wakeup timer",
                "value": 1
            }
        },
        "detect_code": ["0743"],
        "macros_add": ["USB_STM_HAL", "USBHOST_OTHER"],
        "device_has_add": ["ANALOGOUT", "CAN", "SERIAL_ASYNCH", "SERIAL_FC", "TRNG", "FLASH"],
        "bootloader_supported": true,
        "release_versions": ["2", "5"],
        "device_name": "STM32F413ZH"
    },
    "ELMO_F411RE": {
        "inherits": ["FAMILY_STM32"],
        "supported_form_factors": ["ARDUINO"],
        "core": "Cortex-M4F",
        "default_toolchain": "uARM",
        "extra_labels_add": ["STM32F4", "STM32F411xE", "STM32F411RE"],
        "supported_toolchains": ["ARM", "uARM", "GCC_ARM"],
        "detect_code": ["----"],
        "device_has_add": [],
        "default_lib": "small",
        "release_versions": ["2"],
        "device_name": "STM32F411RE"
    },
    "NUCLEO_F429ZI": {
        "inherits": ["FAMILY_STM32"],
        "supported_form_factors": ["ARDUINO"],
        "core": "Cortex-M4F",
        "config": {
            "d11_configuration": {
                "help": "Value: PA_7 for the default board configuration, PB_5 in case of solder bridge update (SB121 off/ SB122 on)",
                "value": "PA_7",
                "macro_name": "STM32_D11_SPI_ETHERNET_PIN"
            },
            "clock_source": {
                "help": "Mask value : USE_PLL_HSE_EXTC | USE_PLL_HSE_XTAL (need HW patch) | USE_PLL_HSI",
                "value": "USE_PLL_HSE_EXTC|USE_PLL_HSI",
                "macro_name": "CLOCK_SOURCE"
            },
            "clock_source_usb": {
                "help": "As 48 Mhz clock is configured for USB, SYSCLK has to be reduced from 180 to 168 MHz (set 0 for the max SYSCLK value)",
                "value": "1",
                "macro_name": "CLOCK_SOURCE_USB"
            }
        },
        "extra_labels_add": ["STM32F4", "STM32F429", "STM32F429ZI", "STM32F429xx", "STM32F429xI", "STM_EMAC"],
        "macros_add": ["USB_STM_HAL", "USBHOST_OTHER"],
        "device_has_add": ["ANALOGOUT", "CAN", "EMAC", "SERIAL_ASYNCH", "SERIAL_FC", "TRNG", "FLASH"],
        "detect_code": ["0796"],
        "release_versions": ["2", "5"],
        "device_name": "STM32F429ZI",
        "bootloader_supported": true,
        "overrides": {
            "network-default-interface-type": "ETHERNET"
        }
    },
    "NUCLEO_F439ZI": {
        "inherits": ["FAMILY_STM32"],
        "supported_form_factors": ["ARDUINO"],
        "core": "Cortex-M4F",
        "config": {
            "d11_configuration": {
                "help": "Value: PA_7 for the default board configuration, PB_5 in case of solder bridge update (SB121 off/ SB122 on)",
                "value": "PA_7",
                "macro_name": "STM32_D11_SPI_ETHERNET_PIN"
            },
            "clock_source": {
                "help": "Mask value : USE_PLL_HSE_EXTC | USE_PLL_HSE_XTAL (need HW patch) | USE_PLL_HSI",
                "value": "USE_PLL_HSE_EXTC|USE_PLL_HSI",
                "macro_name": "CLOCK_SOURCE"
            },
            "clock_source_usb": {
                "help": "As 48 Mhz clock is configured for USB, SYSCLK has to be reduced from 180 to 168 MHz (set 0 for the max SYSCLK value)",
                "value": "1",
                "macro_name": "CLOCK_SOURCE_USB"
            }
        },
        "extra_labels_add": ["STM32F4", "STM32F439", "STM32F439ZI", "STM32F439xx", "STM32F439xI", "STM_EMAC"],
        "macros_add": ["MBEDTLS_CONFIG_HW_SUPPORT", "USB_STM_HAL", "USBHOST_OTHER"],
        "device_has_add": ["ANALOGOUT", "CAN", "EMAC", "SERIAL_FC", "TRNG", "FLASH"],
        "detect_code": ["0797"],
        "release_versions": ["2", "5"],
        "device_name" : "STM32F439ZI",
        "bootloader_supported": true,
        "overrides": {
            "network-default-interface-type": "ETHERNET"
        }
    },
    "NUCLEO_F446RE": {
        "inherits": ["FAMILY_STM32"],
        "supported_form_factors": ["ARDUINO", "MORPHO"],
        "core": "Cortex-M4F",
        "extra_labels_add": ["STM32F4", "STM32F446xE", "STM32F446RE"],
        "config": {
            "clock_source": {
                "help": "Mask value : USE_PLL_HSE_EXTC | USE_PLL_HSE_XTAL (need HW patch) | USE_PLL_HSI",
                "value": "USE_PLL_HSE_EXTC|USE_PLL_HSI",
                "macro_name": "CLOCK_SOURCE"
            }
        },
        "detect_code": ["0777"],
        "macros_add": ["USB_STM_HAL", "USBHOST_OTHER"],
        "device_has_add": ["ANALOGOUT", "CAN", "SERIAL_ASYNCH", "SERIAL_FC", "FLASH"],
        "release_versions": ["2", "5"],
        "device_name": "STM32F446RE",
        "bootloader_supported": true
    },
    "NUCLEO_F446ZE": {
        "inherits": ["FAMILY_STM32"],
        "supported_form_factors": ["ARDUINO", "MORPHO"],
        "core": "Cortex-M4F",
        "extra_labels_add": ["STM32F4", "STM32F446xE", "STM32F446ZE"],
        "config": {
            "clock_source": {
                "help": "Mask value : USE_PLL_HSE_EXTC | USE_PLL_HSE_XTAL (need HW patch) | USE_PLL_HSI",
                "value": "USE_PLL_HSE_EXTC|USE_PLL_HSI",
                "macro_name": "CLOCK_SOURCE"
            }
        },
        "detect_code": ["0778"],
        "macros_add": ["USB_STM_HAL", "USBHOST_OTHER"],
        "device_has_add": ["ANALOGOUT", "CAN", "SERIAL_ASYNCH", "SERIAL_FC", "FLASH"],
        "release_versions": ["2", "5"],
        "device_name": "STM32F446ZE"
    },
    "B96B_F446VE": {
        "inherits": ["FAMILY_STM32"],
        "supported_form_factors": ["ARDUINO", "MORPHO"],
        "core": "Cortex-M4F",
        "extra_labels_add": ["STM32F4", "STM32F446xE", "STM32F446VE"],
        "detect_code": ["0840"],
        "device_has_add": ["ANALOGOUT", "CAN", "SERIAL_ASYNCH", "SERIAL_FC", "FLASH"],
        "release_versions": ["2", "5"],
        "device_name":"STM32F446VE"
    },
    "NUCLEO_F746ZG": {
        "inherits": ["FAMILY_STM32"],
        "core": "Cortex-M7F",
        "extra_labels_add": ["STM32F7", "STM32F746", "STM32F746xG", "STM32F746ZG", "STM_EMAC"],
        "config": {
            "d11_configuration": {
                "help": "Value: PA_7 for the default board configuration, PB_5 in case of solder bridge update (SB121 off/ SB122 on)",
                "value": "PA_7",
                "macro_name": "STM32_D11_SPI_ETHERNET_PIN"
            },
            "clock_source": {
                "help": "Mask value : USE_PLL_HSE_EXTC | USE_PLL_HSE_XTAL (need HW patch) | USE_PLL_HSI",
                "value": "USE_PLL_HSE_EXTC|USE_PLL_HSI",
                "macro_name": "CLOCK_SOURCE"
            },
            "lpticker_lptim": {
                "help": "This target supports LPTIM. Set value 1 to use LPTIM for LPTICKER, or 0 to use RTC wakeup timer",
                "value": 1
            }
        },
        "macros_add": ["USBHOST_OTHER"],
        "supported_form_factors": ["ARDUINO"],
        "detect_code": ["0816"],
        "device_has_add": ["ANALOGOUT", "CAN", "CRC", "EMAC", "SERIAL_ASYNCH", "TRNG", "FLASH"],
        "release_versions": ["2", "5"],
        "device_name": "STM32F746ZG",
        "bootloader_supported": true,
        "overrides": {
            "network-default-interface-type": "ETHERNET"
        }
    },
    "NUCLEO_F756ZG": {
        "inherits": ["FAMILY_STM32"],
        "core": "Cortex-M7F",
        "extra_labels_add": ["STM32F7", "STM32F756", "STM32F756xG", "STM32F756ZG", "STM_EMAC"],
        "config": {
            "d11_configuration": {
                "help": "Value: PA_7 for the default board configuration, PB_5 in case of solder bridge update (SB121 off/ SB122 on)",
                "value": "PA_7",
                "macro_name": "STM32_D11_SPI_ETHERNET_PIN"
            },
            "clock_source": {
                "help": "Mask value : USE_PLL_HSE_EXTC | USE_PLL_HSE_XTAL (need HW patch) | USE_PLL_HSI",
                "value": "USE_PLL_HSE_EXTC|USE_PLL_HSI",
                "macro_name": "CLOCK_SOURCE"
            },
            "lpticker_lptim": {
                "help": "This target supports LPTIM. Set value 1 to use LPTIM for LPTICKER, or 0 to use RTC wakeup timer",
                "value": 1
            }
        },
        "macros_add": ["TRANSACTION_QUEUE_SIZE_SPI=2", "USBHOST_OTHER", "MBEDTLS_CONFIG_HW_SUPPORT"],
        "supported_form_factors": ["ARDUINO"],
        "detect_code": ["0819"],
        "device_has_add": ["ANALOGOUT", "CAN", "CRC", "EMAC", "SERIAL_ASYNCH", "TRNG", "FLASH"],
        "release_versions": ["2", "5"],
        "device_name": "STM32F756ZG",
        "overrides": {
            "network-default-interface-type": "ETHERNET"
        }
    },
    "NUCLEO_F767ZI": {
        "inherits": ["FAMILY_STM32"],
        "core": "Cortex-M7FD",
        "extra_labels_add": ["STM32F7", "STM32F767", "STM32F767xI", "STM32F767ZI", "STM_EMAC"],
        "config": {
            "flash_dual_bank": {
                "help": "Default board configuration is Single Bank Flash. If you enable Dual Bank with ST Link Utility, set value to 1",
                "value": "0"
            },
            "d11_configuration": {
                "help": "Value: PA_7 for the default board configuration, PB_5 in case of solder bridge update (SB121 off/ SB122 on)",
                "value": "PA_7",
                "macro_name": "STM32_D11_SPI_ETHERNET_PIN"
            },
            "clock_source": {
                "help": "Mask value : USE_PLL_HSE_EXTC | USE_PLL_HSE_XTAL (need HW patch) | USE_PLL_HSI",
                "value": "USE_PLL_HSE_EXTC|USE_PLL_HSI",
                "macro_name": "CLOCK_SOURCE"
            },
            "lpticker_lptim": {
                "help": "This target supports LPTIM. Set value 1 to use LPTIM for LPTICKER, or 0 to use RTC wakeup timer",
                "value": 1
            }
        },
        "supported_form_factors": ["ARDUINO"],
        "macros_add": ["USBHOST_OTHER"],
        "detect_code": ["0818"],
        "device_has_add": ["ANALOGOUT", "CAN", "CRC", "EMAC", "SERIAL_ASYNCH", "TRNG", "FLASH"],
        "release_versions": ["2", "5"],
        "device_name": "STM32F767ZI",
        "bootloader_supported": true,
        "overrides": {
            "network-default-interface-type": "ETHERNET"
        }
    },
    "NUCLEO_L011K4": {
        "inherits": ["FAMILY_STM32"],
        "core": "Cortex-M0+",
        "extra_labels_add": ["STM32L0", "STM32L011K4"],
        "supported_toolchains": ["uARM"],
        "default_toolchain": "uARM",
        "supported_form_factors": ["ARDUINO"],
        "config": {
            "clock_source": {
                "help": "Mask value : USE_PLL_HSE_EXTC | USE_PLL_HSE_XTAL (need HW patch) | USE_PLL_HSI",
                "value": "USE_PLL_HSE_EXTC|USE_PLL_HSI",
                "macro_name": "CLOCK_SOURCE"
            },
            "lpticker_lptim": {
                "help": "This target supports LPTIM. Set value 1 to use LPTIM for LPTICKER, or 0 to use RTC wakeup timer",
                "value": 1
            }
        },
        "overrides": {"lpticker_delay_ticks": 4},
        "detect_code": ["0780"],
        "device_has_add": ["CRC", "SERIAL_FC", "FLASH"],
        "default_lib": "small",
        "release_versions": ["2"],
        "device_name": "STM32L011K4"
    },
    "NUCLEO_L031K6": {
        "inherits": ["FAMILY_STM32"],
        "core": "Cortex-M0+",
        "extra_labels_add": ["STM32L0", "STM32L031K6"],
        "default_toolchain": "uARM",
        "supported_form_factors": ["ARDUINO"],
        "config": {
            "clock_source": {
                "help": "Mask value : USE_PLL_HSE_EXTC (need HW patch) | USE_PLL_HSE_XTAL (need HW patch) | USE_PLL_HSI",
                "value": "USE_PLL_HSI",
                "macro_name": "CLOCK_SOURCE"
            },
            "lpticker_lptim": {
                "help": "This target supports LPTIM. Set value 1 to use LPTIM for LPTICKER, or 0 to use RTC wakeup timer",
                "value": 1
            }
        },
        "overrides": {"lpticker_delay_ticks": 4},
        "detect_code": ["0790"],
        "device_has_add": ["CRC", "SERIAL_FC", "FLASH"],
        "default_lib": "small",
        "release_versions": ["2"],
        "device_name": "STM32L031K6"
    },
    "NUCLEO_L053R8": {
        "inherits": ["FAMILY_STM32"],
        "supported_form_factors": ["ARDUINO", "MORPHO"],
        "core": "Cortex-M0+",
        "extra_labels_add": ["STM32L0", "STM32L053x8", "STM32L053R8"],
        "config": {
            "clock_source": {
                "help": "Mask value : USE_PLL_HSE_EXTC | USE_PLL_HSE_XTAL (need HW patch) | USE_PLL_HSI",
                "value": "USE_PLL_HSE_EXTC|USE_PLL_HSI",
                "macro_name": "CLOCK_SOURCE"
            },
            "lpticker_lptim": {
                "help": "This target supports LPTIM. Set value 1 to use LPTIM for LPTICKER, or 0 to use RTC wakeup timer",
                "value": 1
            }
        },
        "overrides": {"lpticker_delay_ticks": 4},
        "detect_code": ["0715"],
        "device_has_add": ["ANALOGOUT", "CRC", "SERIAL_FC", "SERIAL_ASYNCH", "FLASH"],
        "default_lib": "small",
        "release_versions": ["2"],
        "device_name": "STM32L053R8"
    },
    "NUCLEO_L073RZ": {
        "inherits": ["FAMILY_STM32"],
        "supported_form_factors": ["ARDUINO", "MORPHO"],
        "core": "Cortex-M0+",
        "extra_labels_add": ["STM32L0", "STM32L073RZ", "STM32L073xx"],
        "config": {
            "clock_source": {
                "help": "Mask value : USE_PLL_HSE_EXTC | USE_PLL_HSE_XTAL (need HW patch) | USE_PLL_HSI",
                "value": "USE_PLL_HSE_EXTC|USE_PLL_HSI",
                "macro_name": "CLOCK_SOURCE"
            },
            "lpticker_lptim": {
                "help": "This target supports LPTIM. Set value 1 to use LPTIM for LPTICKER, or 0 to use RTC wakeup timer",
                "value": 1
            }
        },
        "overrides": {"lpticker_delay_ticks": 4},
        "detect_code": ["0760"],
        "device_has_add": ["ANALOGOUT", "CRC", "SERIAL_FC", "SERIAL_ASYNCH", "TRNG", "FLASH"],
        "release_versions": ["2", "5"],
        "device_name": "STM32L073RZ"
    },
    "NUCLEO_L152RE": {
        "inherits": ["FAMILY_STM32"],
        "supported_form_factors": ["ARDUINO", "MORPHO"],
        "core": "Cortex-M3",
        "extra_labels_add": ["STM32L1", "STM32L152RE"],
        "config": {
            "clock_source": {
                "help": "Mask value : USE_PLL_HSE_EXTC | USE_PLL_HSE_XTAL (need HW patch) | USE_PLL_HSI",
                "value": "USE_PLL_HSE_EXTC|USE_PLL_HSI",
                "macro_name": "CLOCK_SOURCE"
            }
        },
        "detect_code": ["0710"],
        "device_has_add": ["ANALOGOUT", "SERIAL_ASYNCH", "SERIAL_FC", "FLASH"],
        "release_versions": ["2", "5"],
        "device_name": "STM32L152RE"
    },
    "NUCLEO_L432KC": {
        "inherits": ["FAMILY_STM32"],
        "supported_form_factors": ["ARDUINO"],
        "core": "Cortex-M4F",
        "extra_labels_add": ["STM32L4", "STM32L432xC", "STM32L432KC"],
        "config": {
            "clock_source": {
                "help": "Mask value : USE_PLL_HSE_EXTC (need HW patch) | USE_PLL_HSE_XTAL (need HW patch) | USE_PLL_HSI | USE_PLL_MSI",
                "value": "USE_PLL_MSI",
                "macro_name": "CLOCK_SOURCE"
            },
            "lpticker_lptim": {
                "help": "This target supports LPTIM. Set value 1 to use LPTIM for LPTICKER, or 0 to use RTC wakeup timer",
                "value": 1
            }
        },
        "detect_code": ["0770"],
        "device_has_add": ["ANALOGOUT", "CRC", "SERIAL_FC", "SERIAL_ASYNCH", "CAN", "TRNG", "FLASH"],
        "release_versions": ["2", "5"],
        "device_name": "STM32L432KC",
        "bootloader_supported": true
    },
    "NUCLEO_L433RC_P": {
        "inherits": ["FAMILY_STM32"],
        "supported_form_factors": ["ARDUINO", "MORPHO"],
        "core": "Cortex-M4F",
        "extra_labels_add": ["STM32L4", "STM32L433xC", "STM32L433RC"],
        "config": {
            "clock_source": {
                "help": "Mask value : USE_PLL_HSE_EXTC (need HW patch) | USE_PLL_HSE_XTAL (need HW patch) | USE_PLL_HSI | USE_PLL_MSI",
                "value": "USE_PLL_MSI",
                "macro_name": "CLOCK_SOURCE"
            },
            "lpticker_lptim": {
                "help": "This target supports LPTIM. Set value 1 to use LPTIM for LPTICKER, or 0 to use RTC wakeup timer",
                "value": 1
            }
        },
        "detect_code": ["0779"],
        "device_has_add": ["ANALOGOUT", "CRC", "SERIAL_FC", "SERIAL_ASYNCH", "CAN", "TRNG", "FLASH"],
        "release_versions": ["2", "5"],
        "device_name": "STM32L433RC",
        "bootloader_supported": true
    },
    "MTB_ADV_WISE_1510": {
        "inherits": ["FAMILY_STM32"],
        "core": "Cortex-M4F",
        "extra_labels_add": ["STM32L4", "STM32L443xC", "STM32L443RC"],
        "config": {
            "clock_source": {
                "help": "Mask value : USE_PLL_HSI | USE_PLL_MSI",
                "value": "USE_PLL_HSI",
                "macro_name": "CLOCK_SOURCE"
            }
        },
        "overrides": {"lse_available": 0},
        "release_versions": ["5"],
        "device_has_add": ["ANALOGOUT", "CRC", "SERIAL_FC", "SERIAL_ASYNCH", "CAN", "TRNG", "FLASH"],
        "device_has_remove": ["LPTICKER"],
        "macros_add": ["MBEDTLS_CONFIG_HW_SUPPORT"],
        "device_name" : "STM32L443RC",
        "detect_code": ["0458"],
        "bootloader_supported": true
    },
    "NUCLEO_L476RG": {
        "inherits": ["FAMILY_STM32"],
        "supported_form_factors": ["ARDUINO", "MORPHO"],
        "core": "Cortex-M4F",
        "extra_labels_add": ["STM32L4", "STM32L476RG", "STM32L476xG"],
        "config": {
            "clock_source": {
                "help": "Mask value : USE_PLL_HSE_EXTC (need HW patch) | USE_PLL_HSE_XTAL (need HW patch) | USE_PLL_HSI | USE_PLL_MSI",
                "value": "USE_PLL_MSI",
                "macro_name": "CLOCK_SOURCE"
            },
            "lpticker_lptim": {
                "help": "This target supports LPTIM. Set value 1 to use LPTIM for LPTICKER, or 0 to use RTC wakeup timer",
                "value": 1
            }
        },
        "detect_code": ["0765"],
        "macros_add": ["USBHOST_OTHER", "TWO_RAM_REGIONS"],
        "device_has_add": ["ANALOGOUT", "CAN", "CRC", "SERIAL_ASYNCH", "SERIAL_FC", "TRNG", "FLASH"],
        "release_versions": ["2", "5"],
        "device_name": "STM32L476RG",
        "bootloader_supported": true
    },
    "SILICA_SENSOR_NODE": {
        "inherits": ["FAMILY_STM32"],
        "core": "Cortex-M4F",
        "default_toolchain": "GCC_ARM",
        "extra_labels_add": ["STM32L4", "STM32L476xG", "STM32L476JG"],
        "config": {
            "clock_source": {
                "help": "Mask value : USE_PLL_HSE_EXTC (need HW patch) | USE_PLL_HSE_XTAL (need HW patch) | USE_PLL_HSI | USE_PLL_MSI",
                "value": "USE_PLL_MSI",
                "macro_name": "CLOCK_SOURCE"
            }
        },
        "detect_code": ["0766"],
        "macros_add": ["USBHOST_OTHER", "TWO_RAM_REGIONS"],
        "device_has_add": ["ANALOGOUT", "CAN", "CRC", "SERIAL_ASYNCH", "SERIAL_FC", "TRNG", "FLASH"],
        "release_versions": ["5"],
        "device_name": "STM32L476JG"
    },
    "NUCLEO_L486RG": {
        "inherits": ["FAMILY_STM32"],
        "supported_form_factors": ["ARDUINO", "MORPHO"],
        "core": "Cortex-M4F",
        "extra_labels_add": ["STM32L4", "STM32L486RG", "STM32L486xG"],
        "config": {
            "clock_source": {
                "help": "Mask value : USE_PLL_HSE_EXTC (need HW patch) | USE_PLL_HSE_XTAL (need HW patch) | USE_PLL_HSI | USE_PLL_MSI",
                "value": "USE_PLL_MSI",
                "macro_name": "CLOCK_SOURCE"
            },
            "lpticker_lptim": {
                "help": "This target supports LPTIM. Set value 1 to use LPTIM for LPTICKER, or 0 to use RTC wakeup timer",
                "value": 1
            }
        },
        "detect_code": ["0827"],
        "macros_add": ["USBHOST_OTHER", "MBEDTLS_CONFIG_HW_SUPPORT", "TWO_RAM_REGIONS"],
        "device_has_add": ["ANALOGOUT", "CAN", "CRC", "SERIAL_ASYNCH", "SERIAL_FC", "TRNG", "FLASH"],
        "release_versions": ["2", "5"],
        "device_name": "STM32L486RG"
    },
    "MTB_ADV_WISE_1570": {
        "components": ["FLASHIAP"],
        "inherits": ["FAMILY_STM32"],
        "core": "Cortex-M4F",
        "extra_labels_add": ["STM32L4", "STM32L486RG", "STM32L486xG", "WISE_1570"],
        "config": {
            "clock_source": {
                "help": "Mask value : USE_PLL_HSE_EXTC (need HW patch) | USE_PLL_HSE_XTAL (need HW patch) | USE_PLL_HSI | USE_PLL_MSI",
                "value": "USE_PLL_HSE_XTAL",
                "macro_name": "CLOCK_SOURCE"
            }
        },
        "overrides": {"lpuart_clock_source": "USE_LPUART_CLK_HSI"},
        "detect_code": ["0460"],
        "macros_add": ["MBEDTLS_CONFIG_HW_SUPPORT", "WISE_1570", "TWO_RAM_REGIONS"],
        "device_has_add": ["ANALOGOUT", "CRC", "SERIAL_ASYNCH", "SERIAL_FC", "TRNG", "FLASH"],
        "device_has_remove": ["LPTICKER"],
        "release_versions": ["5"],
        "device_name": "STM32L486RG",
        "bootloader_supported": true,
        "OUTPUT_EXT": "hex"
    },
    "ARCH_MAX": {
        "inherits": ["FAMILY_STM32"],
        "supported_form_factors": ["ARDUINO"],
        "core": "Cortex-M4F",
        "supported_toolchains": ["ARM", "uARM", "GCC_ARM"],
        "program_cycle_s": 2,
        "extra_labels_add": ["STM32F4", "STM32F407", "STM32F407xG", "STM32F407VG"],
        "device_has_add": ["ANALOGOUT", "TRNG", "FLASH"],
        "release_versions": ["2"],
        "device_name": "STM32F407VG"
    },
    "WIO_3G": {
        "inherits": ["FAMILY_STM32"],
        "core": "Cortex-M4F",
        "config": {
            "clock_source": {
                "help": "Mask value : USE_PLL_HSE_EXTC | USE_PLL_HSE_XTAL | USE_PLL_HSI",
                "value": "USE_PLL_HSE_XTAL|USE_PLL_HSI",
                "macro_name": "CLOCK_SOURCE"
            },
            "clock_source_usb": {
                "help": "As 48 Mhz clock is configured for USB, SYSCLK has to be reduced from 180 to 168 MHz (set 0 for the max SYSCLK value)",
                "value": "1",
                "macro_name": "CLOCK_SOURCE_USB"
            },
            "modem_is_on_board": {
                "help": "Value: Tells the build system that the modem is on-board as oppose to a plug-in shield/module.",
                "value": 1,
                "macro_name": "MODEM_ON_BOARD"
            },
            "modem_data_connection_type": {
                "help": "Value: Defines how the modem is wired up to the MCU, e.g., data connection can be a UART or USB and so forth.",
                "value": 1,
                "macro_name": "MODEM_ON_BOARD_UART"
            }
        },
        "extra_labels_add": ["STM32F4", "STM32F439", "STM32F439VI", "STM32F439xx", "STM32F439xI"],
        "macros_add": ["MBEDTLS_CONFIG_HW_SUPPORT", "USB_STM_HAL", "USBHOST_OTHER"],
        "device_has_add": ["ANALOGOUT", "CAN", "LOWPOWERTIMER", "SERIAL_FC", "TRNG", "FLASH"],
        "detect_code": ["9014"],
        "release_versions": ["2", "5"],
        "device_name" : "STM32F439VI",
        "bootloader_supported": true
    },
    "DISCO_F051R8": {
        "inherits": ["FAMILY_STM32"],
        "core": "Cortex-M0",
        "extra_labels_add": ["STM32F0", "STM32F051", "STM32F051R8"],
        "supported_toolchains": ["GCC_ARM"],
        "config": {
            "clock_source": {
                "help": "Mask value : USE_PLL_HSE_EXTC | USE_PLL_HSE_XTAL (need HW patch) | USE_PLL_HSI",
                "value": "USE_PLL_HSE_EXTC|USE_PLL_HSI",
                "macro_name": "CLOCK_SOURCE"
            }
        },
        "macros_add": ["CMSIS_VECTAB_VIRTUAL", "CMSIS_VECTAB_VIRTUAL_HEADER_FILE=\"cmsis_nvic.h\""],
        "device_has_add": ["CRC", "SERIAL_FC"],
        "device_has_remove": ["LPTICKER"],
        "device_name": "STM32F051R8"
    },
    "DISCO_F100RB": {
        "inherits": ["FAMILY_STM32"],
        "core": "Cortex-M3",
        "extra_labels_add": ["STM32F1", "STM32F100RB"],
        "supported_toolchains": ["GCC_ARM"],
        "device_has_add": [],
        "device_has_remove": ["LPTICKER"],
        "device_name": "STM32F100RB"
    },
    "DISCO_F303VC": {
        "inherits": ["FAMILY_STM32"],
        "core": "Cortex-M4F",
        "extra_labels_add": ["STM32F3", "STM32F303", "STM32F303xC", "STM32F303VC"],
        "overrides": {"lse_available": 0},
        "config": {
            "clock_source": {
                "help": "Mask value : USE_PLL_HSE_EXTC | USE_PLL_HSI",
                "value": "USE_PLL_HSE_EXTC|USE_PLL_HSI",
                "macro_name": "CLOCK_SOURCE"
            }
        },
        "supported_toolchains": ["ARM", "uARM", "GCC_ARM", "IAR"],
        "release_versions": ["2", "5"],
        "device_has_add": ["ANALOGOUT", "CAN", "CRC", "SERIAL_FC"],
        "device_name": "STM32F303VC"
    },
    "DISCO_F334C8": {
        "inherits": ["FAMILY_STM32"],
        "core": "Cortex-M4F",
        "extra_labels_add": ["STM32F3", "STM32F334x8","STM32F334C8"],
        "config": {
            "clock_source": {
                "help": "Mask value : USE_PLL_HSE_EXTC | USE_PLL_HSE_XTAL (need HW patch) | USE_PLL_HSI",
                "value": "USE_PLL_HSE_EXTC|USE_PLL_HSI",
                "macro_name": "CLOCK_SOURCE"
            }
        },
        "overrides": {"lse_available": 0},
        "detect_code": ["0810"],
        "device_has_add": ["ANALOGOUT", "CRC", "SERIAL_ASYNCH", "SERIAL_FC"],
        "default_lib": "small",
        "release_versions": ["2"],
        "device_name": "STM32F334C8"
    },
    "DISCO_F407VG": {
        "inherits": ["FAMILY_STM32"],
        "core": "Cortex-M4F",
        "extra_labels_add": ["STM32F4", "STM32F407", "STM32F407xG", "STM32F407VG"],
        "supported_toolchains": ["ARM", "uARM", "GCC_ARM", "IAR"],
        "config": {
            "clock_source": {
                "help": "Mask value : USE_PLL_HSE_EXTC (need HW patch) | USE_PLL_HSE_XTAL | USE_PLL_HSI",
                "value": "USE_PLL_HSE_XTAL|USE_PLL_HSI",
                "macro_name": "CLOCK_SOURCE"
            }
        },
        "macros_add": ["USB_STM_HAL"],
        "overrides": {"lse_available": 0},
        "device_has_add": ["ANALOGOUT", "TRNG", "FLASH"],
        "release_versions": ["2", "5"],
        "device_name": "STM32F407VG"
    },
    "DISCO_F429ZI": {
        "inherits": ["FAMILY_STM32"],
        "core": "Cortex-M4F",
        "extra_labels_add": ["STM32F4", "STM32F429", "STM32F429ZI", "STM32F429xI", "STM32F429xx"],
        "config": {
            "clock_source": {
                "help": "Mask value : USE_PLL_HSE_EXTC (need HW patch) | USE_PLL_HSE_XTAL | USE_PLL_HSI",
                "value": "USE_PLL_HSE_XTAL|USE_PLL_HSI",
                "macro_name": "CLOCK_SOURCE"
            },
            "clock_source_usb": {
                "help": "As 48 Mhz clock is configured for USB, SYSCLK has to be reduced from 180 to 168 MHz (set 0 for the max SYSCLK value)",
                "value": "1",
                "macro_name": "CLOCK_SOURCE_USB"
            }
        },
        "overrides": {"lse_available": 0},
        "macros_add": ["USB_STM_HAL", "USBHOST_OTHER"],
        "device_has_add": ["ANALOGOUT", "CAN", "SERIAL_ASYNCH", "SERIAL_FC", "TRNG", "FLASH"],
        "release_versions": ["2", "5"],
        "device_name": "STM32F429ZI",
        "bootloader_supported": true
    },
    "DISCO_F469NI": {
        "inherits": ["FAMILY_STM32"],
        "supported_form_factors": ["ARDUINO"],
        "core": "Cortex-M4F",
        "extra_labels_add": ["STM32F4", "STM32F469", "STM32F469NI", "STM32F469xI", "STM32F469xx"],
        "config": {
            "clock_source": {
                "help": "Mask value : USE_PLL_HSE_EXTC (need HW patch) | USE_PLL_HSE_XTAL | USE_PLL_HSI",
                "value": "USE_PLL_HSE_XTAL|USE_PLL_HSI",
                "macro_name": "CLOCK_SOURCE"
            }
        },
        "detect_code": ["0788"],
        "macros_add": ["USB_STM_HAL", "USBHOST_OTHER"],
        "device_has_add": ["ANALOGOUT", "CAN", "SERIAL_FC", "TRNG", "FLASH", "QSPI"],
        "release_versions": ["2", "5"],
        "device_name": "STM32F469NI"
    },
    "DISCO_L053C8": {
        "inherits": ["FAMILY_STM32"],
        "core": "Cortex-M0+",
        "extra_labels_add": ["STM32L0", "STM32L053x8", "STM32L053C8"],
        "config": {
            "clock_source": {
                "help": "Mask value : USE_PLL_HSE_EXTC | USE_PLL_HSE_XTAL (need HW patch) | USE_PLL_HSI",
                "value": "USE_PLL_HSE_EXTC|USE_PLL_HSI",
                "macro_name": "CLOCK_SOURCE"
            },
            "lpticker_lptim": {
                "help": "This target supports LPTIM. Set value 1 to use LPTIM for LPTICKER, or 0 to use RTC wakeup timer",
                "value": 1

            }
        },
        "overrides": {
            "lse_available": 0,
            "lpticker_delay_ticks": 4
        },
        "device_has_add": ["ANALOGOUT", "CRC", "SERIAL_FC", "FLASH"],
        "default_lib": "small",
        "release_versions": ["2"],
        "device_name": "STM32L053C8"
    },
    "DISCO_L072CZ_LRWAN1": {
        "inherits": ["FAMILY_STM32"],
        "core": "Cortex-M0+",
        "extra_labels_add": ["STM32L0", "STM32L072CZ", "STM32L072xZ", "STM32L072xx"],
        "supported_form_factors": ["ARDUINO", "MORPHO"],
        "config": {
            "clock_source": {
                "help": "Mask value : USE_PLL_HSE_EXTC (need HW patch) | USE_PLL_HSE_XTAL (need HW patch) | USE_PLL_HSI",
                "value": "USE_PLL_HSI",
                "macro_name": "CLOCK_SOURCE"
            },
            "lpticker_lptim": {
                "help": "This target supports LPTIM. Set value 1 to use LPTIM for LPTICKER, or 0 to use RTC wakeup timer",
                "value": 1
            }
        },
        "overrides": {"lpticker_delay_ticks": 4},
        "detect_code": ["0833"],
        "device_has_add": ["ANALOGOUT", "SERIAL_FC", "SERIAL_ASYNCH", "TRNG", "FLASH"],
        "release_versions": ["2", "5"],
        "device_name": "STM32L072CZ"
    },
    "MTB_MURATA_ABZ": {
        "inherits": ["FAMILY_STM32"],
        "core": "Cortex-M0+",
        "extra_labels_add": ["STM32L0", "STM32L0x2xZ", "STM32L082CZ", "STM32L082xx"],
        "detect_code": ["0456"],
        "device_has_add": ["ANALOGOUT", "SERIAL_FC", "SERIAL_ASYNCH", "TRNG", "FLASH"],
        "device_has_remove": ["LPTICKER"],
        "release_versions": ["5"],
        "device_name": "STM32L082CZ"
    },
    "DISCO_F746NG": {
        "inherits": ["FAMILY_STM32"],
        "core": "Cortex-M7F",
        "extra_labels_add": ["STM32F7", "STM32F746", "STM32F746xG", "STM32F746NG", "STM_EMAC"],
        "supported_form_factors": ["ARDUINO"],
        "config": {
            "clock_source": {
                "help": "Mask value : USE_PLL_HSE_EXTC | USE_PLL_HSE_XTAL | USE_PLL_HSI",
                "value": "USE_PLL_HSE_XTAL|USE_PLL_HSI",
                "macro_name": "CLOCK_SOURCE"
            },
            "usb_speed": {
                "help": "Select the USB speed/connector (0=FullSpeed, 1=HighSpeed)",
                "value": "1"
            },
            "lpticker_lptim": {
                "help": "This target supports LPTIM. Set value 1 to use LPTIM for LPTICKER, or 0 to use RTC wakeup timer",
                "value": 1
            }
        },
        "detect_code": ["0815"],
        "macros_add": ["USB_STM_HAL", "USBHOST_OTHER"],
        "device_has_add": ["ANALOGOUT", "CAN", "EMAC", "SERIAL_ASYNCH", "TRNG", "FLASH", "QSPI"],
        "release_versions": ["2", "5"],
        "device_name": "STM32F746NG",
        "overrides": {
            "network-default-interface-type": "ETHERNET"
        }
    },
    "DISCO_F769NI": {
        "inherits": ["FAMILY_STM32"],
        "core": "Cortex-M7FD",
        "extra_labels_add": ["STM32F7", "STM32F769", "STM32F769xI", "STM32F769NI", "STM_EMAC"],
        "supported_form_factors": ["ARDUINO"],
        "config": {
            "flash_dual_bank": {
                "help": "Default board configuration is Single Bank Flash. If you enable Dual Bank with ST Link Utility, set value to 1",
                "value": "0"
            },
            "clock_source": {
                "help": "Mask value : USE_PLL_HSE_EXTC | USE_PLL_HSE_XTAL | USE_PLL_HSI",
                "value": "USE_PLL_HSE_EXTC|USE_PLL_HSI",
                "macro_name": "CLOCK_SOURCE"
            },
            "lpticker_lptim": {
                "help": "This target supports LPTIM. Set value 1 to use LPTIM for LPTICKER, or 0 to use RTC wakeup timer",
                "value": 1
            }
        },
        "detect_code": ["0817"],
        "macros_add": ["USB_STM_HAL", "USBHOST_OTHER"],
        "device_has_add": ["ANALOGOUT", "CAN", "EMAC", "SERIAL_ASYNCH", "TRNG", "FLASH"],
        "bootloader_supported": true,
        "release_versions": ["2", "5"],
        "device_name": "STM32F769NI",
        "overrides": {
            "network-default-interface-type": "ETHERNET"
        }
    },
    "DISCO_L475VG_IOT01A": {
        "inherits": ["FAMILY_STM32"],
        "core": "Cortex-M4F",
        "extra_labels_add": ["STM32L4", "STM32L475xG", "STM32L475VG"],
        "config": {
            "clock_source": {
                "help": "Mask value : USE_PLL_HSE_EXTC (need HW patch) | USE_PLL_HSE_XTAL (need HW patch) | USE_PLL_HSI | USE_PLL_MSI",
                "value": "USE_PLL_MSI",
                "macro_name": "CLOCK_SOURCE"
            },
            "lpticker_lptim": {
                "help": "This target supports LPTIM. Set value 1 to use LPTIM for LPTICKER, or 0 to use RTC wakeup timer",
                "value": 1
            }
        },
        "supported_form_factors": ["ARDUINO"],
        "detect_code": ["0764"],
        "macros_add": ["USBHOST_OTHER", "TWO_RAM_REGIONS"],
        "device_has_add": ["ANALOGOUT", "CAN", "SERIAL_FC", "TRNG", "FLASH", "QSPI"],
        "release_versions": ["2", "5"],
        "device_name": "STM32L475VG",
        "bootloader_supported": true
    },
    "DISCO_L476VG": {
        "inherits": ["FAMILY_STM32"],
        "core": "Cortex-M4F",
        "extra_labels_add": ["STM32L4", "STM32L476xG", "STM32L476VG"],
        "config": {
            "clock_source": {
                "help": "Mask value : USE_PLL_HSE_EXTC (need HW patch) | USE_PLL_HSE_XTAL (need HW patch) | USE_PLL_HSI | USE_PLL_MSI",
                "value": "USE_PLL_MSI",
                "macro_name": "CLOCK_SOURCE"
            },
            "lpticker_lptim": {
                "help": "This target supports LPTIM. Set value 1 to use LPTIM for LPTICKER, or 0 to use RTC wakeup timer",
                "value": 1
            }
        },
        "detect_code": ["0820"],
        "macros_add": ["USBHOST_OTHER", "TWO_RAM_REGIONS"],
        "device_has_add": ["ANALOGOUT", "CAN", "SERIAL_FC", "TRNG", "FLASH", "QSPI"],
        "release_versions": ["2", "5"],
        "device_name": "STM32L476VG",
        "bootloader_supported": true
    },
    "MTS_MDOT_F405RG": {
        "inherits": ["FAMILY_STM32"],
        "core": "Cortex-M4F",
        "extra_labels_add": ["STM32F4", "STM32F405RG"],
        "is_disk_virtual": true,
        "macros_add": ["HSE_VALUE=26000000"],
        "device_has_add": ["ANALOGOUT"],
        "release_versions": ["2"],
        "device_name": "STM32F405RG"
    },
    "MTS_MDOT_F411RE": {
        "inherits": ["FAMILY_STM32"],
        "core": "Cortex-M4F",
        "extra_labels_add": ["STM32F4", "STM32F411RE"],
        "macros_add": ["HSE_VALUE=26000000", "USE_PLL_HSE_EXTC=0", "VECT_TAB_OFFSET=0x00010000"],
        "post_binary_hook": {
            "function": "MTSCode.combine_bins_mts_dot",
            "toolchains": ["GCC_ARM", "ARM_STD", "ARM_MICRO", "IAR"]
        },
        "device_has_add": [],
        "release_versions": ["2", "5"],
        "device_name": "STM32F411RE"
    },
    "MTS_DRAGONFLY_F411RE": {
        "inherits": ["FAMILY_STM32"],
        "core": "Cortex-M4F",
        "extra_labels_add": ["STM32F4", "STM32F411RE"],
        "config": {
            "modem_is_on_board": {
                "help": "Value: Tells the build system that the modem is on-board as oppose to a plug-in shield/module.",
                "value": 1,
                "macro_name": "MODEM_ON_BOARD"
            },
            "modem_data_connection_type": {
                "help": "Value: Defines how an on-board modem is wired up to the MCU, e.g., data connection can be a UART or USB and so forth.",
                "value": 1,
                "macro_name": "MODEM_ON_BOARD_UART"
            }
        },
        "overrides": {"lse_available": 0},
        "macros_add": ["HSE_VALUE=26000000", "VECT_TAB_OFFSET=0x08010000"],
        "post_binary_hook": {
            "function": "MTSCode.combine_bins_mts_dragonfly",
            "toolchains": ["GCC_ARM", "ARM_STD", "ARM_MICRO", "IAR"]
        },
        "device_has_add": [],
        "release_versions": ["2", "5"],
        "device_name": "STM32F411RE"
    },
    "MTS_DRAGONFLY_L471QG": {
        "inherits": ["FAMILY_STM32"],
        "supported_form_factors": ["ARDUINO"],
        "core": "Cortex-M4F",
        "extra_labels_add": ["STM32L4", "STM32L471QG", "STM32L471xG", "STM32L471xx"],
        "config": {
            "clock_source": {
                "help": "Mask value : USE_PLL_HSI | USE_PLL_MSI",
                "value": "USE_PLL_MSI",
                "macro_name": "CLOCK_SOURCE"
            },
            "modem_is_on_board": {
                "help": "Value: Tells the build system that the modem is on-board as oppose to a plug-in shield/module.",
                "value": 1,
                "macro_name": "MODEM_ON_BOARD"
            },
            "modem_data_connection_type": {
                "help": "Value: Defines how an on-board modem is wired up to the MCU, e.g., data connection can be a UART or USB and so forth.",
                "value": 1,
                "macro_name": "MODEM_ON_BOARD_UART"
            }
        },
        "macros_add": ["TWO_RAM_REGIONS"],
        "detect_code": ["0312"],
        "device_has_add": ["ANALOGOUT", "CAN", "SERIAL_ASYNCH", "SERIAL_FC", "TRNG", "FLASH"],
        "release_versions": ["2", "5"],
        "device_name": "STM32L471QG",
        "bootloader_supported": true
    },
    "MTB_MTS_DRAGONFLY": {
        "inherits": ["FAMILY_STM32"],
        "core": "Cortex-M4F",
        "extra_labels_add": ["STM32F4", "STM32F411RE"],
        "config": {
            "modem_is_on_board": {
                "help": "Value: Tells the build system that the modem is on-board as oppose to a plug-in shield/module.",
                "value": 1,
                "macro_name": "MODEM_ON_BOARD"
            },
            "modem_data_connection_type": {
                "help": "Value: Defines how an on-board modem is wired up to the MCU, e.g., data connection can be a UART or USB and so forth.",
                "value": 1,
                "macro_name": "MODEM_ON_BOARD_UART"
            }
        },
        "overrides": {
                 "lse_available": 0
        },
        "macros_add": ["HSE_VALUE=26000000", "VECT_TAB_OFFSET=0x08010000"],
        "post_binary_hook": {
            "function": "MTSCode.combine_bins_mtb_mts_dragonfly",
            "toolchains": ["GCC_ARM", "ARM_STD", "ARM_MICRO", "IAR"]
        },
        "release_versions": ["2", "5"],
        "device_name": "STM32F411RE",
        "bootloader_supported": true
    },
    "XDOT_L151CC": {
        "inherits": ["FAMILY_STM32"],
        "core": "Cortex-M3",
        "default_toolchain": "ARM",
        "extra_labels_add": ["STM32L1", "STM32L151CC"],
        "config": {
            "hse_value": {
            "value": "24000000",
            "macro_name": "HSE_VALUE"
            }
        },
        "supported_toolchains": ["ARM", "GCC_ARM", "IAR"],
        "device_has_add": ["ANALOGOUT", "FLASH"],
        "release_versions": ["5"],
        "device_name": "STM32L151CC",
        "bootloader_supported": true
    },
    "FF1705_L151CC": {
        "supported_form_factors": ["ARDUINO"],
        "inherits": ["XDOT_L151CC"],
        "detect_code": ["8080"]
    },
    "MTB_MTS_XDOT": {
        "inherits": ["FAMILY_STM32"],
        "core": "Cortex-M3",
        "default_toolchain": "ARM",
        "extra_labels_add": ["STM32L1", "STM32L151CC"],
        "config": {
            "hse_value": {
            "value": "24000000",
            "macro_name": "HSE_VALUE"
            }
        },
        "overrides": {
            "stdio_uart_tx": "PA_2",
            "stdio_uart_rx": "PA_3"
        },
        "supported_toolchains": ["ARM", "GCC_ARM", "IAR"],
        "device_has_add": ["ANALOGOUT", "FLASH"],
        "release_versions": ["5"],
        "device_name": "STM32L151CC",
        "bootloader_supported": true
    },
    "MTB_RAK811": {
        "inherits": ["FAMILY_STM32"],
        "core": "Cortex-M3",
        "default_toolchain": "ARM",
        "extra_labels_add": ["STM32L1", "STM32L151xBA", "STM32L151CBA"],
        "supported_toolchains": ["ARM", "GCC_ARM", "IAR"],
        "device_has_add": ["ANALOGOUT"],
        "release_versions": ["5"],
        "device_name": "STM32L151CBxxA",
        "bootloader_supported": true
    },
    "MOTE_L152RC": {
        "inherits": ["FAMILY_STM32"],
        "supported_form_factors": ["ARDUINO"],
        "core": "Cortex-M3",
        "default_toolchain": "ARM",
        "supported_toolchains": ["ARM", "GCC_ARM", "IAR"],
        "extra_labels_add": ["STM32L1", "STM32L152RC"],
        "detect_code": ["4100"],
        "device_has_add": ["ANALOGOUT", "SERIAL_ASYNCH", "FLASH"],
        "release_versions": ["2", "5"],
        "device_name": "STM32L152RC"
    },
    "DISCO_F401VC": {
        "inherits": ["FAMILY_STM32"],
        "core": "Cortex-M4F",
        "default_toolchain": "GCC_ARM",
        "extra_labels_add": ["STM32F4", "STM32F401", "STM32F401xC", "STM32F401VC"],
        "supported_toolchains": ["GCC_ARM"],
        "device_has_add": [],
        "device_name": "STM32F401VC"
    },
    "MODULE_UBLOX_ODIN_W2": {
        "inherits": ["FAMILY_STM32"],
        "core": "Cortex-M4F",
        "extra_labels_add": ["STM32F4", "STM32F439", "STM32F439ZI","STM32F439xx", "STM32F439xI", "STM_EMAC","CORDIO", "CORDIO_ODIN_W2"],
        "macros": ["MBEDTLS_CONFIG_HW_SUPPORT", "HSE_VALUE=24000000", "HSE_STARTUP_TIMEOUT=5000", "CB_INTERFACE_SDIO","CB_CHIP_WL18XX","SUPPORT_80211D_ALWAYS","WLAN_ENABLED","CB_FEATURE_802DOT11W","CB_FEATURE_802DOT11R","MBEDTLS_ARC4_C","MBEDTLS_DES_C","MBEDTLS_MD4_C","MBEDTLS_MD5_C","MBEDTLS_SHA1_C"],
        "device_has_add": ["CAN", "EMAC", "TRNG", "FLASH", "WIFI", "SERIAL_FC", "SERIAL"],
        "features": ["BLE"],
        "device_has_remove": [],
        "device_name": "STM32F439ZI",
        "public": false,
        "bootloader_supported": true,
        "config": {
            "BLE_STACK_UBX": {
                "help": "It should be set to true to enable ublox ODIN own stack/driver rather than CORDIO",
                "value": false,
                "macro_name": "BLE_STACK_UBX"
            }
        },
        "overrides": {
            "network-default-interface-type": "WIFI"
        }
    },
    "UBLOX_EVK_ODIN_W2": {
        "inherits": ["MODULE_UBLOX_ODIN_W2"],
        "supported_form_factors": ["ARDUINO"],
        "release_versions": ["5"],
        "device_has_remove": [],
        "config": {
            "stdio_uart_tx_help": {
                "help": "Value: D8(default) or D1"
            },
            "stdio_uart_rx_help": {
                "help": "Value: D2(default) or D0"
            }
        },
        "overrides": {
            "stdio_uart_tx": "D8",
            "stdio_uart_rx": "D2"
        }
    },
    "MBED_CONNECT_ODIN": {
        "inherits": ["MODULE_UBLOX_ODIN_W2"],
        "release_versions": ["5"],
        "config": {
            "stdio_uart_tx_help": {
                "help": "Value: PA_9(default) or PD_8"
            },
            "stdio_uart_rx_help": {
                "help": "Value: PA_10(default) or PD_9"
            }
        },
        "overrides": {
            "stdio_uart_tx": "PA_9",
            "stdio_uart_rx": "PA_10"
        }
    },
    "MTB_UBLOX_ODIN_W2": {
        "inherits": ["MODULE_UBLOX_ODIN_W2"],
        "device_has_add": [],
        "release_versions": ["5"]
     },
    "UBLOX_C030": {
        "inherits": ["FAMILY_STM32"],
        "supported_form_factors": ["ARDUINO"],
        "core": "Cortex-M4F",
        "supported_toolchains": ["GCC_ARM", "ARM", "IAR"],
        "extra_labels_add": ["STM32F4", "STM32F437", "STM32F437VG", "STM32F437xx", "STM32F437xG", "STM_EMAC"],
        "config": {
            "modem_is_on_board": {
                "help": "Value: Tells the build system that the modem is on-board as oppose to a plug-in shield/module.",
                "value": 1,
                "macro_name": "MODEM_ON_BOARD"
            },
            "modem_data_connection_type": {
                "help": "Value: Defines how the modem is wired up to the MCU, e.g., data connection can be a UART or USB and so forth.",
                "value": 1,
                "macro_name": "MODEM_ON_BOARD_UART"
            }
        },
        "macros_add": ["MBEDTLS_CONFIG_HW_SUPPORT", "HSE_VALUE=12000000", "GNSSBAUD=9600"],
        "overrides": {"lse_available": 0},
        "device_has_add": ["ANALOGOUT", "EMAC", "SERIAL_FC", "TRNG", "FLASH"],
        "public": false,
        "device_name": "STM32F437VG",
        "bootloader_supported": true,
        "overrides": {
            "network-default-interface-type": "ETHERNET"
        }
    },
    "UBLOX_C030_U201": {
        "inherits": ["UBLOX_C030"],
        "release_versions": ["5"]
    },
    "UBLOX_C030_N211": {
        "inherits": ["UBLOX_C030"],
        "release_versions": ["5"]
    },
    "UBLOX_C030_R410M": {
        "inherits": ["UBLOX_C030"],
        "release_versions": ["5"]
    },
    "NZ32_SC151": {
        "inherits": ["FAMILY_STM32"],
        "core": "Cortex-M3",
        "default_toolchain": "uARM",
        "program_cycle_s": 1.5,
        "extra_labels_add": ["STM32L1", "STM32L151RC"],
        "overrides": {"lse_available": 0},
        "supported_toolchains": ["ARM", "uARM", "GCC_ARM"],
        "device_has_add": ["ANALOGOUT"],
        "default_lib": "small",
        "device_name": "STM32L151RC"
    },
    "MCU_NRF51": {
        "inherits": ["Target"],
        "core": "Cortex-M0",
        "OVERRIDE_BOOTLOADER_FILENAME": "nrf51822_bootloader.hex",
        "macros": ["NRF51", "TARGET_NRF51822", "CMSIS_VECTAB_VIRTUAL", "CMSIS_VECTAB_VIRTUAL_HEADER_FILE=\"cmsis_nvic.h\""],
        "MERGE_BOOTLOADER": false,
        "extra_labels": ["NORDIC", "MCU_NRF51", "MCU_NRF51822"],
        "OUTPUT_EXT": "hex",
        "is_disk_virtual": true,
        "supported_toolchains": ["ARM", "GCC_ARM"],
        "public": false,
        "MERGE_SOFT_DEVICE": true,
        "EXPECTED_SOFTDEVICES_WITH_OFFSETS": [
            {
                "boot": "s130_nrf51_1.0.0_bootloader.hex",
                "name": "s130_nrf51_1.0.0_softdevice.hex",
                "offset": 114688
            },
            {
                "boot": "s110_nrf51822_8.0.0_bootloader.hex",
                "name": "s110_nrf51822_8.0.0_softdevice.hex",
                "offset": 98304
            },
            {
                "boot": "s110_nrf51822_7.1.0_bootloader.hex",
                "name": "s110_nrf51822_7.1.0_softdevice.hex",
                "offset": 90112
            },
            {
                "boot": "s110_nrf51822_7.0.0_bootloader.hex",
                "name": "s110_nrf51822_7.0.0_softdevice.hex",
                "offset": 90112
            },
            {
                "boot": "s110_nrf51822_6.0.0_bootloader.hex",
                "name": "s110_nrf51822_6.0.0_softdevice.hex",
                "offset": 81920
            }
        ],
        "detect_code": ["1070"],
        "post_binary_hook": {
            "function": "MCU_NRF51Code.binary_hook",
            "toolchains": ["ARM_STD", "GCC_ARM"]
        },
        "program_cycle_s": 6,
        "features": ["BLE"],
        "device_has": ["ANALOGIN", "I2C", "INTERRUPTIN", "PORTIN", "PORTINOUT", "PORTOUT", "PWMOUT", "SERIAL", "SLEEP", "SPI", "SPISLAVE"]
    },
    "MCU_NRF51_16K_BASE": {
        "inherits": ["MCU_NRF51"],
        "extra_labels_add": ["MCU_NORDIC_16K", "MCU_NRF51_16K"],
        "macros_add": ["TARGET_MCU_NORDIC_16K", "TARGET_MCU_NRF51_16K"],
        "public": false,
        "default_lib": "small"
    },
    "MCU_NRF51_16K_BOOT_BASE": {
        "inherits": ["MCU_NRF51_16K_BASE"],
        "MERGE_BOOTLOADER": true,
        "extra_labels_add": ["MCU_NRF51_16K_BOOT"],
        "macros_add": ["TARGET_MCU_NRF51_16K_BOOT", "TARGET_OTA_ENABLED"],
        "public": false
    },
    "MCU_NRF51_16K_OTA_BASE": {
        "inherits": ["MCU_NRF51_16K_BASE"],
        "public": false,
        "extra_labels_add": ["MCU_NRF51_16K_OTA"],
        "macros_add": ["TARGET_MCU_NRF51_16K_OTA", "TARGET_OTA_ENABLED"],
        "MERGE_SOFT_DEVICE": false
    },
    "MCU_NRF51_16K": {
        "inherits": ["MCU_NRF51_16K_BASE"],
        "extra_labels_add": ["MCU_NRF51_16K_S130"],
        "macros_add": ["TARGET_MCU_NRF51_16K_S130"],
        "public": false
    },
    "MCU_NRF51_S110": {
        "extra_labels_add": ["MCU_NRF51_16K_S110"],
        "macros_add": ["TARGET_MCU_NRF51_16K_S110"],
        "EXPECTED_SOFTDEVICES_WITH_OFFSETS": [
            {
                "name": "s110_nrf51822_8.0.0_softdevice.hex",
                "boot": "s110_nrf51822_8.0.0_bootloader.hex",
                "offset": 98304
            },
            {
                "name": "s110_nrf51822_7.1.0_softdevice.hex",
                "boot": "s110_nrf51822_7.1.0_bootloader.hex",
                "offset": 90112
            }
        ],
        "public": false
    },
    "MCU_NRF51_16K_S110": {
        "inherits": ["MCU_NRF51_S110", "MCU_NRF51_16K_BASE"],
        "public": false
    },
    "MCU_NRF51_16K_BOOT": {
        "inherits": ["MCU_NRF51_16K_BOOT_BASE"],
        "extra_labels_add": ["MCU_NRF51_16K_S130"],
        "macros_add": ["TARGET_MCU_NRF51_16K_S130"],
        "public": false
    },
    "MCU_NRF51_16K_BOOT_S110": {
        "inherits": ["MCU_NRF51_S110", "MCU_NRF51_16K_BOOT_BASE"],
        "public": false
    },
    "MCU_NRF51_16K_OTA": {
        "inherits": ["MCU_NRF51_16K_OTA_BASE"],
        "extra_labels_add": ["MCU_NRF51_16K_S130"],
        "macros_add": ["TARGET_MCU_NRF51_16K_S130"],
        "public": false
    },
    "MCU_NRF51_16K_OTA_S110": {
        "inherits": ["MCU_NRF51_S110", "MCU_NRF51_16K_OTA_BASE"],
        "public": false
    },
    "MCU_NRF51_32K": {
        "inherits": ["MCU_NRF51"],
        "extra_labels_add": ["MCU_NORDIC_32K", "MCU_NRF51_32K"],
        "macros_add": ["TARGET_MCU_NORDIC_32K", "TARGET_MCU_NRF51_32K"],
        "public": false
    },
    "MCU_NRF51_32K_BOOT": {
        "inherits": ["MCU_NRF51_32K"],
        "MERGE_BOOTLOADER": true,
        "extra_labels_add": ["MCU_NRF51_32K_BOOT"],
        "macros_add": ["TARGET_MCU_NRF51_32K_BOOT", "TARGET_OTA_ENABLED"],
        "public": false
    },
    "MCU_NRF51_32K_OTA": {
        "inherits": ["MCU_NRF51_32K"],
        "public": false,
        "extra_labels_add": ["MCU_NRF51_32K_OTA"],
        "macros_add": ["TARGET_MCU_NRF51_32K_OTA", "TARGET_OTA_ENABLED"],
        "MERGE_SOFT_DEVICE": false
    },
    "NRF51822": {
        "inherits": ["MCU_NRF51_16K"],
        "extra_labels_add": ["NRF51822", "NRF51822_MKIT"],
        "macros_add": ["TARGET_NRF51822_MKIT"],
        "release_versions": ["2"],
        "device_name": "nRF51822_xxAA"
    },
    "NRF51822_BOOT": {
        "inherits": ["MCU_NRF51_16K_BOOT"],
        "extra_labels_add": ["NRF51822", "NRF51822_MKIT"],
        "macros_add": ["TARGET_NRF51822_MKIT"]
    },
    "NRF51822_OTA": {
        "inherits": ["MCU_NRF51_16K_OTA"],
        "extra_labels_add": ["NRF51822", "NRF51822_MKIT"],
        "macros_add": ["TARGET_NRF51822_MKIT"]
    },
    "ARCH_BLE": {
        "supported_form_factors": ["ARDUINO"],
        "inherits": ["MCU_NRF51_16K"],
        "release_versions": ["2"],
        "device_name": "nRF51822_xxAA"
    },
    "ARCH_BLE_BOOT": {
        "supported_form_factors": ["ARDUINO"],
        "inherits": ["MCU_NRF51_16K_BOOT"],
        "extra_labels_add": ["ARCH_BLE"],
        "macros_add": ["TARGET_ARCH_BLE"]
    },
    "ARCH_BLE_OTA": {
        "supported_form_factors": ["ARDUINO"],
        "inherits": ["MCU_NRF51_16K_OTA"],
        "extra_labels_add": ["ARCH_BLE"],
        "macros_add": ["TARGET_ARCH_BLE"]
    },
    "ARCH_LINK": {
        "supported_form_factors": ["ARDUINO"],
        "inherits": ["MCU_NRF51_16K"],
        "extra_labels_add": ["ARCH_BLE"],
        "macros_add": ["TARGET_ARCH_BLE"]
    },
    "ARCH_LINK_BOOT": {
        "supported_form_factors": ["ARDUINO"],
        "inherits": ["MCU_NRF51_16K_BOOT"],
        "extra_labels_add": ["ARCH_BLE", "ARCH_LINK"],
        "macros_add": ["TARGET_ARCH_BLE", "TARGET_ARCH_LINK"]
    },
    "ARCH_LINK_OTA": {
        "supported_form_factors": ["ARDUINO"],
        "inherits": ["MCU_NRF51_16K_OTA"],
        "extra_labels_add": ["ARCH_BLE", "ARCH_LINK"],
        "macros_add": ["TARGET_ARCH_BLE", "TARGET_ARCH_LINK"]
    },
    "SEEED_TINY_BLE": {
        "inherits": ["MCU_NRF51_16K"],
        "release_versions": ["2"],
        "device_name": "nRF51822_xxAA"
    },
    "SEEED_TINY_BLE_BOOT": {
        "inherits": ["MCU_NRF51_16K_BOOT"],
        "extra_labels_add": ["SEEED_TINY_BLE"],
        "macros_add": ["TARGET_SEEED_TINY_BLE"]
    },
    "SEEED_TINY_BLE_OTA": {
        "inherits": ["MCU_NRF51_16K_OTA"],
        "extra_labels_add": ["SEEED_TINY_BLE"],
        "macros_add": ["TARGET_SEEED_TINY_BLE"]
    },
    "HRM1017": {
        "inherits": ["MCU_NRF51_16K"],
        "macros_add": ["TARGET_NRF_LFCLK_RC"],
        "release_versions": ["2"],
        "device_name": "nRF51822_xxAA"
    },
    "HRM1017_BOOT": {
        "inherits": ["MCU_NRF51_16K_BOOT"],
        "extra_labels_add": ["HRM1017"],
        "macros_add": ["TARGET_HRM1017", "TARGET_NRF_LFCLK_RC"]
    },
    "HRM1017_OTA": {
        "inherits": ["MCU_NRF51_16K_OTA"],
        "extra_labels_add": ["HRM1017"],
        "macros_add": ["TARGET_HRM1017", "TARGET_NRF_LFCLK_RC"]
    },
    "RBLAB_NRF51822": {
        "supported_form_factors": ["ARDUINO"],
        "inherits": ["MCU_NRF51_16K"],
        "release_versions": ["2"],
        "device_name": "nRF51822_xxAA"
    },
    "RBLAB_NRF51822_BOOT": {
        "supported_form_factors": ["ARDUINO"],
        "inherits": ["MCU_NRF51_16K_BOOT"],
        "extra_labels_add": ["RBLAB_NRF51822"],
        "macros_add": ["TARGET_RBLAB_NRF51822"]
    },
    "RBLAB_NRF51822_OTA": {
        "supported_form_factors": ["ARDUINO"],
        "inherits": ["MCU_NRF51_16K_OTA"],
        "extra_labels_add": ["RBLAB_NRF51822"],
        "macros_add": ["TARGET_RBLAB_NRF51822"]
    },
    "RBLAB_BLENANO": {
        "inherits": ["MCU_NRF51_16K"],
        "release_versions": ["2"]
    },
    "RBLAB_BLENANO_BOOT": {
        "inherits": ["MCU_NRF51_16K_BOOT"],
        "extra_labels_add": ["RBLAB_BLENANO"],
        "macros_add": ["TARGET_RBLAB_BLENANO"]
    },
    "RBLAB_BLENANO_OTA": {
        "inherits": ["MCU_NRF51_16K_OTA"],
        "extra_labels_add": ["RBLAB_BLENANO"],
        "macros_add": ["TARGET_RBLAB_BLENANO"]
    },
    "RBLAB_BLENANO2": {
        "supported_form_factors": ["ARDUINO"],
        "inherits": ["MCU_NRF52832"],
        "release_versions": ["5"],
        "device_name": "nRF52832_xxAA"
    },
    "NRF51822_Y5_MBUG": {
        "inherits": ["MCU_NRF51_16K"]
    },
    "WALLBOT_BLE": {
        "inherits": ["MCU_NRF51_16K"],
        "release_versions": ["2"]
    },
    "WALLBOT_BLE_BOOT": {
        "inherits": ["MCU_NRF51_16K_BOOT"],
        "extra_labels_add": ["WALLBOT_BLE"],
        "macros_add": ["TARGET_WALLBOT_BLE"]
    },
    "WALLBOT_BLE_OTA": {
        "inherits": ["MCU_NRF51_16K_OTA"],
        "extra_labels_add": ["WALLBOT_BLE"],
        "macros_add": ["TARGET_WALLBOT_BLE"]
    },
    "DELTA_DFCM_NNN40": {
        "inherits": ["MCU_NRF51_32K"],
        "program_cycle_s": 10,
        "macros_add": ["TARGET_NRF_LFCLK_RC"],
        "device_has": ["ANALOGIN", "DEBUG_AWARENESS", "I2C", "INTERRUPTIN", "PORTIN", "PORTINOUT", "PORTOUT", "PWMOUT", "SERIAL", "SLEEP", "SPI", "SPISLAVE"],
        "release_versions": ["2"],
        "device_name": "nRF51822_xxAA"
    },
    "DELTA_DFCM_NNN40_BOOT": {
        "inherits": ["MCU_NRF51_32K_BOOT"],
        "program_cycle_s": 10,
        "extra_labels_add": ["DELTA_DFCM_NNN40"],
        "macros_add": ["TARGET_DELTA_DFCM_NNN40", "TARGET_NRF_LFCLK_RC"]
    },
    "DELTA_DFCM_NNN40_OTA": {
        "inherits": ["MCU_NRF51_32K_OTA"],
        "program_cycle_s": 10,
        "extra_labels_add": ["DELTA_DFCM_NNN40"],
        "macros_add": ["TARGET_DELTA_DFCM_NNN40", "TARGET_NRF_LFCLK_RC"]
    },
    "DELTA_DFCM_NNN50": {
        "supported_form_factors": ["ARDUINO"],
        "inherits": ["MCU_NRF51_32K_UNIFIED"],
        "device_has": ["USTICKER", "LPTICKER", "ANALOGIN", "I2C", "I2C_ASYNCH", "INTERRUPTIN", "PORTIN", "PORTINOUT", "PORTOUT", "PWMOUT", "SERIAL", "SERIAL_ASYNCH", "SERIAL_FC", "SLEEP", "SPI", "SPI_ASYNCH", "SPISLAVE"],
        "device_name": "nRF51822_xxAC"
    },
    "DELTA_DFCM_NNN50_BOOT": {
        "supported_form_factors": ["ARDUINO"],
        "inherits": ["MCU_NRF51_32K_BOOT"],
        "extra_labels_add": ["DELTA_DFCM_NNN50"],
        "macros_add": ["TARGET_DELTA_DFCM_NNN50"]
    },
    "DELTA_DFCM_NNN50_OTA": {
        "supported_form_factors": ["ARDUINO"],
        "inherits": ["MCU_NRF51_32K_OTA"],
        "extra_labels_add": ["DELTA_DFCM_NNN50"],
        "macros_add": ["TARGET_DELTA_DFCM_NNN50"]
    },
    "NRF51_DK_LEGACY": {
        "supported_form_factors": ["ARDUINO"],
        "inherits": ["MCU_NRF51_32K"],
        "extra_labels_add": ["NRF51_DK"]
    },
    "NRF51_DK_BOOT": {
        "supported_form_factors": ["ARDUINO"],
        "inherits": ["MCU_NRF51_32K_BOOT"],
        "extra_labels_add": ["NRF51_DK"],
        "macros_add": ["TARGET_NRF51_DK"]
    },
    "NRF51_DK_OTA": {
        "supported_form_factors": ["ARDUINO"],
        "inherits": ["MCU_NRF51_32K_OTA"],
        "extra_labels_add": ["NRF51_DK"],
        "macros_add": ["TARGET_NRF51_DK"]
    },
    "NRF51_DONGLE_LEGACY": {
        "inherits": ["MCU_NRF51_32K"],
        "extra_labels_add": ["NRF51_DONGLE"],
        "release_versions": ["2"],
        "device_name": "nRF51822_xxAA"
    },
    "NRF51_DONGLE_BOOT": {
        "inherits": ["MCU_NRF51_32K_BOOT"],
        "extra_labels_add": ["NRF51_DONGLE"],
        "macros_add": ["TARGET_NRF51_DONGLE"]
    },
    "NRF51_DONGLE_OTA": {
        "inherits": ["MCU_NRF51_32K_OTA"],
        "extra_labels_add": ["NRF51_DONGLE"],
        "macros_add": ["TARGET_NRF51_DONGLE"]
    },
    "NRF51_MICROBIT": {
        "inherits": ["MCU_NRF51_16K_S110"],
        "macros_add": ["TARGET_NRF_LFCLK_RC"],
        "release_versions": ["2"],
        "device_name": "nRF51822_xxAA"
    },
    "NRF51_MICROBIT_BOOT": {
        "inherits": ["MCU_NRF51_16K_BOOT_S110"],
        "extra_labels_add": ["NRF51_MICROBIT"],
        "macros_add": ["TARGET_NRF51_MICROBIT", "TARGET_NRF_LFCLK_RC"]
    },
    "NRF51_MICROBIT_OTA": {
        "inherits": ["MCU_NRF51_16K_OTA_S110"],
        "extra_labels_add": ["NRF51_MICROBIT"],
        "macros_add": ["TARGET_NRF51_MICROBIT", "TARGET_NRF_LFCLK_RC"]
    },
    "NRF51_MICROBIT_B": {
        "inherits": ["MCU_NRF51_16K"],
        "extra_labels_add": ["NRF51_MICROBIT"],
        "macros_add": ["TARGET_NRF51_MICROBIT", "TARGET_NRF_LFCLK_RC"],
        "release_versions": ["2"]
    },
    "NRF51_MICROBIT_B_BOOT": {
        "inherits": ["MCU_NRF51_16K_BOOT"],
        "extra_labels_add": ["NRF51_MICROBIT"],
        "macros_add": ["TARGET_NRF51_MICROBIT", "TARGET_NRF_LFCLK_RC"]
    },
    "NRF51_MICROBIT_B_OTA": {
        "inherits": ["MCU_NRF51_16K_OTA"],
        "extra_labels_add": ["NRF51_MICROBIT"],
        "macros_add": ["TARGET_NRF51_MICROBIT", "TARGET_NRF_LFCLK_RC"]
    },
    "MTM_MTCONNECT04S": {
        "inherits": ["MCU_NRF51_32K"],
        "release_versions": ["2"],
        "device_name": "nRF51822_xxAA"
    },
    "MTM_MTCONNECT04S_BOOT": {
        "inherits": ["MCU_NRF51_32K_BOOT"],
        "extra_labels_add": ["MTM_CONNECT04S"],
        "macros_add": ["TARGET_MTM_CONNECT04S"]
    },
    "MTM_MTCONNECT04S_OTA": {
        "inherits": ["MCU_NRF51_32K_OTA"],
        "extra_labels_add": ["MTM_CONNECT04S"],
        "macros_add": ["TARGET_MTM_CONNECT04S"]
    },
    "MTB_LAIRD_BL600": {
        "inherits": ["MCU_NRF51_32K_UNIFIED"],
        "device_has": ["USTICKER", "LPTICKER", "ANALOGIN", "I2C", "I2C_ASYNCH", "INTERRUPTIN", "PORTIN", "PORTINOUT", "PORTOUT", "PWMOUT", "SERIAL", "SERIAL_ASYNCH", "SERIAL_FC", "SLEEP", "SPI", "SPI_ASYNCH", "SPISLAVE"],
        "device_name": "nRF51822_xxAA",
        "release_versions" : ["5"],
        "extra_labels_add": ["MTB_LAIRD_BL600"],
        "config": {
            "usb_tx": {
                "help": "Value SIO_21",
                "value": "SIO_21"
            },
            "usb_rx": {
                "help": "Value SIO_22",
                "value": "SIO_22"
            },
            "stdio_uart": {
                "help": "Value: UART_0",
                "value": "UART_0",
                "macro_name": "STDIO_UART"
             }
        },
        "overrides": {
                "uart_hwfc": 0
        }
    },
    "TY51822R3": {
        "inherits": ["MCU_NRF51_32K_UNIFIED"],
        "macros_add": ["TARGET_NRF_32MHZ_XTAL"],
        "device_has": ["USTICKER", "LPTICKER", "ANALOGIN", "I2C", "I2C_ASYNCH", "INTERRUPTIN", "PORTIN", "PORTINOUT", "PORTOUT", "PWMOUT", "SERIAL", "SERIAL_ASYNCH", "SLEEP", "SPI", "SPI_ASYNCH", "SPISLAVE"],
        "detect_code": ["1019"],
        "release_versions": ["2", "5"],
        "overrides": {"uart_hwfc": 0},
        "device_name": "nRF51822_xxAA"
    },
    "TY51822R3_BOOT": {
        "inherits": ["MCU_NRF51_32K_BOOT"],
        "extra_labels_add": ["TY51822R3"],
        "macros_add": ["TARGET_TY51822R3", "TARGET_NRF_32MHZ_XTAL"]
    },
    "TY51822R3_OTA": {
        "inherits": ["MCU_NRF51_32K_OTA"],
        "extra_labels_add": ["NRF51_DK"],
        "macros_add": ["TARGET_TY51822R3", "TARGET_NRF_32MHZ_XTAL"]
    },
    "ARM_MPS2_Target": {
        "inherits": ["Target"],
        "public": false,
        "device_has": ["AACI", "ANALOGIN", "CLCD", "ETHERNET", "I2C", "INTERRUPTIN", "PORTIN", "PORTINOUT", "PORTOUT", "SERIAL", "SERIAL_FC", "SPI", "SPISLAVE", "TSC"]
    },
    "ARM_MPS2_M0": {
        "inherits": ["ARM_MPS2_Target"],
        "core": "Cortex-M0",
        "supported_toolchains": ["ARM"],
        "extra_labels": ["ARM_SSG", "MPS2", "MPS2_M0"],
        "macros": ["CMSDK_CM0", "CMSIS_VECTAB_VIRTUAL", "CMSIS_VECTAB_VIRTUAL_HEADER_FILE=\"cmsis_nvic.h\""],
        "device_has": ["AACI", "ANALOGIN", "CLCD", "ETHERNET", "I2C", "INTERRUPTIN", "PORTIN", "PORTINOUT", "PORTOUT", "SERIAL", "SERIAL_FC", "SPI", "SPISLAVE", "TSC"],
        "release_versions": ["2"]
    },
    "ARM_MPS2_M0P": {
        "inherits": ["ARM_MPS2_Target"],
        "core": "Cortex-M0+",
        "supported_toolchains": ["ARM"],
        "extra_labels": ["ARM_SSG", "MPS2", "MPS2_M0P"],
        "macros": ["CMSDK_CM0plus"],
        "device_has": ["AACI", "ANALOGIN", "CLCD", "ETHERNET", "I2C", "INTERRUPTIN", "PORTIN", "PORTINOUT", "PORTOUT", "SERIAL", "SERIAL_FC", "SPI", "SPISLAVE", "TSC"],
        "release_versions": ["2"]
    },
    "ARM_MPS2_M3": {
        "inherits": ["ARM_MPS2_Target"],
        "core": "Cortex-M3",
        "supported_toolchains": ["ARM"],
        "extra_labels": ["ARM_SSG", "MPS2", "MPS2_M3"],
        "macros": ["CMSDK_CM3"],
        "device_has": ["AACI", "ANALOGIN", "CLCD", "ETHERNET", "I2C", "INTERRUPTIN", "PORTIN", "PORTINOUT", "PORTOUT", "SERIAL", "SERIAL_FC", "SPI", "SPISLAVE", "TSC"],
        "release_versions": ["2"]
    },
    "ARM_MPS2_M4": {
        "inherits": ["ARM_MPS2_Target"],
        "core": "Cortex-M4F",
        "supported_toolchains": ["ARM"],
        "extra_labels": ["ARM_SSG", "MPS2", "MPS2_M4"],
        "macros": ["CMSDK_CM4"],
        "device_has": ["AACI", "ANALOGIN", "CLCD", "ETHERNET", "I2C", "INTERRUPTIN", "PORTIN", "PORTINOUT", "PORTOUT", "SERIAL", "SERIAL_FC", "SPI", "SPISLAVE", "TSC"],
        "release_versions": ["2"]
    },
    "ARM_MPS2_M7": {
        "inherits": ["ARM_MPS2_Target"],
        "core": "Cortex-M7",
        "supported_toolchains": ["ARM"],
        "extra_labels": ["ARM_SSG", "MPS2", "MPS2_M7"],
        "macros": ["CMSDK_CM7"],
        "device_has": ["AACI", "ANALOGIN", "CLCD", "ETHERNET", "I2C", "INTERRUPTIN", "PORTIN", "PORTINOUT", "PORTOUT", "SERIAL", "SERIAL_FC", "SPI", "SPISLAVE", "TSC"],
        "release_versions": ["2"]
    },
    "ARM_IOTSS_Target": {
        "inherits": ["Target"],
        "public": false,
        "device_has": ["AACI", "ANALOGIN", "CLCD", "ETHERNET", "I2C", "INTERRUPTIN", "PORTIN", "PORTINOUT", "PORTOUT", "SERIAL", "SERIAL_FC", "SPI", "SPISLAVE", "TSC"]
    },
    "ARM_IOTSS_BEID": {
        "inherits": ["ARM_IOTSS_Target"],
        "core": "Cortex-M3",
        "supported_toolchains": ["ARM"],
        "extra_labels": ["ARM_SSG", "IOTSS", "IOTSS_BEID"],
        "macros": ["CMSDK_BEID"],
        "device_has": ["AACI", "ANALOGIN", "CLCD", "ETHERNET", "I2C", "INTERRUPTIN", "PORTIN", "PORTINOUT", "PORTOUT", "SERIAL", "SERIAL_FC", "SPI", "SPISLAVE", "TSC"],
        "release_versions": ["2"]
    },
     "ARM_CM3DS_MPS2": {
        "inherits": ["ARM_IOTSS_Target"],
        "core": "Cortex-M3",
        "supported_toolchains": ["ARM", "GCC_ARM", "IAR"],
        "components": ["SMSC9220"],
        "extra_labels": ["ARM_SSG", "CM3DS_MPS2"],
        "OUTPUT_EXT": "elf",
        "macros": ["CMSDK_CM3DS"],
        "device_has": ["ANALOGIN", "EMAC", "FLASH", "I2C", "INTERRUPTIN", "PORTIN", "PORTINOUT", "PORTOUT", "SERIAL", "SPI", "TRNG"],
        "release_versions": ["2", "5"],
        "copy_method": "mps2",
        "reset_method": "reboot.txt",
        "overrides": {
                "target.network-default-interface-type": "ETHERNET"
        }
    },
    "ARM_BEETLE_SOC": {
        "inherits": ["ARM_IOTSS_Target"],
        "core": "Cortex-M3",
        "supported_toolchains": ["ARM", "GCC_ARM", "IAR"],
        "default_toolchain": "ARM",
        "extra_labels": ["ARM_SSG", "BEETLE"],
        "macros": ["CMSDK_BEETLE", "WSF_MS_PER_TICK=20", "WSF_TOKEN_ENABLED=FALSE", "WSF_TRACE_ENABLED=TRUE", "WSF_ASSERT_ENABLED=FALSE", "WSF_PRINTF_MAX_LEN=128", "ASIC", "CONFIG_HOST_REV=0x20", "CONFIG_ALLOW_DEEP_SLEEP=FALSE", "HCI_VS_TARGET", "CONFIG_ALLOW_SETTING_WRITE=TRUE", "WSF_MAX_HANDLERS=20", "NO_LEDS"],
        "device_has": ["ANALOGIN", "CLCD", "I2C", "INTERRUPTIN", "PORTIN", "PORTINOUT", "PORTOUT", "SERIAL", "SLEEP", "SPI"],
        "features": ["BLE"],
        "release_versions": ["2", "5"]
    },
    "RZ_A1XX": {
        "inherits": ["Target"],
        "core": "Cortex-A9",
        "supported_toolchains": ["ARM", "GCC_ARM", "IAR"],
        "extra_labels": ["RENESAS", "RZ_A1XX"],
        "device_has": ["SLEEP", "USTICKER", "RTC", "ANALOGIN", "CAN", "ETHERNET", "I2C", "I2CSLAVE", "I2C_ASYNCH", "INTERRUPTIN", "PORTIN", "PORTINOUT", "PORTOUT", "PWMOUT", "SERIAL", "SERIAL_ASYNCH", "SERIAL_FC", "SPI", "SPISLAVE", "SPI_ASYNCH", "STDIO_MESSAGES"],
        "program_cycle_s": 2,
        "overrides": {
            "network-default-interface-type": "ETHERNET"
        }
    },
    "RZ_A1H": {
        "inherits": ["RZ_A1XX"],
        "supported_form_factors": ["ARDUINO"],
        "extra_labels_add": ["RZA1H", "MBRZA1H", "RZ_A1_EMAC"],
        "device_has_add": ["EMAC", "FLASH", "LPTICKER"],
        "release_versions": ["2", "5"],
        "device_name": "R7S72100",
        "bootloader_supported": true
    },
    "VK_RZ_A1H": {
        "inherits": ["RZ_A1XX"],
        "extra_labels_add": ["RZA1H", "VKRZA1H", "RZ_A1_EMAC"],
        "device_has_add": ["EMAC"],
        "release_versions": ["2", "5"]
    },
    "GR_LYCHEE": {
        "inherits": ["RZ_A1XX"],
        "supported_form_factors": ["ARDUINO"],
        "extra_labels_add": ["RZA1UL", "MBRZA1LU"],
        "device_has_add": ["TRNG", "FLASH", "LPTICKER"],
        "device_has_remove": ["ETHERNET"],
        "release_versions": ["2", "5"],
        "device_name": "R7S72103",
        "bootloader_supported": true,
        "overrides": {
            "network-default-interface-type": null
        }
    },
    "MAXWSNENV": {
        "inherits": ["Target"],
        "core": "Cortex-M3",
        "macros": ["__SYSTEM_HFX=24000000"],
        "extra_labels": ["Maxim", "MAX32610"],
        "supported_toolchains": ["GCC_ARM", "IAR", "ARM"],
        "device_has": ["ANALOGIN", "ANALOGOUT", "I2C", "INTERRUPTIN", "PORTIN", "PORTINOUT", "PORTOUT", "PWMOUT", "SERIAL", "SERIAL_FC", "SLEEP", "SPI", "STDIO_MESSAGES"],
        "features": ["BLE"],
        "release_versions": []
    },
    "MAX32600MBED": {
        "inherits": ["Target"],
        "core": "Cortex-M3",
        "macros": ["__SYSTEM_HFX=24000000"],
        "extra_labels": ["Maxim", "MAX32600"],
        "supported_toolchains": ["GCC_ARM", "IAR", "ARM"],
        "device_has": ["ANALOGIN", "ANALOGOUT", "I2C", "INTERRUPTIN", "PORTIN", "PORTINOUT", "PORTOUT", "PWMOUT", "SERIAL", "SERIAL_FC", "SLEEP", "SPI", "STDIO_MESSAGES"],
        "release_versions": ["2", "5"]
    },
    "MAX32620HSP": {
        "inherits": ["Target"],
        "core": "Cortex-M4F",
        "extra_labels": ["Maxim", "MAX32620"],
        "supported_toolchains": ["GCC_ARM", "IAR", "ARM"],
        "device_has": ["ANALOGIN", "I2C", "INTERRUPTIN", "PORTIN", "PORTINOUT", "PORTOUT", "PWMOUT", "SERIAL", "SERIAL_FC", "SLEEP", "SPI", "SPI_ASYNCH", "STDIO_MESSAGES"],
        "features": ["BLE"],
        "release_versions": []
    },
    "MAX32620FTHR": {
        "inherits": ["Target"],
        "core": "Cortex-M4F",
        "macros": ["__SYSTEM_HFX=96000000","TARGET=MAX32620","TARGET_REV=0x4332","OPEN_DRAIN_LEDS"],
        "extra_labels": ["Maxim", "MAX32620C"],
        "supported_toolchains": ["GCC_ARM", "IAR", "ARM"],
        "device_has": ["ANALOGIN", "I2C", "INTERRUPTIN", "LPTICKER", "PORTIN", "PORTINOUT", "PORTOUT", "PWMOUT", "SERIAL", "SERIAL_FC", "SLEEP", "SPI", "STDIO_MESSAGES", "USTICKER"],
        "release_versions": ["2", "5"]
    },
    "SDT32620B": {
        "inherits": ["Target"],
        "core": "Cortex-M4F",
        "macros": ["__SYSTEM_HFX=96000000","TARGET=MAX32620","TARGET_REV=0x4332","OPEN_DRAIN_LEDS"],
        "detect_code": ["3101"],
        "extra_labels": ["Maxim", "MAX32620C"],
        "supported_toolchains": ["GCC_ARM", "IAR", "ARM"],
        "device_has": ["ANALOGIN", "I2C", "INTERRUPTIN", "LPTICKER", "PORTIN", "PORTINOUT", "PORTOUT", "PWMOUT", "SERIAL", "SERIAL_FC", "SLEEP", "SPI", "STDIO_MESSAGES", "USTICKER"],
        "release_versions": ["2", "5"]
    },
    "MAX32625_BASE": {
        "inherits": ["Target"],
        "core": "Cortex-M4F",
        "macros": ["TARGET=MAX32625","TARGET_REV=0x4132", "OPEN_DRAIN_LEDS"],
        "extra_labels": ["Maxim", "MAX32625"],
        "supported_toolchains": ["GCC_ARM", "IAR", "ARM"],
        "device_has": ["ANALOGIN", "I2C", "INTERRUPTIN", "LPTICKER", "PORTIN", "PORTINOUT", "PORTOUT", "PWMOUT", "RTC", "SERIAL", "SERIAL_FC", "SLEEP", "SPI", "STDIO_MESSAGES", "USTICKER"],
        "device_name": "MAX32625",
        "release_versions": ["2", "5"],
        "public": false
    },
    "MAX32625MBED": {
        "inherits": ["MAX32625_BASE"],
        "extra_labels_add": ["MAX32625_NO_BOOT"]
    },
    "SDT32625B": {
        "inherits": ["MAX32625_BASE"],
        "extra_labels_add": ["MAX32625_NO_BOOT"],
        "detect_code": ["3102"]
    },
    "MAX32625PICO": {
        "inherits": ["MAX32625_BASE"],
        "extra_labels_add": ["MAX32625_BOOT"],
        "bootloader_supported": true
    },
    "MAX32625NEXPAQ": {
        "inherits": ["MAX32625_BASE"]
    },
    "MAX32630FTHR": {
        "inherits": ["Target"],
        "core": "Cortex-M4F",
        "macros": ["__SYSTEM_HFX=96000000", "TARGET=MAX32630", "TARGET_REV=0x4132", "BLE_HCI_UART", "OPEN_DRAIN_LEDS"],
        "extra_labels": ["Maxim", "MAX32630"],
        "supported_toolchains": ["GCC_ARM", "IAR", "ARM"],
        "device_has": ["ANALOGIN", "I2C", "INTERRUPTIN", "LPTICKER", "PORTIN", "PORTINOUT", "PORTOUT", "PWMOUT", "SERIAL", "SERIAL_FC", "SPI", "STDIO_MESSAGES", "USTICKER"],
        "features": ["BLE"],
        "release_versions": ["2", "5"]
    },
    "EFM32": {
        "inherits": ["Target"],
        "extra_labels": ["Silicon_Labs", "EFM32"],
        "macros": ["MBEDTLS_CONFIG_HW_SUPPORT", "MBED_TICKLESS", "EM_MSC_RUN_FROM_FLASH"],
        "public": false
    },
    "EFM32GG990F1024": {
        "inherits": ["EFM32"],
        "extra_labels_add": ["EFM32GG", "1024K", "SL_AES"],
        "core": "Cortex-M3",
        "macros_add": ["EFM32GG990F1024", "TRANSACTION_QUEUE_SIZE_SPI=4"],
        "supported_toolchains": ["GCC_ARM", "ARM", "uARM", "IAR"],
        "release_versions": ["2", "5"],
        "device_name": "EFM32GG990F1024",
        "public": false,
        "bootloader_supported": true
    },
    "EFM32GG_STK3700": {
        "inherits": ["EFM32GG990F1024"],
        "progen": {"target": "efm32gg-stk"},
        "device_has": ["ANALOGIN", "ANALOGOUT", "I2C", "I2CSLAVE", "I2C_ASYNCH", "INTERRUPTIN", "LPTICKER", "PORTIN", "PORTINOUT", "PORTOUT", "PWMOUT", "RTC", "SERIAL", "SERIAL_ASYNCH", "SLEEP", "SPI", "SPISLAVE", "SPI_ASYNCH", "STDIO_MESSAGES", "USTICKER", "FLASH", "ITM"],
        "forced_reset_timeout": 2,
        "config": {
            "hf_clock_src": {
                "help": "Value: HFXO for external crystal, HFRCO for internal RC oscillator",
                "value": "HFXO",
                "macro_name": "CORE_CLOCK_SOURCE"
            },
            "hfxo_clock_freq": {
                "help": "Value: External crystal frequency in hertz",
                "value": "48000000",
                "macro_name": "HFXO_FREQUENCY"
            },
            "lf_clock_src": {
                "help": "Value: LFXO for external crystal, LFRCO for internal RC oscillator, ULFRCO for internal 1KHz RC oscillator",
                "value": "LFXO",
                "macro_name": "LOW_ENERGY_CLOCK_SOURCE"
            },
            "lfxo_clock_freq": {
                "help": "Value: External crystal frequency in hertz",
                "value": "32768",
                "macro_name": "LFXO_FREQUENCY"
            },
            "hfrco_clock_freq": {
                "help": "Value: Frequency in hertz, must correspond to setting of hfrco_band_select",
                "value": "21000000",
                "macro_name": "HFRCO_FREQUENCY"
            },
            "hfrco_band_select": {
                "help": "Value: One of _CMU_HFRCOCTRL_BAND_28MHZ, _CMU_HFRCOCTRL_BAND_21MHZ, _CMU_HFRCOCTRL_BAND_14MHZ, _CMU_HFRCOCTRL_BAND_11MHZ, _CMU_HFRCOCTRL_BAND_7MHZ, _CMU_HFRCOCTRL_BAND_1MHZ. Be sure to set hfrco_clock_freq accordingly!",
                "value": "_CMU_HFRCOCTRL_BAND_21MHZ",
                "macro_name": "HFRCO_FREQUENCY_ENUM"
            },
            "board_controller_enable": {
                "help": "Pin to pull high for enabling the USB serial port",
                "value": "PF7",
                "macro_name": "EFM_BC_EN"
            }
        }
    },
    "EFM32LG990F256": {
        "inherits": ["EFM32"],
        "extra_labels_add": ["EFM32LG", "256K", "SL_AES"],
        "core": "Cortex-M3",
        "macros_add": ["EFM32LG990F256", "TRANSACTION_QUEUE_SIZE_SPI=4"],
        "supported_toolchains": ["GCC_ARM", "ARM", "uARM", "IAR"],
        "release_versions": ["2", "5"],
        "device_name": "EFM32LG990F256",
        "public": false,
        "bootloader_supported": true
    },
    "EFM32LG_STK3600": {
        "inherits": ["EFM32LG990F256"],
        "device_has": ["ANALOGIN", "ANALOGOUT", "I2C", "I2CSLAVE", "I2C_ASYNCH", "INTERRUPTIN", "LPTICKER", "PORTIN", "PORTINOUT", "PORTOUT", "PWMOUT", "RTC", "SERIAL", "SERIAL_ASYNCH", "SLEEP", "SPI", "SPISLAVE", "SPI_ASYNCH", "STDIO_MESSAGES", "USTICKER", "FLASH"],
        "forced_reset_timeout": 2,
        "device_name": "EFM32LG990F256",
        "config": {
            "hf_clock_src": {
                "help": "Value: HFXO for external crystal, HFRCO for internal RC oscillator",
                "value": "HFXO",
                "macro_name": "CORE_CLOCK_SOURCE"
            },
            "hfxo_clock_freq": {
                "help": "Value: External crystal frequency in hertz",
                "value": "48000000",
                "macro_name": "HFXO_FREQUENCY"
            },
            "lf_clock_src": {
                "help": "Value: LFXO for external crystal, LFRCO for internal RC oscillator, ULFRCO for internal 1KHz RC oscillator",
                "value": "LFXO",
                "macro_name": "LOW_ENERGY_CLOCK_SOURCE"
            },
            "lfxo_clock_freq": {
                "help": "Value: External crystal frequency in hertz",
                "value": "32768",
                "macro_name": "LFXO_FREQUENCY"
            },
            "hfrco_clock_freq": {
                "help": "Value: Frequency in hertz, must correspond to setting of hfrco_band_select",
                "value": "21000000",
                "macro_name": "HFRCO_FREQUENCY"
            },
            "hfrco_band_select": {
                "help": "Value: One of _CMU_HFRCOCTRL_BAND_28MHZ, _CMU_HFRCOCTRL_BAND_21MHZ, _CMU_HFRCOCTRL_BAND_14MHZ, _CMU_HFRCOCTRL_BAND_11MHZ, _CMU_HFRCOCTRL_BAND_7MHZ, _CMU_HFRCOCTRL_BAND_1MHZ. Be sure to set hfrco_clock_freq accordingly!",
                "value": "_CMU_HFRCOCTRL_BAND_21MHZ",
                "macro_name": "HFRCO_FREQUENCY_ENUM"
            },
            "board_controller_enable": {
                "help": "Pin to pull high for enabling the USB serial port",
                "value": "PF7",
                "macro_name": "EFM_BC_EN"
            }
        }
    },
    "EFM32WG990F256": {
        "inherits": ["EFM32"],
        "extra_labels_add": ["EFM32WG", "256K", "SL_AES"],
        "core": "Cortex-M4F",
        "macros_add": ["EFM32WG990F256", "TRANSACTION_QUEUE_SIZE_SPI=4"],
        "supported_toolchains": ["GCC_ARM", "ARM", "uARM", "IAR"],
        "release_versions": ["2", "5"],
        "device_name": "EFM32WG990F256",
        "public": false,
        "bootloader_supported": true
    },
    "EFM32WG_STK3800": {
        "inherits": ["EFM32WG990F256"],
        "progen": {"target": "efm32wg-stk"},
        "device_has": ["ANALOGIN", "ANALOGOUT", "I2C", "I2CSLAVE", "I2C_ASYNCH", "INTERRUPTIN", "LPTICKER", "PORTIN", "PORTINOUT", "PORTOUT", "PWMOUT", "RTC", "SERIAL", "SERIAL_ASYNCH", "SLEEP", "SPI", "SPISLAVE", "SPI_ASYNCH", "STDIO_MESSAGES", "USTICKER", "FLASH"],
        "forced_reset_timeout": 2,
        "config": {
            "hf_clock_src": {
                "help": "Value: HFXO for external crystal, HFRCO for internal RC oscillator",
                "value": "HFXO",
                "macro_name": "CORE_CLOCK_SOURCE"
            },
            "hfxo_clock_freq": {
                "help": "Value: External crystal frequency in hertz",
                "value": "48000000",
                "macro_name": "HFXO_FREQUENCY"
            },
            "lf_clock_src": {
                "help": "Value: LFXO for external crystal, LFRCO for internal RC oscillator, ULFRCO for internal 1KHz RC oscillator",
                "value": "LFXO",
                "macro_name": "LOW_ENERGY_CLOCK_SOURCE"
            },
            "lfxo_clock_freq": {
                "help": "Value: External crystal frequency in hertz",
                "value": "32768",
                "macro_name": "LFXO_FREQUENCY"
            },
            "hfrco_clock_freq": {
                "help": "Value: Frequency in hertz, must correspond to setting of hfrco_band_select",
                "value": "21000000",
                "macro_name": "HFRCO_FREQUENCY"
            },
            "hfrco_band_select": {
                "help": "Value: One of _CMU_HFRCOCTRL_BAND_28MHZ, _CMU_HFRCOCTRL_BAND_21MHZ, _CMU_HFRCOCTRL_BAND_14MHZ, _CMU_HFRCOCTRL_BAND_11MHZ, _CMU_HFRCOCTRL_BAND_7MHZ, _CMU_HFRCOCTRL_BAND_1MHZ. Be sure to set hfrco_clock_freq accordingly!",
                "value": "_CMU_HFRCOCTRL_BAND_21MHZ",
                "macro_name": "HFRCO_FREQUENCY_ENUM"
            },
            "board_controller_enable": {
                "help": "Pin to pull high for enabling the USB serial port",
                "value": "PF7",
                "macro_name": "EFM_BC_EN"
            }
        }
    },
    "EFM32ZG222F32": {
        "inherits": ["EFM32"],
        "extra_labels_add": ["EFM32ZG", "32K", "SL_AES"],
        "core": "Cortex-M0+",
        "default_toolchain": "uARM",
        "macros_add": ["EFM32ZG222F32", "TRANSACTION_QUEUE_SIZE_SPI=0"],
        "supported_toolchains": ["GCC_ARM", "uARM", "IAR"],
        "default_lib": "small",
        "release_versions": ["2"],
        "device_name": "EFM32ZG222F32",
        "public": false
    },
    "EFM32ZG_STK3200": {
        "inherits": ["EFM32ZG222F32"],
        "device_has": ["ANALOGIN", "I2C", "I2CSLAVE", "I2C_ASYNCH", "INTERRUPTIN", "LPTICKER", "PORTIN", "PORTINOUT", "PORTOUT", "PWMOUT", "SERIAL", "SERIAL_ASYNCH", "SLEEP", "SPI", "SPISLAVE", "SPI_ASYNCH", "STDIO_MESSAGES", "USTICKER"],
        "forced_reset_timeout": 2,
        "config": {
            "hf_clock_src": {
                "help": "Value: HFXO for external crystal, HFRCO for internal RC oscillator",
                "value": "HFXO",
                "macro_name": "CORE_CLOCK_SOURCE"
            },
            "hfxo_clock_freq": {
                "help": "Value: External crystal frequency in hertz",
                "value": "24000000",
                "macro_name": "HFXO_FREQUENCY"
            },
            "lf_clock_src": {
                "help": "Value: LFXO for external crystal, LFRCO for internal RC oscillator, ULFRCO for internal 1KHz RC oscillator",
                "value": "LFXO",
                "macro_name": "LOW_ENERGY_CLOCK_SOURCE"
            },
            "lfxo_clock_freq": {
                "help": "Value: External crystal frequency in hertz",
                "value": "32768",
                "macro_name": "LFXO_FREQUENCY"
            },
            "hfrco_clock_freq": {
                "help": "Value: Frequency in hertz, must correspond to setting of hfrco_band_select",
                "value": "21000000",
                "macro_name": "HFRCO_FREQUENCY"
            },
            "hfrco_band_select": {
                "help": "Value: One of _CMU_HFRCOCTRL_BAND_21MHZ, _CMU_HFRCOCTRL_BAND_14MHZ, _CMU_HFRCOCTRL_BAND_11MHZ, _CMU_HFRCOCTRL_BAND_7MHZ, _CMU_HFRCOCTRL_BAND_1MHZ. Be sure to set hfrco_clock_freq accordingly!",
                "value": "_CMU_HFRCOCTRL_BAND_21MHZ",
                "macro_name": "HFRCO_FREQUENCY_ENUM"
            },
            "board_controller_enable": {
                "help": "Pin to pull high for enabling the USB serial port",
                "value": "PA9",
                "macro_name": "EFM_BC_EN"
            }
        }
    },
    "EFM32HG322F64": {
        "inherits": ["EFM32"],
        "extra_labels_add": ["EFM32HG", "64K", "SL_AES"],
        "core": "Cortex-M0+",
        "default_toolchain": "uARM",
        "macros_add": ["EFM32HG322F64", "TRANSACTION_QUEUE_SIZE_SPI=0"],
        "supported_toolchains": ["GCC_ARM", "uARM", "IAR"],
        "default_lib": "small",
        "release_versions": ["2"],
        "device_name": "EFM32HG322F64",
        "public": false
    },
    "EFM32HG_STK3400": {
        "inherits": ["EFM32HG322F64"],
        "device_has": ["ANALOGIN", "I2C", "I2CSLAVE", "I2C_ASYNCH", "INTERRUPTIN", "LPTICKER", "PORTIN", "PORTINOUT", "PORTOUT", "PWMOUT", "SERIAL", "SERIAL_ASYNCH", "SLEEP", "SPI", "SPISLAVE", "SPI_ASYNCH", "STDIO_MESSAGES", "USTICKER"],
        "forced_reset_timeout": 2,
        "config": {
            "hf_clock_src": {
                "help": "Value: HFXO for external crystal, HFRCO for internal RC oscillator",
                "value": "HFXO",
                "macro_name": "CORE_CLOCK_SOURCE"
            },
            "hfxo_clock_freq": {
                "help": "Value: External crystal frequency in hertz",
                "value": "24000000",
                "macro_name": "HFXO_FREQUENCY"
            },
            "lf_clock_src": {
                "help": "Value: LFXO for external crystal, LFRCO for internal RC oscillator, ULFRCO for internal 1KHz RC oscillator",
                "value": "LFXO",
                "macro_name": "LOW_ENERGY_CLOCK_SOURCE"
            },
            "lfxo_clock_freq": {
                "help": "Value: External crystal frequency in hertz",
                "value": "32768",
                "macro_name": "LFXO_FREQUENCY"
            },
            "hfrco_clock_freq": {
                "help": "Value: Frequency in hertz, must correspond to setting of hfrco_band_select",
                "value": "21000000",
                "macro_name": "HFRCO_FREQUENCY"
            },
            "hfrco_band_select": {
                "help": "Value: One of _CMU_HFRCOCTRL_BAND_21MHZ, _CMU_HFRCOCTRL_BAND_14MHZ, _CMU_HFRCOCTRL_BAND_11MHZ, _CMU_HFRCOCTRL_BAND_7MHZ, _CMU_HFRCOCTRL_BAND_1MHZ. Be sure to set hfrco_clock_freq accordingly!",
                "value": "_CMU_HFRCOCTRL_BAND_21MHZ",
                "macro_name": "HFRCO_FREQUENCY_ENUM"
            },
            "board_controller_enable": {
                "help": "Pin to pull high for enabling the USB serial port",
                "value": "PA9",
                "macro_name": "EFM_BC_EN"
            }
        }
    },
    "EFM32PG1B100F256GM32": {
        "inherits": ["EFM32"],
        "extra_labels_add": ["EFM32PG", "256K", "SL_CRYPTO"],
        "core": "Cortex-M4F",
        "macros_add": ["EFM32PG1B100F256GM32", "TRANSACTION_QUEUE_SIZE_SPI=4"],
        "supported_toolchains": ["GCC_ARM", "ARM", "uARM", "IAR"],
        "release_versions": ["2", "5"],
        "device_name": "EFM32PG1B100F256GM32",
        "public": false,
        "bootloader_supported": true
    },
    "EFM32PG_STK3401": {
        "inherits": ["EFM32PG1B100F256GM32"],
        "device_has": ["ANALOGIN", "CRC", "I2C", "I2CSLAVE", "I2C_ASYNCH", "INTERRUPTIN", "LPTICKER", "PORTIN", "PORTINOUT", "PORTOUT", "PWMOUT", "RTC", "SERIAL", "SERIAL_ASYNCH", "SLEEP", "SPI", "SPISLAVE", "SPI_ASYNCH", "STDIO_MESSAGES", "USTICKER", "FLASH"],
        "forced_reset_timeout": 2,
        "config": {
            "hf_clock_src": {
                "help": "Value: HFXO for external crystal, HFRCO for internal RC oscillator",
                "value": "HFXO",
                "macro_name": "CORE_CLOCK_SOURCE"
            },
            "hfxo_clock_freq": {
                "help": "Value: External crystal frequency in hertz",
                "value": "40000000",
                "macro_name": "HFXO_FREQUENCY"
            },
            "lf_clock_src": {
                "help": "Value: LFXO for external crystal, LFRCO for internal RC oscillator, ULFRCO for internal 1KHz RC oscillator",
                "value": "LFXO",
                "macro_name": "LOW_ENERGY_CLOCK_SOURCE"
            },
            "lfxo_clock_freq": {
                "help": "Value: External crystal frequency in hertz",
                "value": "32768",
                "macro_name": "LFXO_FREQUENCY"
            },
            "hfrco_clock_freq": {
                "help": "Value: Frequency in hertz, must correspond to setting of hfrco_band_select",
                "value": "32000000",
                "macro_name": "HFRCO_FREQUENCY"
            },
            "hfrco_band_select": {
                "help": "Value: One of cmuHFRCOFreq_1M0Hz, cmuHFRCOFreq_2M0Hz, cmuHFRCOFreq_4M0Hz, cmuHFRCOFreq_7M0Hz, cmuHFRCOFreq_13M0Hz, cmuHFRCOFreq_16M0Hz, cmuHFRCOFreq_19M0Hz, cmuHFRCOFreq_26M0Hz, cmuHFRCOFreq_32M0Hz, cmuHFRCOFreq_38M0Hz. Be sure to set hfrco_clock_freq accordingly!",
                "value": "cmuHFRCOFreq_32M0Hz",
                "macro_name": "HFRCO_FREQUENCY_ENUM"
            },
            "board_controller_enable": {
                "help": "Pin to pull high for enabling the USB serial port",
                "value": "PA5",
                "macro_name": "EFM_BC_EN"
            }
        }
    },
    "EFR32MG1P132F256GM48": {
        "inherits": ["EFM32"],
        "extra_labels_add": ["EFR32MG1", "EFR32_1", "256K", "SL_RAIL", "SL_CRYPTO"],
        "core": "Cortex-M4F",
        "macros_add": ["EFR32MG1P132F256GM48", "TRANSACTION_QUEUE_SIZE_SPI=4"],
        "supported_toolchains": ["GCC_ARM", "ARM", "uARM", "IAR"],
        "release_versions": ["2", "5"],
        "device_name": "EFR32MG1P132F256GM48",
        "public": false,
        "bootloader_supported": true
    },
    "EFR32MG1P233F256GM48": {
        "inherits": ["EFM32"],
        "extra_labels_add": ["EFR32MG1", "EFR32_1", "256K", "SL_RAIL", "SL_CRYPTO"],
        "core": "Cortex-M4F",
        "macros_add": ["EFR32MG1P233F256GM48", "TRANSACTION_QUEUE_SIZE_SPI=4"],
        "supported_toolchains": ["GCC_ARM", "ARM", "uARM", "IAR"],
        "release_versions": ["2", "5"],
        "public": false,
        "bootloader_supported": true
    },
    "EFR32MG1_BRD4150": {
        "inherits": ["EFR32MG1P132F256GM48"],
        "device_has": ["802_15_4_PHY", "ANALOGIN", "CRC", "I2C", "I2CSLAVE", "I2C_ASYNCH", "INTERRUPTIN", "LPTICKER", "PORTIN", "PORTINOUT", "PORTOUT", "PWMOUT", "RTC", "SERIAL", "SERIAL_ASYNCH", "SLEEP", "SPI", "SPISLAVE", "SPI_ASYNCH", "STDIO_MESSAGES", "USTICKER", "FLASH"],
        "forced_reset_timeout": 2,
        "config": {
            "hf_clock_src": {
                "help": "Value: HFXO for external crystal, HFRCO for internal RC oscillator",
                "value": "HFXO",
                "macro_name": "CORE_CLOCK_SOURCE"
            },
            "hfxo_clock_freq": {
                "help": "Value: External crystal frequency in hertz",
                "value": "38400000",
                "macro_name": "HFXO_FREQUENCY"
            },
            "lf_clock_src": {
                "help": "Value: LFXO for external crystal, LFRCO for internal RC oscillator, ULFRCO for internal 1KHz RC oscillator",
                "value": "LFXO",
                "macro_name": "LOW_ENERGY_CLOCK_SOURCE"
            },
            "lfxo_clock_freq": {
                "help": "Value: External crystal frequency in hertz",
                "value": "32768",
                "macro_name": "LFXO_FREQUENCY"
            },
            "hfrco_clock_freq": {
                "help": "Value: Frequency in hertz, must correspond to setting of hfrco_band_select",
                "value": "32000000",
                "macro_name": "HFRCO_FREQUENCY"
            },
            "hfrco_band_select": {
                "help": "Value: One of cmuHFRCOFreq_1M0Hz, cmuHFRCOFreq_2M0Hz, cmuHFRCOFreq_4M0Hz, cmuHFRCOFreq_7M0Hz, cmuHFRCOFreq_13M0Hz, cmuHFRCOFreq_16M0Hz, cmuHFRCOFreq_19M0Hz, cmuHFRCOFreq_26M0Hz, cmuHFRCOFreq_32M0Hz, cmuHFRCOFreq_38M0Hz. Be sure to set hfrco_clock_freq accordingly!",
                "value": "cmuHFRCOFreq_32M0Hz",
                "macro_name": "HFRCO_FREQUENCY_ENUM"
            },
            "board_controller_enable": {
                "help": "Pin to pull high for enabling the USB serial port",
                "value": "PA5",
                "macro_name": "EFM_BC_EN"
            }
        },
        "overrides": {
            "network-default-interface-type": "MESH"
        },
        "public": false
    },
    "TB_SENSE_1": {
        "inherits": ["EFR32MG1P233F256GM48"],
        "device_has": ["802_15_4_PHY", "ANALOGIN", "CRC", "I2C", "I2CSLAVE", "I2C_ASYNCH", "INTERRUPTIN", "LPTICKER", "PORTIN", "PORTINOUT", "PORTOUT", "PWMOUT", "RTC", "SERIAL", "SERIAL_ASYNCH", "SLEEP", "SPI", "SPISLAVE", "SPI_ASYNCH", "STDIO_MESSAGES", "USTICKER", "FLASH"],
        "forced_reset_timeout": 5,
        "config": {
            "hf_clock_src": {
                "help": "Value: HFXO for external crystal, HFRCO for internal RC oscillator",
                "value": "HFXO",
                "macro_name": "CORE_CLOCK_SOURCE"
            },
            "hfxo_clock_freq": {
                "help": "Value: External crystal frequency in hertz",
                "value": "38400000",
                "macro_name": "HFXO_FREQUENCY"
            },
            "lf_clock_src": {
                "help": "Value: LFXO for external crystal, LFRCO for internal RC oscillator, ULFRCO for internal 1KHz RC oscillator",
                "value": "LFXO",
                "macro_name": "LOW_ENERGY_CLOCK_SOURCE"
            },
            "lfxo_clock_freq": {
                "help": "Value: External crystal frequency in hertz",
                "value": "32768",
                "macro_name": "LFXO_FREQUENCY"
            },
            "hfrco_clock_freq": {
                "help": "Value: Frequency in hertz, must correspond to setting of hfrco_band_select",
                "value": "32000000",
                "macro_name": "HFRCO_FREQUENCY"
            },
            "hfrco_band_select": {
                "help": "Value: One of cmuHFRCOFreq_1M0Hz, cmuHFRCOFreq_2M0Hz, cmuHFRCOFreq_4M0Hz, cmuHFRCOFreq_7M0Hz, cmuHFRCOFreq_13M0Hz, cmuHFRCOFreq_16M0Hz, cmuHFRCOFreq_19M0Hz, cmuHFRCOFreq_26M0Hz, cmuHFRCOFreq_32M0Hz, cmuHFRCOFreq_38M0Hz. Be sure to set hfrco_clock_freq accordingly!",
                "value": "cmuHFRCOFreq_32M0Hz",
                "macro_name": "HFRCO_FREQUENCY_ENUM"
            }
        },
        "overrides": {
            "network-default-interface-type": "MESH"
        }
    },
    "EFM32PG12B500F1024GL125": {
        "inherits": ["EFM32"],
        "extra_labels_add": ["EFM32PG12", "1024K", "SL_CRYPTO"],
        "core": "Cortex-M4F",
        "macros_add": ["EFM32PG12B500F1024GL125", "TRANSACTION_QUEUE_SIZE_SPI=4"],
        "supported_toolchains": ["GCC_ARM", "ARM", "uARM", "IAR"],
        "release_versions": ["2", "5"],
        "device_name": "EFM32PG12B500F1024GL125",
        "public": false,
        "bootloader_supported": true
    },
    "EFM32PG12_STK3402": {
        "inherits": ["EFM32PG12B500F1024GL125"],
        "device_has": ["ANALOGIN", "CRC", "I2C", "I2CSLAVE", "I2C_ASYNCH", "INTERRUPTIN", "LPTICKER", "PORTIN", "PORTINOUT", "PORTOUT", "PWMOUT", "RTC", "SERIAL", "SERIAL_ASYNCH", "SLEEP", "SPI", "SPISLAVE", "SPI_ASYNCH", "STDIO_MESSAGES", "USTICKER", "TRNG", "FLASH"],
        "forced_reset_timeout": 2,
        "config": {
            "hf_clock_src": {
                "help": "Value: HFXO for external crystal, HFRCO for internal RC oscillator",
                "value": "HFXO",
                "macro_name": "CORE_CLOCK_SOURCE"
            },
            "hfxo_clock_freq": {
                "help": "Value: External crystal frequency in hertz",
                "value": "40000000",
                "macro_name": "HFXO_FREQUENCY"
            },
            "lf_clock_src": {
                "help": "Value: LFXO for external crystal, LFRCO for internal RC oscillator, ULFRCO for internal 1KHz RC oscillator",
                "value": "LFXO",
                "macro_name": "LOW_ENERGY_CLOCK_SOURCE"
            },
            "lfxo_clock_freq": {
                "help": "Value: External crystal frequency in hertz",
                "value": "32768",
                "macro_name": "LFXO_FREQUENCY"
            },
            "hfrco_clock_freq": {
                "help": "Value: Frequency in hertz, must correspond to setting of hfrco_band_select",
                "value": "32000000",
                "macro_name": "HFRCO_FREQUENCY"
            },
            "hfrco_band_select": {
                "help": "Value: One of cmuHFRCOFreq_1M0Hz, cmuHFRCOFreq_2M0Hz, cmuHFRCOFreq_4M0Hz, cmuHFRCOFreq_7M0Hz, cmuHFRCOFreq_13M0Hz, cmuHFRCOFreq_16M0Hz, cmuHFRCOFreq_19M0Hz, cmuHFRCOFreq_26M0Hz, cmuHFRCOFreq_32M0Hz, cmuHFRCOFreq_38M0Hz. Be sure to set hfrco_clock_freq accordingly!",
                "value": "cmuHFRCOFreq_32M0Hz",
                "macro_name": "HFRCO_FREQUENCY_ENUM"
            },
            "board_controller_enable": {
                "help": "Pin to pull high for enabling the USB serial port",
                "value": "PA5",
                "macro_name": "EFM_BC_EN"
            }
        }
    },
    "EFR32MG12P332F1024GL125": {
        "inherits": ["EFM32"],
        "extra_labels_add": ["EFR32MG12", "EFR32_12", "1024K", "SL_RAIL", "SL_CRYPTO"],
        "core": "Cortex-M4F",
        "macros_add": ["EFR32MG12P332F1024GL125", "TRANSACTION_QUEUE_SIZE_SPI=4"],
        "supported_toolchains": ["GCC_ARM", "ARM", "uARM", "IAR"],
        "release_versions": ["2", "5"],
        "device_name": "EFR32MG12P332F1024GL125",
        "public": false,
        "bootloader_supported": true
    },
    "TB_SENSE_12": {
        "inherits": ["EFR32MG12P332F1024GL125"],
        "device_name": "EFR32MG12P332F1024GL125",
        "device_has": ["802_15_4_PHY", "ANALOGIN", "CRC", "I2C", "I2CSLAVE", "I2C_ASYNCH", "INTERRUPTIN", "LPTICKER", "PORTIN", "PORTINOUT", "PORTOUT", "PWMOUT", "RTC", "SERIAL", "SERIAL_ASYNCH", "SLEEP", "SPI", "SPISLAVE", "SPI_ASYNCH", "STDIO_MESSAGES", "USTICKER", "TRNG", "FLASH"],
        "forced_reset_timeout": 5,
        "config": {
            "hf_clock_src": {
                "help": "Value: HFXO for external crystal, HFRCO for internal RC oscillator",
                "value": "HFXO",
                "macro_name": "CORE_CLOCK_SOURCE"
            },
            "hfxo_clock_freq": {
                "help": "Value: External crystal frequency in hertz",
                "value": "38400000",
                "macro_name": "HFXO_FREQUENCY"
            },
            "lf_clock_src": {
                "help": "Value: LFXO for external crystal, LFRCO for internal RC oscillator, ULFRCO for internal 1KHz RC oscillator",
                "value": "LFXO",
                "macro_name": "LOW_ENERGY_CLOCK_SOURCE"
            },
            "lfxo_clock_freq": {
                "help": "Value: External crystal frequency in hertz",
                "value": "32768",
                "macro_name": "LFXO_FREQUENCY"
            },
            "hfrco_clock_freq": {
                "help": "Value: Frequency in hertz, must correspond to setting of hfrco_band_select",
                "value": "32000000",
                "macro_name": "HFRCO_FREQUENCY"
            },
            "hfrco_band_select": {
                "help": "Value: One of cmuHFRCOFreq_1M0Hz, cmuHFRCOFreq_2M0Hz, cmuHFRCOFreq_4M0Hz, cmuHFRCOFreq_7M0Hz, cmuHFRCOFreq_13M0Hz, cmuHFRCOFreq_16M0Hz, cmuHFRCOFreq_19M0Hz, cmuHFRCOFreq_26M0Hz, cmuHFRCOFreq_32M0Hz, cmuHFRCOFreq_38M0Hz. Be sure to set hfrco_clock_freq accordingly!",
                "value": "cmuHFRCOFreq_32M0Hz",
                "macro_name": "HFRCO_FREQUENCY_ENUM"
            }
        },
        "overrides": {
            "network-default-interface-type": "MESH"
        }
    },
    "EFM32GG11B820F2048GL192": {
        "inherits": ["EFM32"],
        "extra_labels_add": ["EFM32GG11", "2048K", "SL_CRYPTO"],
        "core": "Cortex-M4F",
        "macros_add": ["EFM32GG11B820F2048GL192", "TRANSACTION_QUEUE_SIZE_SPI=4"],
        "supported_toolchains": ["GCC_ARM", "ARM", "uARM", "IAR"],
        "release_versions": ["2", "5"],
        "device_name": "EFM32GG11B820F2048GL192",
        "public": false,
        "bootloader_supported": true
    },
    "EFM32GG11_STK3701": {
        "inherits": ["EFM32GG11B820F2048GL192"],
        "device_name": "EFM32GG11B820F2048GL192",
        "device_has": ["ANALOGIN", "CRC", "EMAC", "I2C", "I2CSLAVE", "I2C_ASYNCH", "INTERRUPTIN", "LPTICKER", "PORTIN", "PORTINOUT", "PORTOUT", "PWMOUT", "QSPI", "RTC", "SERIAL", "SERIAL_ASYNCH", "SLEEP", "SPI", "SPISLAVE", "SPI_ASYNCH", "STDIO_MESSAGES", "USTICKER", "TRNG", "FLASH"],
        "forced_reset_timeout": 5,
        "config": {
            "hf_clock_src": {
                "help": "Value: HFXO for external crystal, HFRCO for internal RC oscillator",
                "value": "HFXO",
                "macro_name": "CORE_CLOCK_SOURCE"
            },
            "hfxo_clock_freq": {
                "help": "Value: External crystal frequency in hertz",
                "value": "50000000",
                "macro_name": "HFXO_FREQUENCY"
            },
            "lf_clock_src": {
                "help": "Value: LFXO for external crystal, LFRCO for internal RC oscillator, ULFRCO for internal 1KHz RC oscillator",
                "value": "LFXO",
                "macro_name": "LOW_ENERGY_CLOCK_SOURCE"
            },
            "lfxo_clock_freq": {
                "help": "Value: External crystal frequency in hertz",
                "value": "32768",
                "macro_name": "LFXO_FREQUENCY"
            },
            "hfrco_clock_freq": {
                "help": "Value: Frequency in hertz, must correspond to setting of hfrco_band_select",
                "value": "32000000",
                "macro_name": "HFRCO_FREQUENCY"
            },
            "hfrco_band_select": {
                "help": "Value: One of cmuHFRCOFreq_1M0Hz, cmuHFRCOFreq_2M0Hz, cmuHFRCOFreq_4M0Hz, cmuHFRCOFreq_7M0Hz, cmuHFRCOFreq_13M0Hz, cmuHFRCOFreq_16M0Hz, cmuHFRCOFreq_19M0Hz, cmuHFRCOFreq_26M0Hz, cmuHFRCOFreq_32M0Hz, cmuHFRCOFreq_38M0Hz. Be sure to set hfrco_clock_freq accordingly!",
                "value": "cmuHFRCOFreq_32M0Hz",
                "macro_name": "HFRCO_FREQUENCY_ENUM"
            },
            "board_controller_enable": {
                "help": "Pin to pull high for enabling the USB serial port",
                "value": "PE1",
                "macro_name": "EFM_BC_EN"
            },
            "qspi_flash_enable": {
                "help": "Pin to pull high for enabling the on-board QSPI flash",
                "value": "PG13",
                "macro_name": "QSPI_FLASH_EN"
            }
        },
        "overrides": {
            "network-default-interface-type": "ETHERNET"
        }
    },
    "WIZWIKI_W7500": {
        "supported_form_factors": ["ARDUINO"],
        "core": "Cortex-M0",
        "extra_labels": ["WIZNET", "W7500x", "WIZwiki_W7500"],
        "macros": ["CMSIS_VECTAB_VIRTUAL", "CMSIS_VECTAB_VIRTUAL_HEADER_FILE=\"cmsis_nvic.h\""],
        "supported_toolchains": ["uARM", "ARM", "GCC_ARM", "IAR"],
        "inherits": ["Target"],
        "device_has": ["ANALOGIN", "I2C", "INTERRUPTIN", "PORTIN", "PORTINOUT", "PORTOUT", "PWMOUT", "SERIAL", "SPI", "SPISLAVE", "STDIO_MESSAGES"],
        "release_versions": ["2", "5"]
    },
    "WIZWIKI_W7500P": {
        "supported_form_factors": ["ARDUINO"],
        "core": "Cortex-M0",
        "extra_labels": ["WIZNET", "W7500x", "WIZwiki_W7500P"],
        "macros": ["CMSIS_VECTAB_VIRTUAL", "CMSIS_VECTAB_VIRTUAL_HEADER_FILE=\"cmsis_nvic.h\""],
        "supported_toolchains": ["uARM", "ARM", "GCC_ARM", "IAR"],
        "inherits": ["Target"],
        "device_has": ["ANALOGIN", "I2C", "INTERRUPTIN", "PORTIN", "PORTINOUT", "PORTOUT", "PWMOUT", "SERIAL", "SPI", "SPISLAVE", "STDIO_MESSAGES"],
        "release_versions": ["2", "5"]
    },
    "WIZWIKI_W7500ECO": {
        "inherits": ["Target"],
        "core": "Cortex-M0",
        "extra_labels": ["WIZNET", "W7500x", "WIZwiki_W7500ECO"],
        "macros": ["CMSIS_VECTAB_VIRTUAL", "CMSIS_VECTAB_VIRTUAL_HEADER_FILE=\"cmsis_nvic.h\""],
        "supported_toolchains": ["uARM", "ARM", "GCC_ARM", "IAR"],
        "device_has": ["ANALOGIN", "I2C", "INTERRUPTIN", "PORTIN", "PORTINOUT", "PORTOUT", "PWMOUT", "SERIAL", "SPI", "SPISLAVE", "STDIO_MESSAGES"],
        "release_versions": ["2", "5"]
    },
    "SAMR21G18A": {
        "inherits": ["Target"],
        "core": "Cortex-M0+",
        "macros": ["__SAMR21G18A__", "I2C_MASTER_CALLBACK_MODE=true", "EXTINT_CALLBACK_MODE=true", "USART_CALLBACK_MODE=true", "TC_ASYNC=true"],
        "extra_labels": ["Atmel", "SAM_CortexM0P", "SAMR21"],
        "supported_toolchains": ["GCC_ARM", "ARM", "uARM"],
        "device_has": ["ANALOGIN", "I2C", "I2CSLAVE", "I2C_ASYNCH", "INTERRUPTIN", "PORTIN", "PORTINOUT", "PORTOUT", "PWMOUT", "SERIAL", "SERIAL_ASYNCH", "SERIAL_FC", "SLEEP", "SPI", "SPISLAVE", "SPI_ASYNCH"],
        "release_versions": ["2"],
        "device_name": "ATSAMR21G18A"
    },
    "SAMD21J18A": {
        "inherits": ["Target"],
        "core": "Cortex-M0+",
        "macros": ["__SAMD21J18A__", "I2C_MASTER_CALLBACK_MODE=true", "EXTINT_CALLBACK_MODE=true", "USART_CALLBACK_MODE=true", "TC_ASYNC=true"],
        "extra_labels": ["Atmel", "SAM_CortexM0P", "SAMD21"],
        "supported_toolchains": ["GCC_ARM", "ARM", "uARM"],
        "device_has": ["ANALOGIN", "ANALOGOUT", "I2C", "I2CSLAVE", "I2C_ASYNCH", "INTERRUPTIN", "PORTIN", "PORTINOUT", "PORTOUT", "PWMOUT", "SERIAL", "SERIAL_ASYNCH", "SERIAL_FC", "SLEEP", "SPI", "SPISLAVE", "SPI_ASYNCH"],
        "release_versions": ["2"],
        "device_name": "ATSAMD21J18A"
    },
    "SAMD21G18A": {
        "inherits": ["Target"],
        "core": "Cortex-M0+",
        "macros": ["__SAMD21G18A__", "I2C_MASTER_CALLBACK_MODE=true", "EXTINT_CALLBACK_MODE=true", "USART_CALLBACK_MODE=true", "TC_ASYNC=true"],
        "extra_labels": ["Atmel", "SAM_CortexM0P", "SAMD21"],
        "supported_toolchains": ["GCC_ARM", "ARM", "uARM"],
        "device_has": ["ANALOGIN", "ANALOGOUT", "I2C", "I2CSLAVE", "I2C_ASYNCH", "INTERRUPTIN", "PORTIN", "PORTINOUT", "PORTOUT", "PWMOUT", "SERIAL", "SERIAL_ASYNCH", "SERIAL_FC", "SLEEP", "SPI", "SPISLAVE", "SPI_ASYNCH"],
        "release_versions": ["2"],
        "device_name": "ATSAMD21G18A"
    },
    "SAML21J18A": {
        "inherits": ["Target"],
        "core": "Cortex-M0+",
        "macros": ["__SAML21J18A__", "I2C_MASTER_CALLBACK_MODE=true", "EXTINT_CALLBACK_MODE=true", "USART_CALLBACK_MODE=true", "TC_ASYNC=true"],
        "extra_labels": ["Atmel", "SAM_CortexM0P", "SAML21"],
        "supported_toolchains": ["GCC_ARM", "ARM", "uARM"],
        "device_has": ["ANALOGIN", "ANALOGOUT", "I2C", "I2CSLAVE", "I2C_ASYNCH", "INTERRUPTIN", "PORTIN", "PORTINOUT", "PORTOUT", "PWMOUT", "SERIAL", "SERIAL_ASYNCH", "SERIAL_FC", "SLEEP", "SPI", "SPISLAVE", "SPI_ASYNCH"],
        "device_name": "ATSAML21J18A"
    },
    "SAMG55J19": {
        "inherits": ["Target"],
        "core": "Cortex-M4",
        "extra_labels": ["Atmel", "SAM_CortexM4", "SAMG55"],
        "macros": ["__SAMG55J19__", "BOARD=75", "I2C_MASTER_CALLBACK_MODE=true", "EXTINT_CALLBACK_MODE=true", "USART_CALLBACK_MODE=true", "TC_ASYNC=true"],
        "supported_toolchains": ["GCC_ARM", "ARM", "uARM"],
        "default_toolchain": "ARM",
        "device_has": ["ANALOGIN", "I2C", "I2CSLAVE", "I2C_ASYNCH", "INTERRUPTIN", "PORTIN", "PORTINOUT", "PORTOUT", "PWMOUT", "SERIAL", "SERIAL_ASYNCH", "SERIAL_FC", "SLEEP", "SPI", "SPISLAVE", "SPI_ASYNCH"],
        "default_lib": "std",
        "device_name": "ATSAMG55J19"
    },
    "MCU_NRF51_UNIFIED": {
        "inherits": ["Target"],
        "core": "Cortex-M0",
        "OVERRIDE_BOOTLOADER_FILENAME": "nrf51822_bootloader.hex",
        "macros": [
            "NRF51",
            "TARGET_NRF51822",
            "BLE_STACK_SUPPORT_REQD",
            "SOFTDEVICE_PRESENT",
            "S130",
            "TARGET_MCU_NRF51822",
            "CMSIS_VECTAB_VIRTUAL",
            "CMSIS_VECTAB_VIRTUAL_HEADER_FILE=\"cmsis_nvic.h\"",
            "NO_SYSTICK",
            "MBED_TICKLESS"
        ],
        "MERGE_BOOTLOADER": false,
        "extra_labels": [
            "NORDIC",
            "MCU_NRF51",
            "MCU_NRF51822_UNIFIED",
            "NRF5x",
            "NRF51",
            "SDK_11"
        ],
        "OUTPUT_EXT": "hex",
        "is_disk_virtual": true,
        "supported_toolchains": ["ARM", "GCC_ARM", "IAR"],
        "public": false,
        "MERGE_SOFT_DEVICE": true,
        "EXPECTED_SOFTDEVICES_WITH_OFFSETS": [
            {
                "boot": "",
                "name": "s130_nrf51_2.0.0_softdevice.hex",
                "offset": 110592
            }
        ],
        "detect_code": ["1070"],
        "post_binary_hook": {
            "function": "MCU_NRF51Code.binary_hook",
            "toolchains": ["ARM_STD", "GCC_ARM", "IAR"]
        },
        "program_cycle_s": 6,
        "features": ["BLE"],
        "config": {
            "lf_clock_src": {
                "value": "NRF_LF_SRC_XTAL",
                "macro_name": "MBED_CONF_NORDIC_NRF_LF_CLOCK_SRC"
            },
            "uart_hwfc": {
                "help": "Value: 1 for enable, 0 for disable",
                "value": 1,
                "macro_name": "MBED_CONF_NORDIC_UART_HWFC"
            }
        },
        "device_has": ["ANALOGIN", "I2C", "INTERRUPTIN", "PORTIN", "PORTINOUT", "PORTOUT", "PWMOUT", "SERIAL", "SLEEP", "SPI", "SPISLAVE"]
    },
    "MCU_NRF51_16K_UNIFIED_S130": {
        "inherits": ["MCU_NRF51_UNIFIED"],
        "extra_labels_add": ["MCU_NORDIC_16K", "MCU_NRF51_16K_S130", "MCU_NRF51_16K"],
        "macros_add": ["TARGET_MCU_NORDIC_16K", "TARGET_MCU_NRF51_16K_S130", "TARGET_MCU_NRF51_16K"],
        "public": false
    },
    "MCU_NRF51_32K_UNIFIED": {
        "inherits": ["MCU_NRF51_UNIFIED"],
        "extra_labels_add": ["MCU_NORDIC_32K", "MCU_NRF51_32K"],
        "macros_add": ["TARGET_MCU_NORDIC_32K", "TARGET_MCU_NRF51_32K"],
        "public": false
    },
    "NRF51_DK": {
        "supported_form_factors": ["ARDUINO"],
        "inherits": ["MCU_NRF51_32K_UNIFIED"],
        "device_has": ["USTICKER", "LPTICKER", "ANALOGIN", "I2C", "I2C_ASYNCH", "INTERRUPTIN", "PORTIN", "PORTINOUT", "PORTOUT", "PWMOUT", "SERIAL", "SERIAL_ASYNCH", "SERIAL_FC", "SLEEP", "SPI", "SPI_ASYNCH", "SPISLAVE"],
        "release_versions": ["2", "5"],
        "device_name": "nRF51822_xxAA"
    },
    "SDT51822B": {
        "inherits": ["MCU_NRF51_32K_UNIFIED"],
        "device_has": ["USTICKER", "LPTICKER", "ANALOGIN", "I2C", "I2C_ASYNCH", "INTERRUPTIN", "PORTIN", "PORTINOUT", "PORTOUT", "PWMOUT", "SERIAL", "SERIAL_ASYNCH", "SERIAL_FC", "SLEEP", "SPI", "SPI_ASYNCH", "SPISLAVE"],
        "detect_code": ["3103"],
        "release_versions": ["2", "5"],
        "device_name": "nRF51822_xxAA"
    },
    "NRF51_DONGLE": {
        "inherits": ["MCU_NRF51_32K_UNIFIED"],
        "progen": {"target": "nrf51-dongle"},
        "device_has": ["USTICKER", "LPTICKER", "I2C", "I2C_ASYNCH", "INTERRUPTIN", "PORTIN", "PORTINOUT", "PORTOUT", "PWMOUT", "SERIAL", "SERIAL_ASYNCH", "SLEEP", "SPI", "SPI_ASYNCH", "SPISLAVE"],
        "release_versions": ["2", "5"]
    },
    "OSHCHIP": {
        "inherits": ["MCU_NRF51_32K_UNIFIED"],
        "overrides": {"lf_clock_src": "NRF_LF_SRC_RC"},
        "device_has": ["USTICKER", "LPTICKER", "ANALOGIN", "I2C", "I2C_ASYNCH", "INTERRUPTIN", "PORTIN", "PORTINOUT", "PORTOUT", "PWMOUT", "SERIAL", "SLEEP", "SPI", "SPISLAVE"],
        "device_name": "nRF51822_xxAC"
    },
    "MCU_NRF52832": {
        "inherits": ["Target"],
        "core": "Cortex-M4F",
        "macros": [
            "BOARD_PCA10040",
            "NRF52",
            "TARGET_NRF52832",
            "CMSIS_VECTAB_VIRTUAL",
            "CMSIS_VECTAB_VIRTUAL_HEADER_FILE=\"cmsis_nvic.h\"",
            "MBED_TICKLESS"
        ],
        "device_has": [
            "ANALOGIN",
            "FLASH",
            "I2C",
            "I2C_ASYNCH",
            "INTERRUPTIN",
            "ITM",
            "LPTICKER",
            "PORTIN",
            "PORTINOUT",
            "PORTOUT",
            "PWMOUT",
            "SERIAL",
            "SERIAL_ASYNCH",
            "SERIAL_FC",
            "SLEEP",
            "SPI",
            "SPI_ASYNCH",
            "SYSTICK_CLK_OFF_DURING_SLEEP",
            "TRNG",
            "USTICKER"
        ],
        "extra_labels": [
            "NORDIC",
            "NRF5x",
            "NRF52",
            "SDK_14_2",
            "SOFTDEVICE_COMMON",
            "SOFTDEVICE_S132_FULL"
        ],
        "config": {
            "lf_clock_src": {
                "macro_name": "MBED_CONF_NORDIC_NRF_LF_CLOCK_SRC",
                "help": "Select Low Frequency clock source. Options: NRF_LF_SRC_XTAL, NRF_LF_SRC_SYNTH, and NRF_LF_SRC_RC",
                "value": "NRF_LF_SRC_XTAL"
            },
            "lf_clock_rc_calib_timer_interval": {
                "macro_name": "MBED_CONF_NORDIC_NRF_LF_CLOCK_CALIB_TIMER_INTERVAL",
                "value": 16
            },
            "lf_clock_rc_calib_mode_config": {
                "macro_name": "MBED_CONF_NORDIC_NRF_LF_CLOCK_CALIB_MODE_CONFIG",
                "value": 0
            }
        },
        "OUTPUT_EXT": "hex",
        "is_disk_virtual": true,
        "supported_toolchains": ["GCC_ARM", "ARM", "IAR"],
        "public": false,
        "detect_code": ["1101"],
        "program_cycle_s": 6,
        "bootloader_supported": true
    },
    "NRF52_DK": {
        "supported_form_factors": ["ARDUINO"],
        "inherits": ["MCU_NRF52832"],
        "release_versions": ["5"],
        "device_name": "nRF52832_xxAA"
    },
    "SDT52832B": {
        "inherits": ["MCU_NRF52832"],
        "release_versions": ["5"],
        "detect_code": ["3104"],
        "device_name": "nRF52832_xxAA"
    },
    "UBLOX_EVA_NINA": {
        "inherits": ["MCU_NRF52832"],
        "release_versions": ["5"],
        "device_name": "nRF52832_xxAA"
    },
    "UBLOX_EVK_NINA_B1": {
        "supported_form_factors": ["ARDUINO"],
        "inherits": ["MCU_NRF52832"],
        "release_versions": ["5"],
        "device_name": "nRF52832_xxAA"
    },
    "MTB_UBLOX_NINA_B1": {
        "inherits": ["MCU_NRF52832"],
        "release_versions": ["5"],
        "device_name": "nRF52832_xxAA"
    },
    "MTB_LAIRD_BL652": {
        "inherits": ["MCU_NRF52832"],
        "release_versions": ["5"],
        "device_name": "nRF52832_xxAA"
    },
    "DELTA_DFBM_NQ620": {
        "supported_form_factors": ["ARDUINO"],
        "inherits": ["MCU_NRF52832"],
        "release_versions": ["5"],
        "device_name": "nRF52832_xxAA"
    },
    "MCU_NRF52840": {
        "inherits": ["Target"],
        "core": "Cortex-M4F",
        "macros": [
            "BOARD_PCA10056",
            "NRF52840_XXAA",
            "TARGET_NRF52840",
            "CMSIS_VECTAB_VIRTUAL",
            "CMSIS_VECTAB_VIRTUAL_HEADER_FILE=\"cmsis_nvic.h\"",
            "MBED_TICKLESS",
            "MBEDTLS_CONFIG_HW_SUPPORT"
        ],
        "features": ["CRYPTOCELL310"],
        "device_has": [
            "ANALOGIN",
            "FLASH",
            "I2C",
            "I2C_ASYNCH",
            "INTERRUPTIN",
            "ITM",
            "LPTICKER",
            "PORTIN",
            "PORTINOUT",
            "PORTOUT",
            "PWMOUT",
            "SERIAL",
            "SERIAL_ASYNCH",
            "SERIAL_FC",
            "SLEEP",
            "SPI",
            "SPI_ASYNCH",
            "SYSTICK_CLK_OFF_DURING_SLEEP",
            "TRNG",
            "USTICKER",
            "QSPI"
        ],
        "extra_labels": [
            "NORDIC",
            "NRF5x",
            "NRF52",
            "SDK_14_2",
            "SOFTDEVICE_COMMON",
            "SOFTDEVICE_S140_FULL"
        ],
        "config": {
            "lf_clock_src": {
                "macro_name": "MBED_CONF_NORDIC_NRF_LF_CLOCK_SRC",
                "help": "Select Low Frequency clock source. Options: NRF_LF_SRC_XTAL, NRF_LF_SRC_SYNTH, and NRF_LF_SRC_RC",
                "value": "NRF_LF_SRC_XTAL"
            },
            "lf_clock_rc_calib_timer_interval": {
                "macro_name": "MBED_CONF_NORDIC_NRF_LF_CLOCK_CALIB_TIMER_INTERVAL",
                "value": 16
            },
            "lf_clock_rc_calib_mode_config": {
                "macro_name": "MBED_CONF_NORDIC_NRF_LF_CLOCK_CALIB_MODE_CONFIG",
                "value": 0
            }
        },
        "OUTPUT_EXT": "hex",
        "is_disk_virtual": true,
        "supported_toolchains": ["GCC_ARM", "ARM", "IAR"],
        "public": false,
        "detect_code": ["1101"],
        "program_cycle_s": 6,
        "bootloader_supported": true
    },
    "NRF52840_DK": {
        "supported_form_factors": ["ARDUINO"],
        "inherits": ["MCU_NRF52840"],
        "release_versions": ["5"],
        "device_name": "nRF52840_xxAA"
    },
    "MTB_LAIRD_BL654": {
        "inherits": ["MCU_NRF52840"],
        "release_versions": ["5"],
        "device_name": "nRF52840_xxAA",
        "detect_code": ["0465"],
        "features_remove": ["CRYPTOCELL310"],
        "macros_remove":  ["MBEDTLS_CONFIG_HW_SUPPORT"],
        "overrides": {
            "lf_clock_src": "NRF_LF_SRC_RC"
        }
    },
    "BLUEPILL_F103C8": {
        "inherits": ["FAMILY_STM32"],
        "core": "Cortex-M3",
        "default_toolchain": "GCC_ARM",
        "extra_labels_add": ["STM32F1", "STM32F103C8"],
        "supported_toolchains": ["GCC_ARM"],
        "device_has_add": ["CAN", "SERIAL_FC", "SERIAL_ASYNCH", "FLASH"],
        "device_has_remove": ["STDIO_MESSAGES", "LPTICKER"]
    },
    "NUMAKER_PFM_NUC472": {
        "core": "Cortex-M4F",
        "default_toolchain": "ARM",
        "extra_labels": ["NUVOTON", "NUC472", "NU_XRAM_SUPPORTED", "FLASH_CMSIS_ALGO", "NUVOTON_EMAC"],
        "is_disk_virtual": true,
        "supported_toolchains": ["ARM", "uARM", "GCC_ARM", "IAR"],
        "config": {
            "gpio-irq-debounce-enable": {
                "help": "Enable GPIO IRQ debounce",
                "value": 0
            },
            "gpio-irq-debounce-enable-list": {
                "help": "Comma separated pin list to enable GPIO IRQ debounce",
                "value": "NC"
            },
            "gpio-irq-debounce-clock-source": {
                "help": "Select GPIO IRQ debounce clock source: GPIO_DBCTL_DBCLKSRC_HCLK or GPIO_DBCTL_DBCLKSRC_IRC10K",
                "value": "GPIO_DBCTL_DBCLKSRC_IRC10K"
            },
            "gpio-irq-debounce-sample-rate": {
                "help": "Select GPIO IRQ debounce sample rate: GPIO_DBCTL_DBCLKSEL_1, GPIO_DBCTL_DBCLKSEL_2, GPIO_DBCTL_DBCLKSEL_4, ..., or GPIO_DBCTL_DBCLKSEL_32768",
                "value": "GPIO_DBCTL_DBCLKSEL_16"
            }
        },
        "inherits": ["Target"],
        "macros_add": ["MBEDTLS_CONFIG_HW_SUPPORT", "LPTICKER_DELAY_TICKS=3"],
        "device_has": ["USTICKER", "LPTICKER", "RTC", "ANALOGIN", "I2C", "I2CSLAVE", "I2C_ASYNCH", "INTERRUPTIN", "PORTIN", "PORTINOUT", "PORTOUT", "PWMOUT", "SERIAL", "SERIAL_ASYNCH", "SERIAL_FC", "STDIO_MESSAGES", "SLEEP", "SPI", "SPISLAVE", "SPI_ASYNCH", "TRNG", "CAN", "FLASH", "EMAC"],
        "release_versions": ["5"],
        "device_name": "NUC472HI8AE",
        "bootloader_supported": true,
        "overrides": {
            "network-default-interface-type": "ETHERNET"
        }
    },
    "NCS36510": {
        "inherits": ["Target"],
        "core": "Cortex-M3",
        "extra_labels": ["ONSEMI"],
        "config": {
            "mac-addr-low": {
                "help": "Lower 32 bits of the MAC extended address. All FFs indicates that factory programmed MAC address shall be used. In order to override the factory programmed MAC address this value needs to be changed from 0xFFFFFFFF to any chosen value.",
                "value": "0xFFFFFFFF"
            },
            "mac-addr-high": {
                "help": "Higher 32 bits of the MAC extended address. All FFs indicates that factory programmed MAC address shall be used. In order to override the factory programmed MAC address this value needs to be changed from 0xFFFFFFFF to any chosen value.",
                "value": "0xFFFFFFFF"
            },
            "32KHz-clk-trim": {
                "help": "32KHz clock trim",
                "value": "0x39"
            },
            "32MHz-clk-trim": {
                "help": "32MHz clock trim",
                "value": "0x17"
            },
            "rssi-trim": {
                "help": "RSSI trim",
                "value": "0x3D"
            },
            "txtune-trim": {
                "help": "TX tune trim",
                "value": "0xFFFFFFFF"
            }
        },
        "OUTPUT_EXT": "hex",
        "post_binary_hook": {"function": "NCS36510TargetCode.ncs36510_addfib"},
        "macros": ["CM3", "CPU_NCS36510", "TARGET_NCS36510", "LOAD_ADDRESS=0x3000"],
        "supported_toolchains": ["GCC_ARM", "ARM", "IAR"],
        "device_has": ["ANALOGIN", "SERIAL", "I2C", "INTERRUPTIN", "PORTIN", "PORTINOUT", "PORTOUT", "PWMOUT", "SERIAL", "SERIAL_FC", "SLEEP", "SPI", "TRNG", "SPISLAVE", "802_15_4_PHY"],
        "release_versions": ["2", "5"]
    },
    "NUMAKER_PFM_M453": {
        "core": "Cortex-M4F",
        "default_toolchain": "ARM",
        "extra_labels": ["NUVOTON", "M451", "NUMAKER_PFM_M453", "FLASH_CMSIS_ALGO"],
        "is_disk_virtual": true,
        "supported_toolchains": ["ARM", "uARM", "GCC_ARM", "IAR"],
        "config": {
            "gpio-irq-debounce-enable": {
                "help": "Enable GPIO IRQ debounce",
                "value": 0
            },
            "gpio-irq-debounce-enable-list": {
                "help": "Comma separated pin list to enable GPIO IRQ debounce",
                "value": "NC"
            },
            "gpio-irq-debounce-clock-source": {
                "help": "Select GPIO IRQ debounce clock source: GPIO_DBCTL_DBCLKSRC_HCLK or GPIO_DBCTL_DBCLKSRC_LIRC",
                "value": "GPIO_DBCTL_DBCLKSRC_LIRC"
            },
            "gpio-irq-debounce-sample-rate": {
                "help": "Select GPIO IRQ debounce sample rate: GPIO_DBCTL_DBCLKSEL_1, GPIO_DBCTL_DBCLKSEL_2, GPIO_DBCTL_DBCLKSEL_4, ..., or GPIO_DBCTL_DBCLKSEL_32768",
                "value": "GPIO_DBCTL_DBCLKSEL_16"
            }
        },
        "inherits": ["Target"],
        "macros_add": ["LPTICKER_DELAY_TICKS=3"],
        "progen": {"target": "numaker-pfm-m453"},
        "device_has": ["USTICKER", "LPTICKER", "RTC", "ANALOGIN", "I2C", "I2CSLAVE", "I2C_ASYNCH", "INTERRUPTIN", "PORTIN", "PORTINOUT", "PORTOUT", "PWMOUT", "SERIAL", "SERIAL_ASYNCH", "SERIAL_FC", "STDIO_MESSAGES", "SLEEP", "SPI", "SPISLAVE", "SPI_ASYNCH", "CAN", "FLASH"],
        "release_versions": ["2", "5"],
        "device_name": "M453VG6AE",
        "bootloader_supported": true
    },
    "NUMAKER_PFM_NANO130": {
        "core": "Cortex-M0",
        "default_toolchain": "ARM",
        "extra_labels": ["NUVOTON", "NANO100", "NANO130KE3BN"],
        "is_disk_virtual": true,
        "supported_toolchains": ["ARM", "uARM", "GCC_ARM", "IAR"],
        "config": {
            "gpio-irq-debounce-enable": {
                "help": "Enable GPIO IRQ debounce",
                "value": 0
            },
            "gpio-irq-debounce-enable-list": {
                "help": "Comma separated pin list to enable GPIO IRQ debounce",
                "value": "NC"
            },
            "gpio-irq-debounce-clock-source": {
                "help": "Select GPIO IRQ debounce clock source: GPIO_DBCLKSRC_HCLK or GPIO_DBCLKSRC_IRC10K",
                "value": "GPIO_DBCLKSRC_IRC10K"
            },
            "gpio-irq-debounce-sample-rate": {
                "help": "Select GPIO IRQ debounce sample rate: GPIO_DBCLKSEL_1, GPIO_DBCLKSEL_2, GPIO_DBCLKSEL_4, ..., or GPIO_DBCLKSEL_32768",
                "value": "GPIO_DBCLKSEL_16"
            },
            "clock-pll": {
                "help": "Choose clock source to clock PLL: NU_HXT_PLL or NU_HIRC_PLL",
                "macro_name": "NU_CLOCK_PLL",
                "value": "NU_HIRC_PLL"
            }
        },
        "inherits": ["Target"],
        "macros": ["CMSIS_VECTAB_VIRTUAL", "CMSIS_VECTAB_VIRTUAL_HEADER_FILE=\"cmsis_nvic.h\"","MBED_FAULT_HANDLER_DISABLED", "LPTICKER_DELAY_TICKS=3"],
        "device_has": ["USTICKER", "LPTICKER", "RTC", "ANALOGIN", "I2C", "I2CSLAVE", "I2C_ASYNCH", "INTERRUPTIN", "PORTIN", "PORTINOUT", "PORTOUT", "PWMOUT", "SERIAL", "SERIAL_ASYNCH", "SERIAL_FC", "STDIO_MESSAGES", "SLEEP", "SPI", "SPISLAVE", "SPI_ASYNCH"],
        "release_versions": ["5"],
        "device_name": "NANO130KE3BN"
    },
    "HI2110": {
        "inherits": ["Target"],
        "core": "Cortex-M0",
        "default_toolchain": "GCC_ARM",
        "supported_toolchains": ["GCC_ARM", "ARM", "IAR"],
        "extra_labels": ["ublox"],
        "macros": ["TARGET_PROCESSOR_FAMILY_BOUDICA", "BOUDICA_SARA", "NDEBUG=1", "CMSIS_VECTAB_VIRTUAL", "CMSIS_VECTAB_VIRTUAL_HEADER_FILE=\"cmsis_nvic.h\""],
        "public": false,
        "target_overrides": {
            "*": {
                "core.stdio-flush-at-exit": false
            }
        },
        "device_has": ["INTERRUPTIN", "PORTIN", "PORTINOUT", "PORTOUT", "SERIAL", "SLEEP", "STDIO_MESSAGES"],
        "default_lib": "std",
        "release_versions": []
   },
    "SARA_NBIOT": {
        "inherits": ["HI2110"],
        "extra_labels": ["ublox", "HI2110"],
        "public": false
    },
    "SARA_NBIOT_EVK": {
        "inherits": ["SARA_NBIOT"],
        "extra_labels": ["ublox", "HI2110", "SARA_NBIOT"]
    },
    "REALTEK_RTL8195AM": {
        "supported_form_factors": ["ARDUINO"],
        "core": "Cortex-M3",
        "default_toolchain": "GCC_ARM",
        "inherits": ["Target"],
        "detect_code": ["4600"],
        "extra_labels": ["Realtek", "AMEBA", "RTL8195A", "RTW_EMAC"],
        "macros": ["__RTL8195A__","CONFIG_PLATFORM_8195A","CONFIG_MBED_ENABLED","PLATFORM_CMSIS_RTOS","MBED_FAULT_HANDLER_DISABLED"],
        "supported_toolchains": ["GCC_ARM", "ARM", "IAR"],
        "device_has": ["ANALOGIN", "ANALOGOUT", "I2C", "I2CSLAVE", "INTERRUPTIN", "PORTIN", "PORTINOUT", "PORTOUT", "PWMOUT", "SERIAL", "SPI", "TRNG", "FLASH"],
        "post_binary_hook": {
            "function": "RTL8195ACode.binary_hook",
            "toolchains": ["ARM_STD", "GCC_ARM", "IAR"]
        },
        "release_versions": ["5"],
        "overrides": {
            "network-default-interface-type": "WIFI"
        }
    },
    "VBLUNO51_LEGACY": {
        "supported_form_factors": ["ARDUINO"],
        "inherits": ["MCU_NRF51_32K"],
        "detect_code": ["C006"],
        "overrides": {"uart_hwfc": 0},
        "extra_labels_add": ["VBLUNO51"]
    },
    "VBLUNO51_BOOT": {
        "supported_form_factors": ["ARDUINO"],
        "inherits": ["MCU_NRF51_32K_BOOT"],
        "detect_code": ["C006"],
        "overrides": {"uart_hwfc": 0},
        "extra_labels_add": ["VBLUNO51"],
        "macros_add": ["TARGET_VBLUNO51"]
    },
    "VBLUNO51_OTA": {
        "supported_form_factors": ["ARDUINO"],
        "inherits": ["MCU_NRF51_32K_OTA"],
        "detect_code": ["C006"],
        "overrides": {"uart_hwfc": 0},
        "extra_labels_add": ["VBLUNO51"],
        "macros_add": ["TARGET_VBLUNO51"]
    },
    "VBLUNO51": {
        "supported_form_factors": ["ARDUINO"],
        "inherits": ["MCU_NRF51_32K_UNIFIED"],
        "detect_code": ["C006"],
        "overrides": {"uart_hwfc": 0},
        "device_has": ["USTICKER", "LPTICKER", "ANALOGIN", "I2C", "I2C_ASYNCH", "INTERRUPTIN", "PORTIN", "PORTINOUT", "PORTOUT", "PWMOUT", "SERIAL", "SERIAL_ASYNCH", "SERIAL_FC", "SLEEP", "SPI", "SPI_ASYNCH", "SPISLAVE"],
        "release_versions": ["2"],
        "device_name": "nRF51822_xxAC"
    },
    "DISCO_L496AG": {
        "inherits": ["FAMILY_STM32"],
        "supported_form_factors": ["ARDUINO"],
        "core": "Cortex-M4F",
        "extra_labels_add": ["STM32L4", "STM32L496AG", "STM32L496xG"],
        "config": {
            "clock_source": {
                "help": "Mask value : USE_PLL_HSE_EXTC (need HW patch) | USE_PLL_HSE_XTAL (need HW patch) | USE_PLL_HSI | USE_PLL_MSI",
                "value": "USE_PLL_MSI",
                "macro_name": "CLOCK_SOURCE"
            },
            "lpticker_lptim": {
                "help": "This target supports LPTIM. Set value 1 to use LPTIM for LPTICKER, or 0 to use RTC wakeup timer",
                "value": 1
            }
        },
        "detect_code": ["0822"],
        "device_has_add": ["ANALOGOUT", "CAN", "CRC", "SERIAL_ASYNCH", "SERIAL_FC", "TRNG", "FLASH"],
        "release_versions": ["2", "5"],
        "device_name": "STM32L496AG",
        "bootloader_supported": true
    },
    "NUCLEO_L496ZG": {
        "inherits": ["FAMILY_STM32"],
        "supported_form_factors": ["ARDUINO", "MORPHO"],
        "core": "Cortex-M4F",
        "extra_labels_add": ["STM32L4", "STM32L496ZG", "STM32L496xG"],
        "config": {
            "clock_source": {
                "help": "Mask value : USE_PLL_HSE_EXTC (need HW patch) | USE_PLL_HSE_XTAL (need HW patch) | USE_PLL_HSI | USE_PLL_MSI",
                "value": "USE_PLL_MSI",
                "macro_name": "CLOCK_SOURCE"
            },
            "lpticker_lptim": {
                "help": "This target supports LPTIM. Set value 1 to use LPTIM for LPTICKER, or 0 to use RTC wakeup timer",
                "value": 1
            }
        },
        "detect_code": ["0823"],
        "device_has_add": ["ANALOGOUT", "CAN", "CRC", "SERIAL_ASYNCH", "SERIAL_FC", "TRNG", "FLASH"],
        "release_versions": ["2", "5"],
        "device_name": "STM32L496ZG",
        "bootloader_supported": true
    },
    "NUCLEO_L496ZG_P": {
        "inherits": ["NUCLEO_L496ZG"],
        "detect_code": ["0828"]
    },
    "NUCLEO_L4R5ZI": {
        "inherits": ["FAMILY_STM32"],
        "supported_form_factors": ["ARDUINO", "MORPHO"],
        "core": "Cortex-M4F",
        "extra_labels_add": ["STM32L4", "STM32L4R5ZI", "STM32L4R5xI"],
        "config": {
            "clock_source": {
                "help": "Mask value : USE_PLL_HSE_EXTC (need HW patch) | USE_PLL_HSE_XTAL (need HW patch) | USE_PLL_HSI | USE_PLL_MSI",
                "value": "USE_PLL_MSI",
                "macro_name": "CLOCK_SOURCE"
            },
            "lpticker_lptim": {
                "help": "This target supports LPTIM. Set value 1 to use LPTIM for LPTICKER, or 0 to use RTC wakeup timer",
                "value": 1
            }
        },
        "detect_code": ["0776"],
        "device_has_add": ["ANALOGOUT", "CAN", "CRC", "SERIAL_ASYNCH", "SERIAL_FC", "TRNG", "FLASH"],
        "release_versions": ["2", "5"],
        "device_name": "STM32L4R5ZI",
        "bootloader_supported": true
    },
    "VBLUNO52": {
        "supported_form_factors": ["ARDUINO"],
        "inherits": ["MCU_NRF52832"],
        "release_versions": ["5"],
        "device_name": "nRF52832_xxAA"
    },
    "MCU_M480": {
        "core": "Cortex-M4F",
        "default_toolchain": "ARM",
        "public": false,
        "extra_labels": ["NUVOTON", "M480", "FLASH_CMSIS_ALGO","NUVOTON_EMAC"],
        "is_disk_virtual": true,
        "supported_toolchains": ["ARM", "uARM", "GCC_ARM", "IAR"],
        "config": {
            "gpio-irq-debounce-enable": {
                "help": "Enable GPIO IRQ debounce",
                "value": 0
            },
            "gpio-irq-debounce-enable-list": {
                "help": "Comma separated pin list to enable GPIO IRQ debounce",
                "value": "NC"
            },
            "gpio-irq-debounce-clock-source": {
                "help": "Select GPIO IRQ debounce clock source: GPIO_DBCTL_DBCLKSRC_HCLK or GPIO_DBCTL_DBCLKSRC_LIRC",
                "value": "GPIO_DBCTL_DBCLKSRC_LIRC"
            },
            "gpio-irq-debounce-sample-rate": {
                "help": "Select GPIO IRQ debounce sample rate: GPIO_DBCTL_DBCLKSEL_1, GPIO_DBCTL_DBCLKSEL_2, GPIO_DBCTL_DBCLKSEL_4, ..., or GPIO_DBCTL_DBCLKSEL_32768",
                "value": "GPIO_DBCTL_DBCLKSEL_16"
            },
            "usb-device-hsusbd": {
                "help": "Select high-speed USB device or not",
                "value": 1
            },
            "ctrl01-enable": {
                "help": "Enable control_01",
                "value": 0
            }
        },
        "inherits": ["Target"],
        "macros_add": ["MBEDTLS_CONFIG_HW_SUPPORT", "LPTICKER_DELAY_TICKS=3"],
        "device_has": ["USTICKER", "LPTICKER", "RTC", "ANALOGIN", "I2C", "I2CSLAVE", "I2C_ASYNCH", "INTERRUPTIN", "PORTIN", "PORTINOUT", "PORTOUT", "PWMOUT", "SERIAL", "SERIAL_ASYNCH", "SERIAL_FC", "STDIO_MESSAGES", "SLEEP", "SPI", "SPISLAVE", "SPI_ASYNCH", "TRNG", "FLASH", "CAN", "EMAC"],
        "release_versions": ["5"],
        "bootloader_supported": true,
        "overrides": {
            "network-default-interface-type": "ETHERNET"
        }
    },
    "NUMAKER_PFM_M487": {
        "inherits": ["MCU_M480"],
        "device_name": "M487JIDAE"
    },
    "NUMAKER_IOT_M487": {
        "inherits": ["MCU_M480"],
        "device_name": "M487JIDAE"
    },
    "TMPM066": {
        "inherits": ["Target"],
        "core": "Cortex-M0",
        "is_disk_virtual": true,
        "extra_labels": ["TOSHIBA"],
        "macros": ["__TMPM066__", "CMSIS_VECTAB_VIRTUAL", "CMSIS_VECTAB_VIRTUAL_HEADER_FILE=\"cmsis_nvic.h\""],
        "supported_toolchains": ["GCC_ARM", "ARM", "IAR"],
        "device_has": ["USTICKER", "ANALOGIN", "INTERRUPTIN", "PORTIN", "PORTINOUT", "PORTOUT", "SERIAL", "SLEEP", "I2C", "I2CSLAVE", "STDIO_MESSAGES", "PWMOUT"],
        "device_name": "TMPM066FWUG",
        "detect_code": ["7011"],
        "release_versions": ["5"]
    },
    "SAKURAIO_EVB_01": {
        "inherits": ["FAMILY_STM32"],
        "supported_form_factors": [],
        "core": "Cortex-M4F",
        "extra_labels_add": ["STM32F4", "STM32F411xE", "STM32F411RE"],
        "device_has": ["ANALOGIN", "I2C", "I2CSLAVE", "I2C_ASYNCH", "INTERRUPTIN", "PORTIN", "PORTINOUT", "PORTOUT", "PWMOUT", "SERIAL", "SLEEP", "SPI", "SPISLAVE", "SPI_ASYNCH", "STDIO_MESSAGES"],
        "config": {
            "clock_source": {
                "help": "Mask value : USE_PLL_HSE_EXTC | USE_PLL_HSE_XTAL (need HW patch) | USE_PLL_HSI",
                "value": "USE_PLL_HSI",
                "macro_name": "CLOCK_SOURCE"
            }
        },
        "device_has_add": ["SERIAL_ASYNCH", "SERIAL_FC", "FLASH"],
        "release_versions": ["2"],
        "device_name": "STM32F411RE"
    },
    "TMPM46B": {
        "inherits": ["Target"],
        "core": "Cortex-M4",
        "is_disk_virtual": true,
        "extra_labels": ["TOSHIBA"],
        "macros": ["__TMPM46B__"],
        "supported_toolchains": ["GCC_ARM", "ARM", "IAR"],
        "device_has": ["USTICKER", "ANALOGIN", "INTERRUPTIN", "PORTIN", "PORTINOUT", "PORTOUT", "PWMOUT", "SERIAL", "SERIAL_FC", "SPI", "I2C", "STDIO_MESSAGES", "TRNG", "FLASH", "SLEEP"],
        "device_name": "TMPM46BF10FG",
        "detect_code": ["7013"],
        "release_versions": ["5"],
        "bootloader_supported": true
    },
    "ARM_FM": {
        "inherits": ["Target"],
        "public": false,
        "macros": ["__ARM_FM"],
        "extra_labels": ["ARM_FM"]
    },
    "FVP_MPS2": {
        "inherits": ["ARM_FM"],
        "public": false,
        "supported_toolchains": ["GCC_ARM", "ARM", "IAR"],
        "OUTPUT_EXT": "elf",
        "device_has": ["AACI", "ANALOGIN", "CLCD", "FLASH", "I2C", "INTERRUPTIN", "PORTIN", "PORTINOUT", "PORTOUT", "SERIAL", "SERIAL_FC", "SPI", "SPISLAVE", "TSC", "USTICKER"],
        "release_versions": ["5"]
    },
    "FVP_MPS2_M0": {
        "inherits": ["FVP_MPS2"],
        "core": "Cortex-M0",
        "macros_add": ["CMSDK_CM0"]
    },
    "FVP_MPS2_M0P": {
        "inherits": ["FVP_MPS2"],
        "core": "Cortex-M0+",
        "macros_add": ["CMSDK_CM0plus"]
    },
    "FVP_MPS2_M3": {
        "inherits": ["FVP_MPS2"],
        "core": "Cortex-M3",
        "macros_add": ["CMSDK_CM3"]
    },
    "FVP_MPS2_M4": {
        "inherits": ["FVP_MPS2"],
        "core": "Cortex-M4",
        "macros_add": ["CMSDK_CM4"]
    },
    "FVP_MPS2_M7": {
        "inherits": ["FVP_MPS2"],
        "core": "Cortex-M7",
        "macros_add": ["CMSDK_CM7"]
    },
    "NUMAKER_PFM_M2351": {
        "core": "Cortex-M23-NS",
        "default_toolchain": "ARMC6",
        "extra_labels": ["NUVOTON", "M2351", "M2351KIAAEES", "FLASH_CMSIS_ALGO"],
        "OUTPUT_EXT": "hex",
        "macros": ["MBED_FAULT_HANDLER_DISABLED", "MBED_TZ_DEFAULT_ACCESS=1", "LPTICKER_DELAY_TICKS=3"],
        "is_disk_virtual": true,
        "supported_toolchains": ["ARMC6"],
        "config": {
            "gpio-irq-debounce-enable": {
                "help": "Enable GPIO IRQ debounce",
                "value": 0
            },
            "gpio-irq-debounce-enable-list": {
                "help": "Comma separated pin list to enable GPIO IRQ debounce",
                "value": "NC"
            },
            "gpio-irq-debounce-clock-source": {
                "help": "Select GPIO IRQ debounce clock source: GPIO_DBCTL_DBCLKSRC_HCLK or GPIO_DBCTL_DBCLKSRC_LIRC",
                "value": "GPIO_DBCTL_DBCLKSRC_LIRC"
            },
            "gpio-irq-debounce-sample-rate": {
                "help": "Select GPIO IRQ debounce sample rate: GPIO_DBCTL_DBCLKSEL_1, GPIO_DBCTL_DBCLKSEL_2, GPIO_DBCTL_DBCLKSEL_4, ..., or GPIO_DBCTL_DBCLKSEL_32768",
                "value": "GPIO_DBCTL_DBCLKSEL_16"
            }
        },
        "mbed_rom_start":   "0x10040000",
        "mbed_rom_size":    "0x40000",
        "mbed_ram_start":   "0x30008000",
        "mbed_ram_size":    "0x10000",
        "inherits": ["Target"],
        "device_has": ["USTICKER", "LPTICKER", "RTC", "ANALOGIN", "I2C", "I2CSLAVE", "I2C_ASYNCH", "INTERRUPTIN", "PORTIN", "PORTINOUT", "PORTOUT", "PWMOUT", "SERIAL", "SERIAL_ASYNCH", "SERIAL_FC", "STDIO_MESSAGES", "SLEEP", "SPI", "SPISLAVE", "SPI_ASYNCH", "TRNG", "FLASH"],
        "detect_code": ["1305"],
        "release_versions": ["5"],
        "device_name": "M2351KIAAEES",
        "bootloader_supported": true
    },
    "TMPM3H6": {
        "inherits": ["Target"],
        "core": "Cortex-M3",
        "is_disk_virtual": true,
        "extra_labels": ["TOSHIBA"],
        "macros": ["__TMPM3H6__"],
        "supported_toolchains": ["GCC_ARM", "ARM", "IAR"],
        "device_has": ["USTICKER", "ANALOGIN", "ANALOGOUT", "INTERRUPTIN", "PORTIN", "PORTINOUT", "PORTOUT", "PWMOUT", "SERIAL", "SLEEP", "SPI", "I2C", "I2CSLAVE", "STDIO_MESSAGES"],
        "device_name": "TMPM3H6FWFG",
        "detect_code": ["7012"],
        "release_versions": ["5"]
    },
    "TMPM4G9": {
        "inherits": ["Target"],
        "core": "Cortex-M4",
        "is_disk_virtual": true,
        "extra_labels": ["TOSHIBA"],
        "macros": ["__TMPM4G9__"],
        "supported_toolchains": ["GCC_ARM", "ARM", "IAR"],
        "device_has": ["ANALOGIN", "ANALOGOUT", "INTERRUPTIN", "PORTIN", "PORTINOUT", "PORTOUT", "PWMOUT", "SERIAL", "SPI", "I2C", "I2CSLAVE", "STDIO_MESSAGES", "FLASH", "SLEEP", "USTICKER"],
        "device_name": "TMPM4G9F15FG",
        "detect_code": ["7016"],
        "release_versions": ["5"],
        "bootloader_supported": true
    },
    "MCU_PSOC6": {
        "inherits": ["Target"],
        "default_toolchain": "GCC_ARM",
        "supported_toolchains": ["GCC_ARM", "IAR", "ARM"],
        "core": "Cortex-M4F",
        "OUTPUT_EXT": "hex",
        "device_has": ["USTICKER", "INTERRUPTIN", "SERIAL", "SERIAL_ASYNCH", "SERIAL_FC", "PORTIN", "PORTOUT", "PORTINOUT", "RTC", "PWMOUT", "ANALOGIN", "ANALOGOUT", "I2C", "I2C_ASYNCH", "SPI", "SPI_ASYNCH", "STDIO_MESSAGES", "LPTICKER", "SLEEP", "FLASH" ],
        "release_versions": ["5"],
        "extra_labels": ["Cypress", "PSOC6"],
        "public": false
    },
    "MCU_PSOC6_M0": {
        "inherits": ["MCU_PSOC6"],
        "core": "Cortex-M0+",
        "macros": ["MCU_PSOC6_M0"],
        "public": false
    },
    "MCU_PSOC6_M4": {
        "inherits": ["MCU_PSOC6"],
        "macros": ["MCU_PSOC6_M4"],
        "public": false
    },
    "FUTURE_SEQUANA_M0": {
        "inherits": ["MCU_PSOC6_M0"],
        "supported_form_factors": ["ARDUINO"],
        "extra_labels_add": ["CY8C63XX", "FUTURE_SEQUANA"],
        "macros_add": ["CY8C6347BZI_BLD53"],
        "detect_code": ["6000"],
        "post_binary_hook": {
            "function": "PSOC6Code.complete"
        },
        "config": {
            "system-clock": {
                "help": "Desired frequency of main clock (Hz)",
                "value": "100000000UL",
                "macro_name": "CY_CLK_HFCLK0_FREQ_HZ"
            },
            "peri-clock": {
                "help": "Desired frequency of peripheral clock (Hz)",
                "value": "50000000UL",
                "macro_name": "CY_CLK_PERICLK_FREQ_HZ"
            },
            "m0-clock": {
                "help": "Desired frequency of M0+ core clock (Hz)",
                "value": "50000000UL",
                "macro_name": "CY_CLK_SLOWCLK_FREQ_HZ"
            }
        }
    },
    "FUTURE_SEQUANA": {
        "inherits": ["MCU_PSOC6_M4"],
        "sub_target": "FUTURE_SEQUANA_M0",
        "supported_form_factors": ["ARDUINO"],
        "extra_labels_add": ["CY8C63XX", "CORDIO"],
        "macros_add": ["CY8C6347BZI_BLD53"],
        "detect_code": ["6000"],
        "m0_core_img": "psoc63_m0_default_1.01.hex",
        "post_binary_hook": {
            "function": "PSOC6Code.complete"
        },
        "config": {
            "system-clock": {
                "help": "Desired frequency of main clock (Hz)",
                "value": "100000000UL",
                "macro_name": "CY_CLK_HFCLK0_FREQ_HZ"
            },
            "peri-clock": {
                "help": "Desired frequency of peripheral clock (Hz)",
                "value": "50000000UL",
                "macro_name": "CY_CLK_PERICLK_FREQ_HZ"
            },
            "m0-clock": {
                "help": "Desired frequency of M0+ core clock (Hz)",
                "value": "50000000UL",
                "macro_name": "CY_CLK_SLOWCLK_FREQ_HZ"
            }
        }
    },
    "TMPM3HQ": {
        "inherits": ["Target"],
        "core": "Cortex-M3",
        "is_disk_virtual": true,
        "extra_labels": ["TOSHIBA"],
        "macros": ["__TMPM3HQ__"],
        "supported_toolchains": ["GCC_ARM", "ARM", "IAR"],
        "device_has": ["USTICKER", "ANALOGIN", "ANALOGOUT", "INTERRUPTIN", "PORTIN", "PORTINOUT", "PORTOUT", "PWMOUT", "SERIAL", "SLEEP", "SPI", "I2C", "I2CSLAVE", "STDIO_MESSAGES"],
        "device_name": "TMPM3HQFDFG",
        "detect_code": ["7014"],
        "release_versions": ["5"]
    },
    "RDA5981X": {
        "inherits": ["Target"],
        "core": "Cortex-M4F",
        "public": true,
        "extra_labels": ["RDA", "UNO_91H", "FLASH_CMSIS_ALGO"],
        "supported_toolchains": ["ARM", "GCC_ARM", "IAR"],
        "macros": ["TWO_RAM_REGIONS", "CMSIS_NVIC_VIRTUAL", "CMSIS_NVIC_VIRTUAL_HEADER_FILE=\"RDA5981_nvic_virtual.h\""],
        "device_has": ["USTICKER", "PORTIN", "PORTOUT", "PORTINOUT", "INTERRUPTIN", "SERIAL", "STDIO_MESSAGES", "PWMOUT", "SPI", "SLEEP", "ANALOGIN", "FLASH", "TRNG"],
        "release_versions": ["2", "5"]
    },
    "UNO_91H": {
        "inherits": ["RDA5981X"],
        "detect_code": ["8001"]
    }
}
