<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<library>
<packages>
<package name="SWD-10-TAGCONNECT">
</package>
<package name="SWD-10-SMD">
</package>
<package name="SWD-10-PTH">
</package>
<package name="BAT60A">
</package>
<package name="SOT23">
<description>&lt;b&gt;SOT-23&lt;/b&gt;</description>
</package>
<package name="MBED-ENABLED-LOGO-250X250-MIL">
</package>
<package name="MBED-ENABLED-LOGO-500X500-MIL">
</package>
<package name="MBED-ENABLED-LOGO-1000X1000-MIL">
</package>
<package name="CE-MARK-0.2">
</package>
<package name="PB-MARK-0.2">
</package>
<package name="SOT223">
<description>SOT223</description>
</package>
<package name="MBED-ICS_LQFP64">
</package>
<package name="LQFP100">
</package>
<package name="0402">
</package>
<package name="0603">
</package>
<package name="0805">
</package>
<package name="C1206">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
<package name="C1210">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
<package name="C1812">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
<package name="FC135">
<description>&lt;B&gt;Abracon ABS07 32.768 kHz crystal&lt;/B&gt;
&lt;P&gt;3.2 x 1.5 x 0.9mm</description>
</package>
<package name="HC49UP">
<description>CRYSTAL SMD</description>
</package>
<package name="TC38">
<description>Crystal TC38</description>
</package>
<package name="HC49U-H">
<description>&lt;b&gt;CRYSTAL&lt;/b&gt;</description>
</package>
<package name="HC49U-V">
<description>&lt;b&gt;CRYSTAL&lt;/b&gt;</description>
</package>
<package name="TC38-SMD">
</package>
<package name="3.2X.2.5">
</package>
<package name="DTSM-32S-B">
</package>
<package name="SKRKAEE010">
</package>
<package name="CHIPLED_0603">
<description>&lt;b&gt;CHIPLED&lt;/b&gt;&lt;p&gt;
Source: http://www.osram.convergy.de/ ... LG_LY Q971.pdf</description>
</package>
<package name="CHIPLED_0805">
<description>&lt;b&gt;CHIPLED&lt;/b&gt;&lt;p&gt;
Source: http://www.osram.convergy.de/ ... LG_R971.pdf</description>
</package>
<package name="CHIPLED_1206">
<description>&lt;b&gt;CHIPLED&lt;/b&gt;&lt;p&gt;
Source: http://www.osram.convergy.de/ ... LG_LY N971.pdf</description>
</package>
<package name="HVQFN33">
<description>&lt;b&gt;HVQFN32&lt;/b&gt; (SOT617-3) 5 x 5 x .85 mm,  Pitch 0.5mm&lt;p&gt;
Source: http://www.semiconductors.philips.com/acrobat_download/datasheets/TDA9885_TDA9886_2.pdf</description>
</package>
<package name="LQFP80">
<description>&lt;b&gt;80 Lead LQFP_ED (SQ-80) (ST-80)&lt;/b&gt;&lt;p&gt;
www.analog.com AD9852_b.pdf</description>
</package>
<package name="SO20-2">
<description>&lt;b&gt;Small Outline Package&lt;/b&gt;</description>
</package>
<package name="TSSOP20">
<description>&lt;b&gt;Thin Shrink Small Outline Plastic 20&lt;/b&gt;&lt;p&gt;
MAX3223-MAX3243.pdf</description>
</package>
<package name="LQFP48">
</package>
<package name="USB-A-H">
<description>&lt;b&gt;USB Series A Hole Mounted&lt;/b&gt;</description>
</package>
<package name="USB-A-S">
<description>&lt;b&gt;USB Series A Surface Mounted&lt;/b&gt;</description>
</package>
<package name="USB-B-H">
<description>&lt;b&gt;USB Series B Hole Mounted&lt;/b&gt;</description>
</package>
<package name="USB-B-SMT">
<description>USB Series B Surface Mounted</description>
</package>
<package name="USB-MB-H">
<description>&lt;b&gt;USB Series Mini-B Hole Mounted&lt;/b&gt;</description>
</package>
<package name="USB-MB-S">
<description>&lt;b&gt;USB Series Mini-B Surface Mounted&lt;/b&gt;</description>
</package>
<package name="5075ABMR-05-SM1">
<description>&lt;B&gt;Neltron 5075ABMR-05-SM1 Mini-USB 5-pin Female Connector&lt;/B&gt;</description>
</package>
<package name="USB-A-V">
</package>
<package name="USB-MS-S-NO-PTH">
</package>
<package name="CASE-B">
<description>Tantal Chip-Elko 10uF</description>
</package>
<package name="LLP-40">
<description>&lt;B&gt;National SQA40A 40-pin 0.5mm pitch LLP package&lt;/B&gt;
&lt;P&gt;Thermal vias should be 8mil-13mil (0.2mm-0.33mm), plugged or tented.
&lt;P&gt;Paste stencil should be 5mil (0.127mm) thick.</description>
</package>
<package name="RJ45">
</package>
<package name="SOT163-1">
<description>&lt;li&gt;&lt;b&gt;SOT163-1&lt;/b&gt;&lt;hr&gt;
&lt;ul&gt;&lt;li&gt;SO20: plastic small outline package; 20 leads; body width 7.5 mm
&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: MS-013
&lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;: 075E04&lt;/ul&gt;</description>
</package>
<package name="SOT360">
<description>&lt;li&gt;&lt;b&gt;SOT360&lt;/b&gt;&lt;hr&gt;
&lt;ul&gt;&lt;li&gt;TSSOP20: plastic thin shrink small outline package; 20 leads; body width 4.4 mm
&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: MO-153
&lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;: &lt;/ul&gt;</description>
</package>
<package name="SOT313-2">
<description>&lt;li&gt;&lt;b&gt;SOT313-2&lt;/b&gt;&lt;hr&gt;
&lt;ul&gt;&lt;li&gt;LQFP48: plastic low profile quad flat package; 48 leads; body 7 x 7 x 1.4 mm
&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: MS-026
&lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;: 136E05&lt;/ul&gt;
Footprint according to NXP SOT313-2 specification, however the cornerpins are 0.4mm in stead of 0.5mm. Probably an error in the specification.</description>
</package>
<package name="SOT314-2">
<description>&lt;li&gt;&lt;b&gt;SOT314-2&lt;/b&gt;
&lt;hr&gt;
&lt;ul&gt;&lt;li&gt;LQFP64: plastic low profile quad flat package; 64 leads; body 10 x 10 x 1.4 mm
&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: MS-026
&lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;: 136E10&lt;/ul&gt;</description>
</package>
<package name="SOT950-1">
<description>&lt;li&gt;&lt;b&gt;SOT950-1&lt;/b&gt;&lt;hr&gt;
&lt;ul&gt;&lt;li&gt;TFBGA208: plastic thin fine-pitch ball grid array package; 208 balls; body 15 x 15 x 0.7 mm&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: --
&lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;: --
&lt;li&gt;&lt;u&gt;JEITA&lt;/u&gt;: --&lt;/ul&gt;</description>
</package>
<package name="SOT117">
<description>&lt;li&gt;&lt;b&gt;SOT117&lt;/b&gt;&lt;hr&gt;
&lt;ul&gt;&lt;li&gt;DIP28: plastic dual in-line package; 28 leads (600 mil)
&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: MO-015
&lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;: 051G05
&lt;li&gt;&lt;u&gt;JEITA&lt;/u&gt;: SC-510-28&lt;/ul&gt;</description>
</package>
<package name="MOLEX-47364-0001">
</package>
<package name="DIL14">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="TSSOP14">
<description>&lt;b&gt;plastic thin shrink small outline package; 14 leads; body width 4.4 mm&lt;/b&gt;&lt;p&gt;
SOT402-1&lt;br&gt;
Source: http://www.nxp.com/documents/data_sheet/74ABT125.pdf</description>
</package>
<package name="SSOP14">
<description>&lt;b&gt;plastic shrink small outline package; 14 leads; body width 5.3 mm&lt;/b&gt;&lt;p&gt;
SOT337-1&lt;br&gt;
Source: http://www.nxp.com/documents/data_sheet/74ABT125.pdf</description>
</package>
<package name="DHVQFN14">
<description>&lt;b&gt;plastic dual in-line compatible thermal enhanced very thin quad flat package; no leads; 14 terminals; body 2.5 x 3 x 0.85 mm&lt;/b&gt;&lt;p&gt;
Source: http://www.nxp.com/documents/data_sheet/74ABT125.pdf</description>
</package>
</packages>
<symbols>
<symbol name="SWD-10">
<pin name="P$1"/>
<pin name="P$2"/>
<pin name="P$3"/>
<pin name="P$4"/>
<pin name="P$5"/>
<pin name="P$6"/>
<pin name="P$7"/>
<pin name="P$8"/>
<pin name="P$9"/>
<pin name="P$10"/>
</symbol>
<symbol name="BAT60A">
<pin name="A" direction="pas"/>
<pin name="K" direction="pas"/>
</symbol>
<symbol name="P-MOS">
<pin name="G" direction="pas"/>
<pin name="D" direction="pas"/>
<pin name="S" direction="pas"/>
</symbol>
<symbol name="MBED_HDK">
</symbol>
<symbol name="MBED-ENABLED-LOGO">
</symbol>
<symbol name="CE-MARK">
</symbol>
<symbol name="PB-FREE">
</symbol>
<symbol name="LD1117S33">
<pin name="IN" direction="in"/>
<pin name="GND" direction="in"/>
<pin name="OUT" direction="pas"/>
<pin name="K" direction="pas"/>
</symbol>
<symbol name="LPC11U24">
<pin name="NTRST/PIO0.14/AD3/CT32B1M1"/>
<pin name="PIO0.0/NRESET"/>
<pin name="PIO0.1/CLKOUT/CT32B0M2/USB_FTOG"/>
<pin name="PIO0.2/SSEL0/CT16B0C0"/>
<pin name="PIO0.3/USB_VBUS"/>
<pin name="PIO0.4/SCL(OD)"/>
<pin name="PIO0.5/SDA(OD)"/>
<pin name="PIO0.6/USB_CON/SCK0"/>
<pin name="PIO0.7/CTS"/>
<pin name="PIO0.8/MISO0/CT16B0M0"/>
<pin name="PIO0.9/MOSI0/CT16B0M1"/>
<pin name="PIO0.16/AD5/CT32B1M3/WAKEUP"/>
<pin name="PIO0.17/RTS/CT32B0C0/SCLK"/>
<pin name="PIO0.18/RXD/CT32B0M0"/>
<pin name="PIO0.19/TXD/CT32B0M1"/>
<pin name="PIO0.20/CT16B1C0"/>
<pin name="PIO0.21/CT16B1M0/MOSI1"/>
<pin name="PIO0.22/AD6/CT16B1M1/MISO1"/>
<pin name="PIO0.23/AD7"/>
<pin name="PIO1.0/CT32B1M0"/>
<pin name="PIO1.1/CT32B1M1"/>
<pin name="PIO1.2/CT32B1M2"/>
<pin name="PIO1.3/CT32B1M3"/>
<pin name="PIO1.4/CT32B1C0"/>
<pin name="PIO1.5/CT32B1C1"/>
<pin name="PIO1.6"/>
<pin name="PIO1.7"/>
<pin name="PIO1.8"/>
<pin name="PIO1.9"/>
<pin name="PIO1.10"/>
<pin name="PIO1.11"/>
<pin name="PIO1.12"/>
<pin name="PIO1.13/DTR/CT16B0M1/TXD"/>
<pin name="PIO1.14/DSR/CT16B0M1/RXD"/>
<pin name="PIO1.15/DCD/CT16B0M2/SCK1"/>
<pin name="PIO1.16/RI/CT16B0C0"/>
<pin name="PIO1.17/CT16B0C1/RXD"/>
<pin name="PIO1.18/CT16B1C1/TXD"/>
<pin name="PIO1.19/DTR/SSEL1"/>
<pin name="PIO1.20/DSR/SCK1"/>
<pin name="PIO1.21/DCD/MISO1"/>
<pin name="PIO1.22/RI/MOSI1"/>
<pin name="PIO1.23/CT16B1M1/SSEL1"/>
<pin name="PIO1.24/CT32B0M0"/>
<pin name="PIO1.25/CT32B0M1"/>
<pin name="PIO1.26/CT32B0M2/RXD"/>
<pin name="PIO1.27/CT32B0M3/TXD"/>
<pin name="PIO1.28/CT32B0C0/SCLK"/>
<pin name="PIO1.29/SCK0/CT32B0C1"/>
<pin name="SWCLK/PIO0.10/SCK0/CT16B0M2"/>
<pin name="SWDIO/PIO0.15/AD4/CT32B1M2"/>
<pin name="TDI/PIO0.11/AD0/CT32B0M3"/>
<pin name="TDO/PIO0.13/AD2/CB32B1M0"/>
<pin name="TMS/PIO0.12/AD1/CT32B1M0"/>
<pin name="USB_D+"/>
<pin name="USB_D-"/>
<pin name="VDD@10"/>
<pin name="VDD@33"/>
<pin name="VDD@48"/>
<pin name="VDD@58"/>
<pin name="VSS@7"/>
<pin name="VSS@54"/>
<pin name="XTALIN"/>
<pin name="XTALOUT"/>
</symbol>
<symbol name="LPC1768">
<pin name="TRST_N"/>
<pin name="TDI"/>
<pin name="TMS/SWDIO"/>
<pin name="TCK/SWDCLK"/>
<pin name="RTCK"/>
<pin name="TDO/SWO"/>
<pin name="RSTOUTN"/>
<pin name="P0.0/CAN_RX1/TXD3/SDA1"/>
<pin name="P0.1/CAN_TX1/RXD3/SCL1"/>
<pin name="P0.2/TXD0/AD0.7"/>
<pin name="P0.3/RXD0/AD0.6"/>
<pin name="P0.4/I2SRX_CLK/CAN_RX2/CAP2.0"/>
<pin name="P0.5/I2SRX_WS/CAN_TX2/CAP2.1"/>
<pin name="P0.6/I2SRX_SDA/SSEL1/MAT2.0"/>
<pin name="P0.7/I2STX_CLK/SCK1/MAT2.1"/>
<pin name="P0.8/I2STX_WS/MISO1/MAT2.2"/>
<pin name="P0.9/I2STX_SDA/MOSI1/MAT2.3"/>
<pin name="P0.10/TXD2/SDA2/MAT3.0"/>
<pin name="P0.11/RXD2/SCL2/MAT3.1"/>
<pin name="P0.15/TXD1/SCK0/SCK"/>
<pin name="P0.16/RXD1/SSEL0/SSEL"/>
<pin name="P0.17/CTS1/MISO0/MISO"/>
<pin name="P0.18/DCD1/MOSI0/MOSI1"/>
<pin name="P0.19/DSR1/MCICLK/SDA1"/>
<pin name="P0.20/DTR1/SCL1"/>
<pin name="P0.21/RI1/CAN_RX1"/>
<pin name="P0.22/RTS1/CAN_TX1"/>
<pin name="P0.23/AD0.0/I2SRX_CLK/CAP3.0"/>
<pin name="P0.24/AD0.1/I2SRX_WS/CAP3.1"/>
<pin name="P0.25/AD0.2/I2SRX_SDA/TXD3"/>
<pin name="P0.26/AD0.3/AOUT/RXD3"/>
<pin name="P0.27/SDA0/USB_SDA"/>
<pin name="P0.28/SCL0/USB_SCL"/>
<pin name="P0.29/USB_D+"/>
<pin name="P0.30/USB_D-"/>
<pin name="P1.0/ENET-TXD0"/>
<pin name="P1.1/ENET-TXD1"/>
<pin name="P1.10/ENET_RXD1"/>
<pin name="P1.14/ENET-RX_ER"/>
<pin name="P1.15/ENET-RX_CLK"/>
<pin name="P1.16/ENET-MDC"/>
<pin name="P1.17/ENET-MDIO"/>
<pin name="P1.18/USB_UP/PWM1.1/CAP1.0"/>
<pin name="P1.19/MC0A/USB_PPWR/CAP1.1"/>
<pin name="P1.20/MCFB0/PWM1.2/SCK0"/>
<pin name="P1.21/MCABORT/PWM1.3/SSEL0"/>
<pin name="P1.22/MC0B/USB_PWRD/MAT1.0"/>
<pin name="P1.23/MCFB1/PWM1.4/MISO0"/>
<pin name="P1.24/MCFB2/PWM1.5/MOSI0"/>
<pin name="P1.25/MC1A/MAT1.1"/>
<pin name="P1.26/MC1B/PWM1.6/CAP0.0"/>
<pin name="P1.31/SCK1/AD0.5"/>
<pin name="P1.30/VBUS/AD0.4"/>
<pin name="P1.29/MC2B/PCAP1.1/MAT0.1"/>
<pin name="P1.28/MC2A/PCAP1.0/MAT0.0"/>
<pin name="P1.27/CLKOUT/USB_OVRCR/CAP0.1"/>
<pin name="P1.9/ENET_RXD0"/>
<pin name="P1.8/ENET_CRS"/>
<pin name="P1.4/ENET-TX_EN"/>
<pin name="P2.13/EINT3N/I2STX_SDA"/>
<pin name="P2.12/EINT2N/I2STX_WS"/>
<pin name="P2.11/EINT1N/I2STX_CLK"/>
<pin name="P2.10/EINT0N/NMI"/>
<pin name="P2.9/USB_CONNECT/RXD2"/>
<pin name="P2.8/CAN_TX2/TXD2"/>
<pin name="P2.7/CAN_RX2/RTS1"/>
<pin name="P2.6/PCAP1.0/RI1/TRACECLK"/>
<pin name="P2.5/PWM1.6/DTR1/TRACEDATA0"/>
<pin name="P2.4/PWM1.5/DSR1/TRACEDATA1"/>
<pin name="P2.3/PWM1.4/DCD1/TRACEDATA2"/>
<pin name="P2.2/PWM1.3/CTS1/TRACEDATA3"/>
<pin name="P2.1/PWM1.2/RXD1"/>
<pin name="P2.0/PWM1.1/TXD1/TRACECLK"/>
<pin name="P3.25/MAT0.0/PWM1.2"/>
<pin name="P3.26/STCLK/MAT0.1/PWM1.3"/>
<pin name="P4.28/RX_MCLK/MAT2.0/TXD3"/>
<pin name="P4.29/TX_MCLK/MAT2.1/RXD3"/>
<pin name="VSS@6"/>
<pin name="VSS@5"/>
<pin name="VSS@4"/>
<pin name="VSS@3"/>
<pin name="VSS@2"/>
<pin name="VSS@1"/>
<pin name="NC"/>
<pin name="VDD3.3V@1"/>
<pin name="VDD3.3V@2"/>
<pin name="VDD3.3V@3"/>
<pin name="VDD3.3V@4"/>
<pin name="VDDREG3.3V@2"/>
<pin name="VREFN"/>
<pin name="VBAT"/>
<pin name="X1"/>
<pin name="X2"/>
<pin name="VDDA"/>
<pin name="VREFP"/>
<pin name="VSSA"/>
<pin name="VDDREG3.3V@1"/>
<pin name="RTCX1"/>
<pin name="RTCX2"/>
<pin name="NRESET"/>
</symbol>
<symbol name="C">
<pin name="P$1" direction="pas"/>
<pin name="P$2" direction="pas"/>
</symbol>
<symbol name="R">
<pin name="P$1" direction="pas"/>
<pin name="P$2" direction="pas"/>
</symbol>
<symbol name="Q">
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
</symbol>
<symbol name="OSCILLATOR">
<pin name="CLK"/>
<pin name="EN"/>
<pin name="GND"/>
<pin name="VCC"/>
</symbol>
<symbol name="TS">
<pin name="P" direction="pas"/>
<pin name="S" direction="pas"/>
</symbol>
<symbol name="LED">
<pin name="C" direction="pas"/>
<pin name="A" direction="pas"/>
</symbol>
<symbol name="MK20DX128VFM5">
<pin name="VDD"/>
<pin name="VSS"/>
<pin name="USB_D+"/>
<pin name="USB_D-"/>
<pin name="VOUT33"/>
<pin name="VREGIN"/>
<pin name="VDDA"/>
<pin name="VSSA"/>
<pin name="NC3"/>
<pin name="NC2"/>
<pin name="NC4"/>
<pin name="XTALIN"/>
<pin name="XTALOUT"/>
<pin name="WAKE_NREQ"/>
<pin name="NRESET_FB_ISP"/>
<pin name="SLEEP_NREQ"/>
<pin name="NC1"/>
<pin name="NRESET_FB_BL"/>
<pin name="IF_NRESET"/>
<pin name="TGT_RX"/>
<pin name="TGT_TX"/>
<pin name="TGT_NRESET"/>
<pin name="NC5"/>
<pin name="NC6"/>
<pin name="NC7"/>
<pin name="TGT_SWCLK"/>
<pin name="TGT_SWDIO"/>
<pin name="LED_UART"/>
<pin name="LED_HID"/>
<pin name="TGT_SWO"/>
<pin name="LED_MSD"/>
<pin name="USB_VBUS"/>
<pin name="EPAD"/>
</symbol>
<symbol name="MKL25Z128VLK4">
<pin name="VDD1"/>
<pin name="VDD2"/>
<pin name="VDD3"/>
<pin name="VREFH"/>
<pin name="VDDA"/>
<pin name="VREGIN"/>
<pin name="NRESET"/>
<pin name="VOUT33"/>
<pin name="USB_D-"/>
<pin name="USB_D+"/>
<pin name="SWCLK"/>
<pin name="SWDIO"/>
<pin name="XTALIN"/>
<pin name="XTALOUT"/>
<pin name="PTE5"/>
<pin name="PTE4"/>
<pin name="PTE3"/>
<pin name="PTE2"/>
<pin name="PTE1"/>
<pin name="PTE0"/>
<pin name="VREFL"/>
<pin name="VSSA"/>
<pin name="VSS1"/>
<pin name="VSS2"/>
<pin name="VSS3"/>
<pin name="PTE29"/>
<pin name="PTE24"/>
<pin name="PTE25"/>
<pin name="PTE23"/>
<pin name="PTE22"/>
<pin name="PTE21"/>
<pin name="PTE20"/>
<pin name="PTA4"/>
<pin name="PTA5"/>
<pin name="PTD5"/>
<pin name="PTA2"/>
<pin name="PTA1"/>
<pin name="PTD0"/>
<pin name="PTE31"/>
<pin name="PTE30"/>
<pin name="PTC0"/>
<pin name="PTB19"/>
<pin name="PTB18"/>
<pin name="PTB17"/>
<pin name="PTB16"/>
<pin name="PTB11"/>
<pin name="PTB9"/>
<pin name="PTB10"/>
<pin name="PTB8"/>
<pin name="PTB3"/>
<pin name="PTB2"/>
<pin name="PTB1"/>
<pin name="PTD6"/>
<pin name="PTD7"/>
<pin name="PTA17"/>
<pin name="PTA16"/>
<pin name="PTA15"/>
<pin name="PTA14"/>
<pin name="PTA13"/>
<pin name="PTA12"/>
<pin name="PTD2"/>
<pin name="PTD1"/>
<pin name="PTC17"/>
<pin name="PTC16"/>
<pin name="PTD4"/>
<pin name="PTD3"/>
<pin name="PTC12"/>
<pin name="PTC13"/>
<pin name="PTC11"/>
<pin name="PTC10"/>
<pin name="PTC9"/>
<pin name="PTC8"/>
<pin name="PTC6"/>
<pin name="PTC7"/>
<pin name="PTC5"/>
<pin name="PTC4"/>
<pin name="PTC3"/>
<pin name="PTC2"/>
<pin name="PTC1"/>
<pin name="PTB0"/>
</symbol>
<symbol name="USB-1">
<pin name="D+"/>
<pin name="D-"/>
<pin name="GND"/>
<pin name="VBUS"/>
</symbol>
<symbol name="C-POL">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="+3.3V_IF">
<pin name="+3,3V" direction="sup"/>
</symbol>
<symbol name="+3.3V_TGT">
<pin name="+3,3V" direction="sup"/>
</symbol>
<symbol name="GND">
<pin name="GND" direction="sup"/>
</symbol>
<symbol name="+VIN">
<pin name="+VIN" direction="sup"/>
</symbol>
<symbol name="DP83848J">
<pin name="TX_CLK" direction="out"/>
<pin name="TX_EN" direction="in"/>
<pin name="TXD_0" direction="in"/>
<pin name="TXD_1" direction="in"/>
<pin name="TXD_2"/>
<pin name="TXD_3"/>
<pin name="RESERVED@1" direction="nc"/>
<pin name="RESERVED@2" direction="nc"/>
<pin name="RESERVED@3" direction="nc"/>
<pin name="RD-"/>
<pin name="RD+"/>
<pin name="AGND@1" direction="pwr"/>
<pin name="TD-"/>
<pin name="TD+"/>
<pin name="PFBIN1" direction="pas"/>
<pin name="AGND@2" direction="pwr"/>
<pin name="AVDD33" direction="pwr"/>
<pin name="PFBOUT" direction="pas"/>
<pin name="RBIAS" direction="pas"/>
<pin name="LED_SPEED/AN1" direction="out"/>
<pin name="LED_LINK/AN0" direction="out"/>
<pin name="RESET_N" direction="in"/>
<pin name="MDIO"/>
<pin name="MDC" direction="in"/>
<pin name="IOVDD33@1" direction="pwr"/>
<pin name="X2" direction="pas"/>
<pin name="X1" direction="pas"/>
<pin name="DGND" direction="pwr"/>
<pin name="PFBIN2" direction="pas"/>
<pin name="RX_CLK" direction="out"/>
<pin name="RX_DV/MII_MODE" direction="out"/>
<pin name="CRS/CRS_DV/LED_CFG" direction="out"/>
<pin name="RX_ER/MDIX_EN" direction="out"/>
<pin name="COL/PHYAD0" direction="out"/>
<pin name="RXD_0/PHYAD1" direction="out"/>
<pin name="RXD_1/PHYAD2" direction="out"/>
<pin name="RXD_2/PHYAD3" direction="out"/>
<pin name="RXD_3/PHYAD4" direction="out"/>
<pin name="IOGND@2" direction="pwr"/>
<pin name="IOVDD33@2" direction="pwr"/>
<pin name="GNDPAD" direction="pwr"/>
</symbol>
<symbol name="RJ45">
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="SHIELD1"/>
<pin name="SHIELD2"/>
</symbol>
<symbol name="L">
<pin name="P$1"/>
<pin name="P$2"/>
</symbol>
<symbol name="LPC812M101FD20-1">
<pin name="!RESET!/PIO0_5"/>
<pin name="PIO0_4/WAKEUP/!TRST!"/>
<pin name="SWCLK/PIO0_3/TCK"/>
<pin name="SWDIO/PIO0_2/TMS"/>
<pin name="PIO0_0/ACMP_I1/TDO"/>
<pin name="VDD" direction="pwr"/>
<pin name="VSS" direction="pwr"/>
<pin name="PIO0_1/ACMP_I2/CLKIN/TDI"/>
<pin name="PIO0_13"/>
<pin name="PIO0_12"/>
<pin name="PIO0_11"/>
<pin name="PIO0_10"/>
<pin name="PIO0_8/XTALIN"/>
<pin name="PIO0_9/XTALOUT"/>
<pin name="PIO0_7"/>
<pin name="PIO0_6/VDDCMP"/>
<pin name="PIO0_17"/>
<pin name="PIO0_16"/>
<pin name="PIO0_15"/>
<pin name="PIO0_14"/>
</symbol>
<symbol name="LPC1347FBD48">
<pin name="PIO1_19/!DTR!/SSEL1"/>
<pin name="!RESET!/PIO0_0"/>
<pin name="PIO0_1/CLKOUT/CT32B0_MAT2/USB_FTOGGLE"/>
<pin name="XTALIN" direction="in"/>
<pin name="XTALOUT" direction="out"/>
<pin name="PIO0_20/CT16B1_CAP0"/>
<pin name="PIO0_2/SSEL0/CT16B0_CAP0"/>
<pin name="PIO1_20/!DSR!/SCK1"/>
<pin name="PIO0_3/USB_VBUS"/>
<pin name="PIO0_4/SCL"/>
<pin name="PIO0_5/SDA"/>
<pin name="PIO0_21/CT16B1_MAT0/MOSI1"/>
<pin name="PIO0_6/!USB_CONNECT!/SCK0"/>
<pin name="PIO0_7/!CTS!"/>
<pin name="PIO1_21/!DCD!/MISO1"/>
<pin name="PIO0_8/MISO0/CT16B0_MAT0"/>
<pin name="PIO0_9/MOSI0/CT16B0_MAT1/SWO"/>
<pin name="SWCLK/PIO0_10/SCK0/CT16B0_MAT2"/>
<pin name="PIO0_22/AD6/CT16B1_MAT1/MISO1"/>
<pin name="TDI/PIO0_11/AD0/CT32B0_MAT3"/>
<pin name="TMS/PIO0_12/AD1/CT32B1_CAP0"/>
<pin name="TDO/PIO0_13/AD2/CT32B1_MAT0"/>
<pin name="!TRST!/PIO0_14/AD3/CT32B1_MAT1"/>
<pin name="PIO1_22/!RI!/MOSI1"/>
<pin name="SWDIO/PIO0_15/AD4/CT32B1_MAT2"/>
<pin name="PIO0_16/AD5/CT32B1_MAT3/WAKEUP"/>
<pin name="VSS" direction="pwr"/>
<pin name="PIO0_23/AD7"/>
<pin name="VDD" direction="pwr"/>
<pin name="PIO0_17/!RTS!/CT32B0_CAP0/SCLK"/>
<pin name="PIO0_18/RXD/CT32B0_MAT0"/>
<pin name="PIO0_19/TXD/CT32B0_MAT1"/>
<pin name="PIO1_13/!DTR!/CT16B0_MAT0/TXD"/>
<pin name="PIO1_14/!DSR!/CT16B0_MAT1/RXD"/>
<pin name="PIO1_15/!DCD!/CT16B0_MAT2/SCK1"/>
<pin name="PIO1_16/!RI!/CT16B0_CAP0"/>
<pin name="PIO1_23/CT16B1_MAT1/SSEL1"/>
<pin name="PIO1_24/CT32B0_MAT0"/>
<pin name="PIO1_25/CT32B0_MAT1"/>
<pin name="PIO1_26/CT32B0_MAT2/RXD"/>
<pin name="PIO1_27/CT32B0_MAT3/TXD"/>
<pin name="PIO1_28/CT32B0_CAP0/SCLK"/>
<pin name="PIO1_29/SCK0/CT32B0_CAP1"/>
<pin name="PIO1_31"/>
<pin name="USB_DM"/>
<pin name="USB_DP"/>
</symbol>
<symbol name="LPC1347FBD64">
<pin name="PIO1_19/!DTR!/SSEL1"/>
<pin name="!RESET!/PIO0_0"/>
<pin name="PIO0_1/CLKOUT/CT32B0_MAT2/USB_FTOGGLE"/>
<pin name="XTALIN" direction="in"/>
<pin name="XTALOUT" direction="out"/>
<pin name="PIO0_20/CT16B1_CAP0"/>
<pin name="PIO0_2/SSEL0/CT16B0_CAP0"/>
<pin name="PIO1_20/!DSR!/SCK1"/>
<pin name="PIO0_3/USB_VBUS"/>
<pin name="PIO0_4/SCL"/>
<pin name="PIO0_5/SDA"/>
<pin name="PIO0_21/CT16B1_MAT0/MOSI1"/>
<pin name="PIO1_0/CT32B1_MAT0"/>
<pin name="PIO0_6/!USB_CONNECT!/SCK0"/>
<pin name="PIO0_7/!CTS!"/>
<pin name="PIO1_21/!DCD!/MISO1"/>
<pin name="PIO0_8/MISO0/CT16B0_MAT0"/>
<pin name="PIO0_9/MOSI0/CT16B0_MAT1/SWO"/>
<pin name="SWCLK/PIO0_10/SCK0/CT16B0_MAT2"/>
<pin name="PIO0_22/AD6/CT16B1_MAT1/MISO1"/>
<pin name="TDI/PIO0_11/AD0/CT32B0_MAT3"/>
<pin name="TMS/PIO0_12/AD1/CT32B1_CAP0"/>
<pin name="TDO/PIO0_13/AD2/CT32B1_MAT0"/>
<pin name="!TRST!/PIO0_14/AD3/CT32B1_MAT1"/>
<pin name="PIO1_22/!RI!/MOSI1"/>
<pin name="SWDIO/PIO0_15/AD4/CT32B1_MAT2"/>
<pin name="PIO0_16/AD5/CT32B1_MAT3/WAKEUP"/>
<pin name="VSS" direction="pwr"/>
<pin name="PIO0_23/AD7"/>
<pin name="VDD" direction="pwr"/>
<pin name="PIO0_17/!RTS!/CT32B0_CAP0/SCLK"/>
<pin name="PIO0_18/RXD/CT32B0_MAT0"/>
<pin name="PIO0_19/TXD/CT32B0_MAT1"/>
<pin name="PIO1_1/CT32B1_MAT1"/>
<pin name="PIO1_2/CT32B1_MAT2"/>
<pin name="PIO1_3/CT32B1_MAT3"/>
<pin name="PIO1_4/CT32B1_CAP0"/>
<pin name="PIO1_5/CT32B1_CAP1"/>
<pin name="PIO1_7"/>
<pin name="PIO1_8"/>
<pin name="PIO1_10"/>
<pin name="PIO1_11"/>
<pin name="PIO1_13/!DTR!/CT16B0_MAT0/TXD"/>
<pin name="PIO1_14/!DSR!/CT16B0_MAT1/RXD"/>
<pin name="PIO1_15/!DCD!/CT16B0_MAT2/SCK1"/>
<pin name="PIO1_16/!RI!/CT16B0_CAP0"/>
<pin name="PIO1_17/CT16B0_CAP1/RXD"/>
<pin name="PIO1_18/CT16B1_CAP1/TXD"/>
<pin name="PIO1_23/CT16B1_MAT1/SSEL1"/>
<pin name="PIO1_24/CT32B0_MAT0"/>
<pin name="PIO1_25/CT32B0_MAT1"/>
<pin name="PIO1_26/CT32B0_MAT2/RXD"/>
<pin name="PIO1_27/CT32B0_MAT3/TXD"/>
<pin name="PIO1_28/CT32B0_CAP0/SCLK"/>
<pin name="PIO1_29/SCK0/CT32B0_CAP1"/>
<pin name="VDDA" direction="pwr"/>
<pin name="VREFP" direction="pwr"/>
<pin name="VSSA" direction="pwr"/>
<pin name="VREFN" direction="pwr"/>
<pin name="USB_DM"/>
<pin name="USB_DP"/>
</symbol>
<symbol name="LPC40X8FYY208">
<pin name="P0[0]"/>
<pin name="P0[1]"/>
<pin name="P0[2]"/>
<pin name="P0[3]"/>
<pin name="P0[4]"/>
<pin name="P0[5]"/>
<pin name="P0[6]"/>
<pin name="P0[7]"/>
<pin name="P0[8]"/>
<pin name="P0[9]"/>
<pin name="P0[10]"/>
<pin name="P0[11]"/>
<pin name="P0[12]"/>
<pin name="P0[13]"/>
<pin name="P0[14]"/>
<pin name="P0[15]"/>
<pin name="P0[16]"/>
<pin name="P0[17]"/>
<pin name="P0[18]"/>
<pin name="P0[19]"/>
<pin name="P0[20]"/>
<pin name="P0[21]"/>
<pin name="P0[22]"/>
<pin name="P0[23]"/>
<pin name="P0[24]"/>
<pin name="P0[25]"/>
<pin name="P0[26]"/>
<pin name="P0[27]"/>
<pin name="P0[28]"/>
<pin name="P0[29]"/>
<pin name="P0[30]"/>
<pin name="P0[31]"/>
<pin name="P1[0]"/>
<pin name="P1[1]"/>
<pin name="P1[2]"/>
<pin name="P1[3]"/>
<pin name="P1[4]"/>
<pin name="P1[5]"/>
<pin name="P1[6]"/>
<pin name="P1[7]"/>
<pin name="P1[8]"/>
<pin name="P1[9]"/>
<pin name="P1[10]"/>
<pin name="P1[11]"/>
<pin name="P1[12]"/>
<pin name="P1[13]"/>
<pin name="P1[14]"/>
<pin name="P1[15]"/>
<pin name="P1[16]"/>
<pin name="P1[17]"/>
<pin name="P1[18]"/>
<pin name="P1[19]"/>
<pin name="P1[20]"/>
<pin name="P1[21]"/>
<pin name="P1[22]"/>
<pin name="P1[23]"/>
<pin name="P1[24]"/>
<pin name="P1[25]"/>
<pin name="P1[26]"/>
<pin name="P1[27]"/>
<pin name="P1[28]"/>
<pin name="P1[29]"/>
<pin name="P1[30]"/>
<pin name="P1[31]"/>
<pin name="P2[0]"/>
<pin name="P2[1]"/>
<pin name="P2[2]"/>
<pin name="P2[3]"/>
<pin name="P2[4]"/>
<pin name="P2[5]"/>
<pin name="P2[6]"/>
<pin name="P2[7]"/>
<pin name="P2[8]"/>
<pin name="P2[9]"/>
<pin name="P2[10]"/>
<pin name="P2[11]"/>
<pin name="P2[12]"/>
<pin name="P2[13]"/>
<pin name="P2[14]"/>
<pin name="P2[15]"/>
<pin name="P2[16]"/>
<pin name="P2[17]"/>
<pin name="P2[18]"/>
<pin name="P2[19]"/>
<pin name="P2[20]"/>
<pin name="P2[21]"/>
<pin name="P2[22]"/>
<pin name="P2[23]"/>
<pin name="P2[24]"/>
<pin name="P2[25]"/>
<pin name="P2[26]"/>
<pin name="P2[27]"/>
<pin name="P2[28]"/>
<pin name="P2[29]"/>
<pin name="P2[30]"/>
<pin name="P2[31]"/>
<pin name="P3[0]"/>
<pin name="P3[1]"/>
<pin name="P3[2]"/>
<pin name="P3[3]"/>
<pin name="P3[4]"/>
<pin name="P3[5]"/>
<pin name="P3[6]"/>
<pin name="P3[7]"/>
<pin name="P3[8]"/>
<pin name="P3[9]"/>
<pin name="P3[10]"/>
<pin name="P3[11]"/>
<pin name="P3[12]"/>
<pin name="P3[13]"/>
<pin name="P3[14]"/>
<pin name="P3[15]"/>
<pin name="P3[16]"/>
<pin name="P3[17]"/>
<pin name="P3[18]"/>
<pin name="P3[19]"/>
<pin name="P3[20]"/>
<pin name="P3[21]"/>
<pin name="P3[22]"/>
<pin name="P3[23]"/>
<pin name="P3[24]"/>
<pin name="P3[25]"/>
<pin name="P3[26]"/>
<pin name="P3[27]"/>
<pin name="P3[28]"/>
<pin name="P3[29]"/>
<pin name="P3[30]"/>
<pin name="P3[31]"/>
<pin name="P4[0]"/>
<pin name="P4[1]"/>
<pin name="P4[2]"/>
<pin name="P4[3]"/>
<pin name="P4[4]"/>
<pin name="P4[5]"/>
<pin name="P4[6]"/>
<pin name="P4[7]"/>
<pin name="P4[8]"/>
<pin name="P4[9]"/>
<pin name="P4[10]"/>
<pin name="P4[11]"/>
<pin name="P4[12]"/>
<pin name="P4[13]"/>
<pin name="P4[14]"/>
<pin name="P4[15]"/>
<pin name="P4[16]"/>
<pin name="P4[17]"/>
<pin name="P4[18]"/>
<pin name="P4[19]"/>
<pin name="P4[20]"/>
<pin name="P4[21]"/>
<pin name="P4[22]"/>
<pin name="P4[23]"/>
<pin name="P4[24]"/>
<pin name="P4[25]"/>
<pin name="P4[26]"/>
<pin name="P4[27]"/>
<pin name="P4[28]"/>
<pin name="P4[29]"/>
<pin name="P4[30]"/>
<pin name="P4[31]"/>
<pin name="P5[0]"/>
<pin name="P5[1]"/>
<pin name="P5[2]"/>
<pin name="P5[3]"/>
<pin name="P5[4]"/>
<pin name="JTAG_TDO/SWO" direction="out"/>
<pin name="JTAG_TDI" direction="in"/>
<pin name="JTAG_TMS/SWDIO" direction="in"/>
<pin name="JTAG_!TRST" direction="in"/>
<pin name="!RESET!" direction="in"/>
<pin name="!RSTOUT!" direction="out"/>
<pin name="RTC_ALARM" direction="out"/>
<pin name="RTCX1" direction="in"/>
<pin name="RTCX2" direction="out"/>
<pin name="USB_D-2"/>
<pin name="VBAT" direction="pwr"/>
<pin name="VDD(REG)(3V3)" direction="pwr"/>
<pin name="VDDA" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="VREFP" direction="pwr"/>
<pin name="VSS" direction="pwr"/>
<pin name="VSSREG" direction="pwr"/>
<pin name="VSSA" direction="pwr"/>
<pin name="XTAL1" direction="in"/>
<pin name="XTAL2" direction="out"/>
<pin name="JTAG_TCK/SWDCLK" direction="in"/>
</symbol>
<symbol name="LPC1112FDH28">
<pin name="RESET/PIO0_0"/>
<pin name="PIO0_1/CLKOUT/CT32B0_MAT2"/>
<pin name="XTALIN" direction="in"/>
<pin name="XTALOUT" direction="out"/>
<pin name="VDDA" direction="pwr"/>
<pin name="PIO1_8/CT16B1_CAP0"/>
<pin name="PIO0_2/SSEL/CT16B0_CAP0"/>
<pin name="PIO0_3"/>
<pin name="PIO0_4/SCL"/>
<pin name="PIO0_5/SDA"/>
<pin name="PIO1_9/CT16B1_MAT0"/>
<pin name="PIO0_6/SCK0"/>
<pin name="PIO0_7/!CTS!"/>
<pin name="PIO0_8/MISO0/CT16B0_MAT0"/>
<pin name="PIO0_9/MOSI0/CT16B0_MAT1"/>
<pin name="SWCLK/PIO0_10/SCK0/CT16B0_MAT2"/>
<pin name="TDI/PIO0_11/AD0/CT32B0_MAT3"/>
<pin name="TMS/PIO1_0/AD1/CT32B1_CAP0"/>
<pin name="TDO/PIO1_1/AD2/CT32B1_MAT0"/>
<pin name="TRST/PIO1_2/AD3/CT32B1_MAT1"/>
<pin name="SWDIO/PIO1_3/AD4/CT32B1_MAT2"/>
<pin name="PIO1_4/AD5/CT32B1_MAT3/WAKEUP"/>
<pin name="VDD" direction="pwr"/>
<pin name="PIO1_5/!RTS!/CT32B0_CAP0"/>
<pin name="PIO1_6/RXD/CT32B0_MAT0"/>
<pin name="PIO1_7/TXD/CT32B0_MAT1"/>
<pin name="VSS" direction="pwr"/>
<pin name="VSSA" direction="pwr"/>
</symbol>
<symbol name="IF-LPC11U35">
<pin name="IF_NRESET"/>
<pin name="LED_HID"/>
<pin name="LED_MSD"/>
<pin name="LED_UART"/>
<pin name="NC2"/>
<pin name="NC3"/>
<pin name="NC4"/>
<pin name="NC5"/>
<pin name="NC6"/>
<pin name="NC7"/>
<pin name="NC8"/>
<pin name="NC9"/>
<pin name="NC10"/>
<pin name="NC11"/>
<pin name="NRESET_FB_BL"/>
<pin name="NRESET_FB_ISP"/>
<pin name="SLEEP_NREQ"/>
<pin name="TGT_NRESET"/>
<pin name="TGT_RX"/>
<pin name="TGT_SWCLK"/>
<pin name="TGT_SWDIO"/>
<pin name="TGT_SWO"/>
<pin name="TGT_TX"/>
<pin name="USB_D+"/>
<pin name="USB_D-"/>
<pin name="USB_SCON"/>
<pin name="USB_VBUS"/>
<pin name="VDD1"/>
<pin name="VDD2"/>
<pin name="VSS"/>
<pin name="WAKE_NREQ"/>
<pin name="XTALIN"/>
<pin name="XTALOUT"/>
</symbol>
<symbol name="74125">
<pin name="OE" direction="in"/>
<pin name="I" direction="in"/>
<pin name="O" direction="hiz"/>
</symbol>
<symbol name="PWRN">
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
</symbol>
<symbol name="+3.3V">
<pin name="+3,3V" direction="sup"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="SWD-10" prefix="CON">
<gates>
<gate name="G$1" symbol="SWD-10"/>
</gates>
<devices>
<device name="_TC" package="SWD-10-TAGCONNECT">
<connects>
<connect gate="G$1" pin="P$1" pad="P$1"/>
<connect gate="G$1" pin="P$10" pad="P$10"/>
<connect gate="G$1" pin="P$2" pad="P$2"/>
<connect gate="G$1" pin="P$3" pad="P$3"/>
<connect gate="G$1" pin="P$4" pad="P$4"/>
<connect gate="G$1" pin="P$5" pad="P$5"/>
<connect gate="G$1" pin="P$6" pad="P$6"/>
<connect gate="G$1" pin="P$7" pad="P$7"/>
<connect gate="G$1" pin="P$8" pad="P$8"/>
<connect gate="G$1" pin="P$9" pad="P$9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_SMD" package="SWD-10-SMD">
<connects>
<connect gate="G$1" pin="P$1" pad="P$1"/>
<connect gate="G$1" pin="P$10" pad="P$10"/>
<connect gate="G$1" pin="P$2" pad="P$2"/>
<connect gate="G$1" pin="P$3" pad="P$3"/>
<connect gate="G$1" pin="P$4" pad="P$4"/>
<connect gate="G$1" pin="P$5" pad="P$5"/>
<connect gate="G$1" pin="P$6" pad="P$6"/>
<connect gate="G$1" pin="P$7" pad="P$7"/>
<connect gate="G$1" pin="P$8" pad="P$8"/>
<connect gate="G$1" pin="P$9" pad="P$9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_PTH" package="SWD-10-PTH">
<connects>
<connect gate="G$1" pin="P$1" pad="1"/>
<connect gate="G$1" pin="P$10" pad="10"/>
<connect gate="G$1" pin="P$2" pad="2"/>
<connect gate="G$1" pin="P$3" pad="3"/>
<connect gate="G$1" pin="P$4" pad="4"/>
<connect gate="G$1" pin="P$5" pad="5"/>
<connect gate="G$1" pin="P$6" pad="6"/>
<connect gate="G$1" pin="P$7" pad="7"/>
<connect gate="G$1" pin="P$8" pad="8"/>
<connect gate="G$1" pin="P$9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BAT60A" prefix="D">
<description>&lt;b&gt;Schottky Diode&lt;/b&gt;&lt;p&gt;</description>
<gates>
<gate name="G$1" symbol="BAT60A"/>
</gates>
<devices>
<device name="" package="BAT60A">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="K" pad="K"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BSS84" prefix="T">
<description>&lt;b&gt;P-CHANNEL MOS FET&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="P-MOS"/>
</gates>
<devices>
<device name="" package="SOT23">
<connects>
<connect gate="G$1" pin="D" pad="3"/>
<connect gate="G$1" pin="G" pad="1"/>
<connect gate="G$1" pin="S" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MBED_HDK">
<gates>
<gate name="G$1" symbol="MBED_HDK"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MBED-ENABLED-LOGO" prefix="SS">
<gates>
<gate name="G$1" symbol="MBED-ENABLED-LOGO"/>
</gates>
<devices>
<device name="SMALL" package="MBED-ENABLED-LOGO-250X250-MIL">
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="MEDIUM" package="MBED-ENABLED-LOGO-500X500-MIL">
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LARGE" package="MBED-ENABLED-LOGO-1000X1000-MIL">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CE-MARK" prefix="SS">
<gates>
<gate name="G$1" symbol="CE-MARK"/>
</gates>
<devices>
<device name="" package="CE-MARK-0.2">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PB-MARK" prefix="SS">
<gates>
<gate name="G$1" symbol="PB-FREE"/>
</gates>
<devices>
<device name="" package="PB-MARK-0.2">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LD1117S33" prefix="IC">
<description>VOLTAGE REGULATOR SMD 3,3V</description>
<gates>
<gate name="G$1" symbol="LD1117S33"/>
</gates>
<devices>
<device name="" package="SOT223">
<connects>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="IN" pad="3"/>
<connect gate="G$1" pin="K" pad="4"/>
<connect gate="G$1" pin="OUT" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LPC11U24" prefix="IC">
<description>NXP Cortex-M0 Micrcontroller</description>
<gates>
<gate name="G$1" symbol="LPC11U24"/>
</gates>
<devices>
<device name="" package="MBED-ICS_LQFP64">
<connects>
<connect gate="G$1" pin="NTRST/PIO0.14/AD3/CT32B1M1" pad="46"/>
<connect gate="G$1" pin="PIO0.0/NRESET" pad="4"/>
<connect gate="G$1" pin="PIO0.1/CLKOUT/CT32B0M2/USB_FTOG" pad="5"/>
<connect gate="G$1" pin="PIO0.16/AD5/CT32B1M3/WAKEUP" pad="53"/>
<connect gate="G$1" pin="PIO0.17/RTS/CT32B0C0/SCLK" pad="60"/>
<connect gate="G$1" pin="PIO0.18/RXD/CT32B0M0" pad="61"/>
<connect gate="G$1" pin="PIO0.19/TXD/CT32B0M1" pad="62"/>
<connect gate="G$1" pin="PIO0.2/SSEL0/CT16B0C0" pad="13"/>
<connect gate="G$1" pin="PIO0.20/CT16B1C0" pad="11"/>
<connect gate="G$1" pin="PIO0.21/CT16B1M0/MOSI1" pad="22"/>
<connect gate="G$1" pin="PIO0.22/AD6/CT16B1M1/MISO1" pad="40"/>
<connect gate="G$1" pin="PIO0.23/AD7" pad="56"/>
<connect gate="G$1" pin="PIO0.3/USB_VBUS" pad="19"/>
<connect gate="G$1" pin="PIO0.4/SCL(OD)" pad="20"/>
<connect gate="G$1" pin="PIO0.5/SDA(OD)" pad="21"/>
<connect gate="G$1" pin="PIO0.6/USB_CON/SCK0" pad="29"/>
<connect gate="G$1" pin="PIO0.7/CTS" pad="30"/>
<connect gate="G$1" pin="PIO0.8/MISO0/CT16B0M0" pad="36"/>
<connect gate="G$1" pin="PIO0.9/MOSI0/CT16B0M1" pad="37"/>
<connect gate="G$1" pin="PIO1.0/CT32B1M0" pad="1"/>
<connect gate="G$1" pin="PIO1.1/CT32B1M1" pad="17"/>
<connect gate="G$1" pin="PIO1.10" pad="12"/>
<connect gate="G$1" pin="PIO1.11" pad="43"/>
<connect gate="G$1" pin="PIO1.12" pad="59"/>
<connect gate="G$1" pin="PIO1.13/DTR/CT16B0M1/TXD" pad="47"/>
<connect gate="G$1" pin="PIO1.14/DSR/CT16B0M1/RXD" pad="49"/>
<connect gate="G$1" pin="PIO1.15/DCD/CT16B0M2/SCK1" pad="57"/>
<connect gate="G$1" pin="PIO1.16/RI/CT16B0C0" pad="63"/>
<connect gate="G$1" pin="PIO1.17/CT16B0C1/RXD" pad="23"/>
<connect gate="G$1" pin="PIO1.18/CT16B1C1/TXD" pad="28"/>
<connect gate="G$1" pin="PIO1.19/DTR/SSEL1" pad="3"/>
<connect gate="G$1" pin="PIO1.2/CT32B1M2" pad="34"/>
<connect gate="G$1" pin="PIO1.20/DSR/SCK1" pad="18"/>
<connect gate="G$1" pin="PIO1.21/DCD/MISO1" pad="35"/>
<connect gate="G$1" pin="PIO1.22/RI/MOSI1" pad="51"/>
<connect gate="G$1" pin="PIO1.23/CT16B1M1/SSEL1" pad="24"/>
<connect gate="G$1" pin="PIO1.24/CT32B0M0" pad="27"/>
<connect gate="G$1" pin="PIO1.25/CT32B0M1" pad="2"/>
<connect gate="G$1" pin="PIO1.26/CT32B0M2/RXD" pad="14"/>
<connect gate="G$1" pin="PIO1.27/CT32B0M3/TXD" pad="15"/>
<connect gate="G$1" pin="PIO1.28/CT32B0C0/SCLK" pad="31"/>
<connect gate="G$1" pin="PIO1.29/SCK0/CT32B0C1" pad="41"/>
<connect gate="G$1" pin="PIO1.3/CT32B1M3" pad="50"/>
<connect gate="G$1" pin="PIO1.4/CT32B1C0" pad="16"/>
<connect gate="G$1" pin="PIO1.5/CT32B1C1" pad="32"/>
<connect gate="G$1" pin="PIO1.6" pad="64"/>
<connect gate="G$1" pin="PIO1.7" pad="6"/>
<connect gate="G$1" pin="PIO1.8" pad="39"/>
<connect gate="G$1" pin="PIO1.9" pad="55"/>
<connect gate="G$1" pin="SWCLK/PIO0.10/SCK0/CT16B0M2" pad="38"/>
<connect gate="G$1" pin="SWDIO/PIO0.15/AD4/CT32B1M2" pad="52"/>
<connect gate="G$1" pin="TDI/PIO0.11/AD0/CT32B0M3" pad="42"/>
<connect gate="G$1" pin="TDO/PIO0.13/AD2/CB32B1M0" pad="45"/>
<connect gate="G$1" pin="TMS/PIO0.12/AD1/CT32B1M0" pad="44"/>
<connect gate="G$1" pin="USB_D+" pad="26"/>
<connect gate="G$1" pin="USB_D-" pad="25"/>
<connect gate="G$1" pin="VDD@10" pad="10"/>
<connect gate="G$1" pin="VDD@33" pad="33"/>
<connect gate="G$1" pin="VDD@48" pad="48"/>
<connect gate="G$1" pin="VDD@58" pad="58"/>
<connect gate="G$1" pin="VSS@54" pad="54"/>
<connect gate="G$1" pin="VSS@7" pad="7"/>
<connect gate="G$1" pin="XTALIN" pad="8"/>
<connect gate="G$1" pin="XTALOUT" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LPC1768" prefix="IC">
<gates>
<gate name="G$1" symbol="LPC1768"/>
</gates>
<devices>
<device name="" package="LQFP100">
<connects>
<connect gate="G$1" pin="NC" pad="13"/>
<connect gate="G$1" pin="NRESET" pad="17"/>
<connect gate="G$1" pin="P0.0/CAN_RX1/TXD3/SDA1" pad="46"/>
<connect gate="G$1" pin="P0.1/CAN_TX1/RXD3/SCL1" pad="47"/>
<connect gate="G$1" pin="P0.10/TXD2/SDA2/MAT3.0" pad="48"/>
<connect gate="G$1" pin="P0.11/RXD2/SCL2/MAT3.1" pad="49"/>
<connect gate="G$1" pin="P0.15/TXD1/SCK0/SCK" pad="62"/>
<connect gate="G$1" pin="P0.16/RXD1/SSEL0/SSEL" pad="63"/>
<connect gate="G$1" pin="P0.17/CTS1/MISO0/MISO" pad="61"/>
<connect gate="G$1" pin="P0.18/DCD1/MOSI0/MOSI1" pad="60"/>
<connect gate="G$1" pin="P0.19/DSR1/MCICLK/SDA1" pad="59"/>
<connect gate="G$1" pin="P0.2/TXD0/AD0.7" pad="98"/>
<connect gate="G$1" pin="P0.20/DTR1/SCL1" pad="58"/>
<connect gate="G$1" pin="P0.21/RI1/CAN_RX1" pad="57"/>
<connect gate="G$1" pin="P0.22/RTS1/CAN_TX1" pad="56"/>
<connect gate="G$1" pin="P0.23/AD0.0/I2SRX_CLK/CAP3.0" pad="9"/>
<connect gate="G$1" pin="P0.24/AD0.1/I2SRX_WS/CAP3.1" pad="8"/>
<connect gate="G$1" pin="P0.25/AD0.2/I2SRX_SDA/TXD3" pad="7"/>
<connect gate="G$1" pin="P0.26/AD0.3/AOUT/RXD3" pad="6"/>
<connect gate="G$1" pin="P0.27/SDA0/USB_SDA" pad="25"/>
<connect gate="G$1" pin="P0.28/SCL0/USB_SCL" pad="24"/>
<connect gate="G$1" pin="P0.29/USB_D+" pad="29"/>
<connect gate="G$1" pin="P0.3/RXD0/AD0.6" pad="99"/>
<connect gate="G$1" pin="P0.30/USB_D-" pad="30"/>
<connect gate="G$1" pin="P0.4/I2SRX_CLK/CAN_RX2/CAP2.0" pad="81"/>
<connect gate="G$1" pin="P0.5/I2SRX_WS/CAN_TX2/CAP2.1" pad="80"/>
<connect gate="G$1" pin="P0.6/I2SRX_SDA/SSEL1/MAT2.0" pad="79"/>
<connect gate="G$1" pin="P0.7/I2STX_CLK/SCK1/MAT2.1" pad="78"/>
<connect gate="G$1" pin="P0.8/I2STX_WS/MISO1/MAT2.2" pad="77"/>
<connect gate="G$1" pin="P0.9/I2STX_SDA/MOSI1/MAT2.3" pad="76"/>
<connect gate="G$1" pin="P1.0/ENET-TXD0" pad="95"/>
<connect gate="G$1" pin="P1.1/ENET-TXD1" pad="94"/>
<connect gate="G$1" pin="P1.10/ENET_RXD1" pad="90"/>
<connect gate="G$1" pin="P1.14/ENET-RX_ER" pad="89"/>
<connect gate="G$1" pin="P1.15/ENET-RX_CLK" pad="88"/>
<connect gate="G$1" pin="P1.16/ENET-MDC" pad="87"/>
<connect gate="G$1" pin="P1.17/ENET-MDIO" pad="86"/>
<connect gate="G$1" pin="P1.18/USB_UP/PWM1.1/CAP1.0" pad="32"/>
<connect gate="G$1" pin="P1.19/MC0A/USB_PPWR/CAP1.1" pad="33"/>
<connect gate="G$1" pin="P1.20/MCFB0/PWM1.2/SCK0" pad="34"/>
<connect gate="G$1" pin="P1.21/MCABORT/PWM1.3/SSEL0" pad="35"/>
<connect gate="G$1" pin="P1.22/MC0B/USB_PWRD/MAT1.0" pad="36"/>
<connect gate="G$1" pin="P1.23/MCFB1/PWM1.4/MISO0" pad="37"/>
<connect gate="G$1" pin="P1.24/MCFB2/PWM1.5/MOSI0" pad="38"/>
<connect gate="G$1" pin="P1.25/MC1A/MAT1.1" pad="39"/>
<connect gate="G$1" pin="P1.26/MC1B/PWM1.6/CAP0.0" pad="40"/>
<connect gate="G$1" pin="P1.27/CLKOUT/USB_OVRCR/CAP0.1" pad="43"/>
<connect gate="G$1" pin="P1.28/MC2A/PCAP1.0/MAT0.0" pad="44"/>
<connect gate="G$1" pin="P1.29/MC2B/PCAP1.1/MAT0.1" pad="45"/>
<connect gate="G$1" pin="P1.30/VBUS/AD0.4" pad="21"/>
<connect gate="G$1" pin="P1.31/SCK1/AD0.5" pad="20"/>
<connect gate="G$1" pin="P1.4/ENET-TX_EN" pad="93"/>
<connect gate="G$1" pin="P1.8/ENET_CRS" pad="92"/>
<connect gate="G$1" pin="P1.9/ENET_RXD0" pad="91"/>
<connect gate="G$1" pin="P2.0/PWM1.1/TXD1/TRACECLK" pad="75"/>
<connect gate="G$1" pin="P2.1/PWM1.2/RXD1" pad="74"/>
<connect gate="G$1" pin="P2.10/EINT0N/NMI" pad="53"/>
<connect gate="G$1" pin="P2.11/EINT1N/I2STX_CLK" pad="52"/>
<connect gate="G$1" pin="P2.12/EINT2N/I2STX_WS" pad="51"/>
<connect gate="G$1" pin="P2.13/EINT3N/I2STX_SDA" pad="50"/>
<connect gate="G$1" pin="P2.2/PWM1.3/CTS1/TRACEDATA3" pad="73"/>
<connect gate="G$1" pin="P2.3/PWM1.4/DCD1/TRACEDATA2" pad="70"/>
<connect gate="G$1" pin="P2.4/PWM1.5/DSR1/TRACEDATA1" pad="69"/>
<connect gate="G$1" pin="P2.5/PWM1.6/DTR1/TRACEDATA0" pad="68"/>
<connect gate="G$1" pin="P2.6/PCAP1.0/RI1/TRACECLK" pad="67"/>
<connect gate="G$1" pin="P2.7/CAN_RX2/RTS1" pad="66"/>
<connect gate="G$1" pin="P2.8/CAN_TX2/TXD2" pad="65"/>
<connect gate="G$1" pin="P2.9/USB_CONNECT/RXD2" pad="64"/>
<connect gate="G$1" pin="P3.25/MAT0.0/PWM1.2" pad="27"/>
<connect gate="G$1" pin="P3.26/STCLK/MAT0.1/PWM1.3" pad="26"/>
<connect gate="G$1" pin="P4.28/RX_MCLK/MAT2.0/TXD3" pad="82"/>
<connect gate="G$1" pin="P4.29/TX_MCLK/MAT2.1/RXD3" pad="85"/>
<connect gate="G$1" pin="RSTOUTN" pad="14"/>
<connect gate="G$1" pin="RTCK" pad="100"/>
<connect gate="G$1" pin="RTCX1" pad="16"/>
<connect gate="G$1" pin="RTCX2" pad="18"/>
<connect gate="G$1" pin="TCK/SWDCLK" pad="5"/>
<connect gate="G$1" pin="TDI" pad="2"/>
<connect gate="G$1" pin="TDO/SWO" pad="1"/>
<connect gate="G$1" pin="TMS/SWDIO" pad="3"/>
<connect gate="G$1" pin="TRST_N" pad="4"/>
<connect gate="G$1" pin="VBAT" pad="19"/>
<connect gate="G$1" pin="VDD3.3V@1" pad="96"/>
<connect gate="G$1" pin="VDD3.3V@2" pad="71"/>
<connect gate="G$1" pin="VDD3.3V@3" pad="54"/>
<connect gate="G$1" pin="VDD3.3V@4" pad="28"/>
<connect gate="G$1" pin="VDDA" pad="10"/>
<connect gate="G$1" pin="VDDREG3.3V@1" pad="42"/>
<connect gate="G$1" pin="VDDREG3.3V@2" pad="84"/>
<connect gate="G$1" pin="VREFN" pad="15"/>
<connect gate="G$1" pin="VREFP" pad="12"/>
<connect gate="G$1" pin="VSS@1" pad="83"/>
<connect gate="G$1" pin="VSS@2" pad="41"/>
<connect gate="G$1" pin="VSS@3" pad="97"/>
<connect gate="G$1" pin="VSS@4" pad="72"/>
<connect gate="G$1" pin="VSS@5" pad="55"/>
<connect gate="G$1" pin="VSS@6" pad="31"/>
<connect gate="G$1" pin="VSSA" pad="11"/>
<connect gate="G$1" pin="X1" pad="22"/>
<connect gate="G$1" pin="X2" pad="23"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="C" prefix="C" uservalue="yes">
<description>&lt;b&gt;Capacitor&lt;/b&gt;&lt;p&gt;</description>
<gates>
<gate name="G$1" symbol="C"/>
</gates>
<devices>
<device name="0402" package="0402">
<connects>
<connect gate="G$1" pin="P$1" pad="1"/>
<connect gate="G$1" pin="P$2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0603" package="0603">
<connects>
<connect gate="G$1" pin="P$1" pad="1"/>
<connect gate="G$1" pin="P$2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0805" package="0805">
<connects>
<connect gate="G$1" pin="P$1" pad="1"/>
<connect gate="G$1" pin="P$2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1206" package="C1206">
<connects>
<connect gate="G$1" pin="P$1" pad="1"/>
<connect gate="G$1" pin="P$2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1210" package="C1210">
<connects>
<connect gate="G$1" pin="P$1" pad="1"/>
<connect gate="G$1" pin="P$2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1812" package="C1812">
<connects>
<connect gate="G$1" pin="P$1" pad="1"/>
<connect gate="G$1" pin="P$2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="R" prefix="R" uservalue="yes">
<gates>
<gate name="G$1" symbol="R"/>
</gates>
<devices>
<device name="0402" package="0402">
<connects>
<connect gate="G$1" pin="P$1" pad="1"/>
<connect gate="G$1" pin="P$2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0603" package="0603">
<connects>
<connect gate="G$1" pin="P$1" pad="1"/>
<connect gate="G$1" pin="P$2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0805" package="0805">
<connects>
<connect gate="G$1" pin="P$1" pad="1"/>
<connect gate="G$1" pin="P$2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1206" package="C1206">
<connects>
<connect gate="G$1" pin="P$1" pad="1"/>
<connect gate="G$1" pin="P$2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1210" package="C1210">
<connects>
<connect gate="G$1" pin="P$1" pad="1"/>
<connect gate="G$1" pin="P$2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1812" package="C1812">
<connects>
<connect gate="G$1" pin="P$1" pad="1"/>
<connect gate="G$1" pin="P$2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="Q" prefix="Q" uservalue="yes">
<gates>
<gate name="G$1" symbol="Q"/>
</gates>
<devices>
<device name="_FC135" package="FC135">
<connects>
<connect gate="G$1" pin="1" pad="X1"/>
<connect gate="G$1" pin="2" pad="X2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_HC49UP" package="HC49UP">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_TC38" package="TC38">
<connects>
<connect gate="G$1" pin="1" pad="+"/>
<connect gate="G$1" pin="2" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_3.2X2.5" package="3.2X.2.5">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="OSCILLATOR" prefix="OSC" uservalue="yes">
<gates>
<gate name="G$1" symbol="OSCILLATOR"/>
</gates>
<devices>
<device name="" package="3.2X.2.5">
<connects>
<connect gate="G$1" pin="CLK" pad="P$3"/>
<connect gate="G$1" pin="EN" pad="P$1"/>
<connect gate="G$1" pin="GND" pad="P$2"/>
<connect gate="G$1" pin="VCC" pad="P$4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SPST" prefix="SW">
<gates>
<gate name="G$1" symbol="TS"/>
</gates>
<devices>
<device name="" package="DTSM-32S-B">
<connects>
<connect gate="G$1" pin="P" pad="P$1"/>
<connect gate="G$1" pin="S" pad="P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_SKRKAWW010" package="SKRKAEE010">
<connects>
<connect gate="G$1" pin="P" pad="P$1"/>
<connect gate="G$1" pin="S" pad="P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LED" prefix="LED" uservalue="yes">
<description>&lt;b&gt;SMD LED&lt;/b&gt;&lt;p&gt;</description>
<gates>
<gate name="G$1" symbol="LED"/>
</gates>
<devices>
<device name="0603" package="CHIPLED_0603">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0805" package="CHIPLED_0805">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1206" package="CHIPLED_1206">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IF-MK20DX128" prefix="IC">
<description>&lt;b&gt;CMSIS-DAP Interface (MK20DX128)&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MK20DX128VFM5"/>
</gates>
<devices>
<device name="" package="HVQFN33">
<connects>
<connect gate="G$1" pin="EPAD" pad="EXP"/>
<connect gate="G$1" pin="IF_NRESET" pad="19"/>
<connect gate="G$1" pin="LED_HID" pad="30"/>
<connect gate="G$1" pin="LED_MSD" pad="29"/>
<connect gate="G$1" pin="LED_UART" pad="31"/>
<connect gate="G$1" pin="NC1" pad="9"/>
<connect gate="G$1" pin="NC2" pad="10"/>
<connect gate="G$1" pin="NC3" pad="11"/>
<connect gate="G$1" pin="NC4" pad="12"/>
<connect gate="G$1" pin="NC5" pad="13"/>
<connect gate="G$1" pin="NC6" pad="14"/>
<connect gate="G$1" pin="NC7" pad="15"/>
<connect gate="G$1" pin="NRESET_FB_BL" pad="16"/>
<connect gate="G$1" pin="NRESET_FB_ISP" pad="21"/>
<connect gate="G$1" pin="SLEEP_NREQ" pad="20"/>
<connect gate="G$1" pin="TGT_NRESET" pad="22"/>
<connect gate="G$1" pin="TGT_RX" pad="25"/>
<connect gate="G$1" pin="TGT_SWCLK" pad="26"/>
<connect gate="G$1" pin="TGT_SWDIO" pad="27"/>
<connect gate="G$1" pin="TGT_SWO" pad="28"/>
<connect gate="G$1" pin="TGT_TX" pad="24"/>
<connect gate="G$1" pin="USB_D+" pad="3"/>
<connect gate="G$1" pin="USB_D-" pad="4"/>
<connect gate="G$1" pin="USB_VBUS" pad="32"/>
<connect gate="G$1" pin="VDD" pad="1"/>
<connect gate="G$1" pin="VDDA" pad="7"/>
<connect gate="G$1" pin="VOUT33" pad="5"/>
<connect gate="G$1" pin="VREGIN" pad="6"/>
<connect gate="G$1" pin="VSS" pad="2"/>
<connect gate="G$1" pin="VSSA" pad="8"/>
<connect gate="G$1" pin="WAKE_NREQ" pad="23"/>
<connect gate="G$1" pin="XTALIN" pad="17"/>
<connect gate="G$1" pin="XTALOUT" pad="18"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MKL25Z128VLK4" prefix="IC">
<gates>
<gate name="G$1" symbol="MKL25Z128VLK4"/>
</gates>
<devices>
<device name="" package="LQFP80">
<connects>
<connect gate="G$1" pin="NRESET" pad="42"/>
<connect gate="G$1" pin="PTA1" pad="27"/>
<connect gate="G$1" pin="PTA12" pad="32"/>
<connect gate="G$1" pin="PTA13" pad="33"/>
<connect gate="G$1" pin="PTA14" pad="34"/>
<connect gate="G$1" pin="PTA15" pad="35"/>
<connect gate="G$1" pin="PTA16" pad="36"/>
<connect gate="G$1" pin="PTA17" pad="37"/>
<connect gate="G$1" pin="PTA2" pad="28"/>
<connect gate="G$1" pin="PTA4" pad="30"/>
<connect gate="G$1" pin="PTA5" pad="31"/>
<connect gate="G$1" pin="PTB0" pad="43"/>
<connect gate="G$1" pin="PTB1" pad="44"/>
<connect gate="G$1" pin="PTB10" pad="49"/>
<connect gate="G$1" pin="PTB11" pad="50"/>
<connect gate="G$1" pin="PTB16" pad="51"/>
<connect gate="G$1" pin="PTB17" pad="52"/>
<connect gate="G$1" pin="PTB18" pad="53"/>
<connect gate="G$1" pin="PTB19" pad="54"/>
<connect gate="G$1" pin="PTB2" pad="45"/>
<connect gate="G$1" pin="PTB3" pad="46"/>
<connect gate="G$1" pin="PTB8" pad="47"/>
<connect gate="G$1" pin="PTB9" pad="48"/>
<connect gate="G$1" pin="PTC0" pad="55"/>
<connect gate="G$1" pin="PTC1" pad="56"/>
<connect gate="G$1" pin="PTC10" pad="67"/>
<connect gate="G$1" pin="PTC11" pad="68"/>
<connect gate="G$1" pin="PTC12" pad="69"/>
<connect gate="G$1" pin="PTC13" pad="70"/>
<connect gate="G$1" pin="PTC16" pad="71"/>
<connect gate="G$1" pin="PTC17" pad="72"/>
<connect gate="G$1" pin="PTC2" pad="57"/>
<connect gate="G$1" pin="PTC3" pad="58"/>
<connect gate="G$1" pin="PTC4" pad="61"/>
<connect gate="G$1" pin="PTC5" pad="62"/>
<connect gate="G$1" pin="PTC6" pad="63"/>
<connect gate="G$1" pin="PTC7" pad="64"/>
<connect gate="G$1" pin="PTC8" pad="65"/>
<connect gate="G$1" pin="PTC9" pad="66"/>
<connect gate="G$1" pin="PTD0" pad="73"/>
<connect gate="G$1" pin="PTD1" pad="74"/>
<connect gate="G$1" pin="PTD2" pad="75"/>
<connect gate="G$1" pin="PTD3" pad="76"/>
<connect gate="G$1" pin="PTD4" pad="77"/>
<connect gate="G$1" pin="PTD5" pad="78"/>
<connect gate="G$1" pin="PTD6" pad="79"/>
<connect gate="G$1" pin="PTD7" pad="80"/>
<connect gate="G$1" pin="PTE0" pad="1"/>
<connect gate="G$1" pin="PTE1" pad="2"/>
<connect gate="G$1" pin="PTE2" pad="3"/>
<connect gate="G$1" pin="PTE20" pad="13"/>
<connect gate="G$1" pin="PTE21" pad="14"/>
<connect gate="G$1" pin="PTE22" pad="15"/>
<connect gate="G$1" pin="PTE23" pad="16"/>
<connect gate="G$1" pin="PTE24" pad="24"/>
<connect gate="G$1" pin="PTE25" pad="25"/>
<connect gate="G$1" pin="PTE29" pad="21"/>
<connect gate="G$1" pin="PTE3" pad="4"/>
<connect gate="G$1" pin="PTE30" pad="22"/>
<connect gate="G$1" pin="PTE31" pad="23"/>
<connect gate="G$1" pin="PTE4" pad="5"/>
<connect gate="G$1" pin="PTE5" pad="6"/>
<connect gate="G$1" pin="SWCLK" pad="26"/>
<connect gate="G$1" pin="SWDIO" pad="29"/>
<connect gate="G$1" pin="USB_D+" pad="9"/>
<connect gate="G$1" pin="USB_D-" pad="10"/>
<connect gate="G$1" pin="VDD1" pad="7"/>
<connect gate="G$1" pin="VDD2" pad="60"/>
<connect gate="G$1" pin="VDD3" pad="38"/>
<connect gate="G$1" pin="VDDA" pad="17"/>
<connect gate="G$1" pin="VOUT33" pad="11"/>
<connect gate="G$1" pin="VREFH" pad="18"/>
<connect gate="G$1" pin="VREFL" pad="19"/>
<connect gate="G$1" pin="VREGIN" pad="12"/>
<connect gate="G$1" pin="VSS1" pad="8"/>
<connect gate="G$1" pin="VSS2" pad="59"/>
<connect gate="G$1" pin="VSS3" pad="39"/>
<connect gate="G$1" pin="VSSA" pad="20"/>
<connect gate="G$1" pin="XTALIN" pad="40"/>
<connect gate="G$1" pin="XTALOUT" pad="41"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="USB" prefix="CON">
<description>&lt;b&gt;USB Connectors&lt;/b&gt;&lt;p&gt;</description>
<gates>
<gate name="A" symbol="USB-1"/>
</gates>
<devices>
<device name="-A-H" package="USB-A-H">
<connects>
<connect gate="A" pin="D+" pad="D+"/>
<connect gate="A" pin="D-" pad="D-"/>
<connect gate="A" pin="GND" pad="GND"/>
<connect gate="A" pin="VBUS" pad="VBUS"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-A-S" package="USB-A-S">
<connects>
<connect gate="A" pin="D+" pad="D+"/>
<connect gate="A" pin="D-" pad="D-"/>
<connect gate="A" pin="GND" pad="GND"/>
<connect gate="A" pin="VBUS" pad="VBUS"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-B-H" package="USB-B-H">
<connects>
<connect gate="A" pin="D+" pad="D+"/>
<connect gate="A" pin="D-" pad="D-"/>
<connect gate="A" pin="GND" pad="GND"/>
<connect gate="A" pin="VBUS" pad="VBUS"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-MB-S" package="USB-MB-S">
<connects>
<connect gate="A" pin="D+" pad="D+"/>
<connect gate="A" pin="D-" pad="D-"/>
<connect gate="A" pin="GND" pad="GND"/>
<connect gate="A" pin="VBUS" pad="VBUS"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-A-V" package="USB-A-V">
<connects>
<connect gate="A" pin="D+" pad="D+"/>
<connect gate="A" pin="D-" pad="D-"/>
<connect gate="A" pin="GND" pad="GND"/>
<connect gate="A" pin="VBUS" pad="VBUS"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_MICROB" package="MOLEX-47364-0001">
<connects>
<connect gate="A" pin="D+" pad="D+"/>
<connect gate="A" pin="D-" pad="D-"/>
<connect gate="A" pin="GND" pad="GND"/>
<connect gate="A" pin="VBUS" pad="VBUS"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="C-POL" prefix="C" uservalue="yes">
<description>&lt;b&gt;Polarised capacitor&lt;/b&gt;&lt;p&gt;</description>
<gates>
<gate name="G$1" symbol="C-POL"/>
</gates>
<devices>
<device name="B" package="CASE-B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="+3.3V_IF">
<gates>
<gate name="G$1" symbol="+3.3V_IF"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="+3.3V_TGT">
<gates>
<gate name="G$1" symbol="+3.3V_TGT"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="GND" prefix="GND">
<description>SUPPLY SYMBOL</description>
<gates>
<gate name="1" symbol="GND"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="+VIN" prefix="U+">
<gates>
<gate name="G$1" symbol="+VIN"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DP83848J" prefix="IC">
<description>&lt;B&gt;National Semiconductor DP83848J PHYTER Mini LS Single Port 10/100 Ethernet Transceiver&lt;/B&gt;</description>
<gates>
<gate name="A" symbol="DP83848J"/>
</gates>
<devices>
<device name="" package="LLP-40">
<connects>
<connect gate="A" pin="AGND@1" pad="13"/>
<connect gate="A" pin="AGND@2" pad="17"/>
<connect gate="A" pin="AVDD33" pad="18"/>
<connect gate="A" pin="COL/PHYAD0" pad="35"/>
<connect gate="A" pin="CRS/CRS_DV/LED_CFG" pad="33"/>
<connect gate="A" pin="DGND" pad="29"/>
<connect gate="A" pin="GNDPAD" pad="DAP"/>
<connect gate="A" pin="IOGND@2" pad="40"/>
<connect gate="A" pin="IOVDD33@1" pad="1"/>
<connect gate="A" pin="IOVDD33@2" pad="26"/>
<connect gate="A" pin="LED_LINK/AN0" pad="22"/>
<connect gate="A" pin="LED_SPEED/AN1" pad="21"/>
<connect gate="A" pin="MDC" pad="25"/>
<connect gate="A" pin="MDIO" pad="24"/>
<connect gate="A" pin="PFBIN1" pad="16"/>
<connect gate="A" pin="PFBIN2" pad="30"/>
<connect gate="A" pin="PFBOUT" pad="19"/>
<connect gate="A" pin="RBIAS" pad="20"/>
<connect gate="A" pin="RD+" pad="12"/>
<connect gate="A" pin="RD-" pad="11"/>
<connect gate="A" pin="RESERVED@1" pad="8"/>
<connect gate="A" pin="RESERVED@2" pad="9"/>
<connect gate="A" pin="RESERVED@3" pad="10"/>
<connect gate="A" pin="RESET_N" pad="23"/>
<connect gate="A" pin="RXD_0/PHYAD1" pad="36"/>
<connect gate="A" pin="RXD_1/PHYAD2" pad="37"/>
<connect gate="A" pin="RXD_2/PHYAD3" pad="38"/>
<connect gate="A" pin="RXD_3/PHYAD4" pad="39"/>
<connect gate="A" pin="RX_CLK" pad="31"/>
<connect gate="A" pin="RX_DV/MII_MODE" pad="32"/>
<connect gate="A" pin="RX_ER/MDIX_EN" pad="34"/>
<connect gate="A" pin="TD+" pad="15"/>
<connect gate="A" pin="TD-" pad="14"/>
<connect gate="A" pin="TXD_0" pad="4"/>
<connect gate="A" pin="TXD_1" pad="5"/>
<connect gate="A" pin="TXD_2" pad="6"/>
<connect gate="A" pin="TXD_3" pad="7"/>
<connect gate="A" pin="TX_CLK" pad="2"/>
<connect gate="A" pin="TX_EN" pad="3"/>
<connect gate="A" pin="X1" pad="28"/>
<connect gate="A" pin="X2" pad="27"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RJ45" prefix="CON">
<description>Magjack SI-68002</description>
<gates>
<gate name="G$1" symbol="RJ45"/>
</gates>
<devices>
<device name="" package="RJ45">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="SHIELD1" pad="P$1"/>
<connect gate="G$1" pin="SHIELD2" pad="P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="L" prefix="L" uservalue="yes">
<description>&lt;b&gt;Inductor&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="0603">
<connects>
<connect gate="G$1" pin="P$1" pad="1"/>
<connect gate="G$1" pin="P$2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LPC812M101" prefix="IC">
<description>&lt;H2&gt;32-bit ARM Cortex-M0+ microcontroller&lt;/H2&gt;
The LPC81xM are an ARM Cortex-M0+ based, low-cost 32-bit MCU family operating at 
CPU frequencies of up to 30 MHz. The LPC81xM support up to 16 kB of flash memory 
and 4 kB of SRAM.
The peripheral complement of the LPC81xM includes a CRC engine, one I
2
C-bus 
interface, up to three USARTs, up to two SPI interfaces, one multi-rate timer, self wake-up 
timer, and state-configurable timer, one comparator, function-configurable I/O ports 
through a switch matrix, an input pattern match engine, and up to 18 general-purpose I/O 
pins.
&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt;
 &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="LPC812M101FD20-1"/>
</gates>
<devices>
<device name="FD20" package="SOT163-1">
<connects>
<connect gate="G$1" pin="!RESET!/PIO0_5" pad="4"/>
<connect gate="G$1" pin="PIO0_0/ACMP_I1/TDO" pad="19"/>
<connect gate="G$1" pin="PIO0_1/ACMP_I2/CLKIN/TDI" pad="12"/>
<connect gate="G$1" pin="PIO0_10" pad="9"/>
<connect gate="G$1" pin="PIO0_11" pad="8"/>
<connect gate="G$1" pin="PIO0_12" pad="3"/>
<connect gate="G$1" pin="PIO0_13" pad="2"/>
<connect gate="G$1" pin="PIO0_14" pad="20"/>
<connect gate="G$1" pin="PIO0_15" pad="11"/>
<connect gate="G$1" pin="PIO0_16" pad="10"/>
<connect gate="G$1" pin="PIO0_17" pad="1"/>
<connect gate="G$1" pin="PIO0_4/WAKEUP/!TRST!" pad="5"/>
<connect gate="G$1" pin="PIO0_6/VDDCMP" pad="18"/>
<connect gate="G$1" pin="PIO0_7" pad="17"/>
<connect gate="G$1" pin="PIO0_8/XTALIN" pad="14"/>
<connect gate="G$1" pin="PIO0_9/XTALOUT" pad="13"/>
<connect gate="G$1" pin="SWCLK/PIO0_3/TCK" pad="6"/>
<connect gate="G$1" pin="SWDIO/PIO0_2/TMS" pad="7"/>
<connect gate="G$1" pin="VDD" pad="15"/>
<connect gate="G$1" pin="VSS" pad="16"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMP" value="1"/>
<attribute name="FLASH" value="16k"/>
<attribute name="GPIO" value="18"/>
<attribute name="I2C" value="1"/>
<attribute name="SPI" value="1"/>
<attribute name="SRAM" value="4k"/>
<attribute name="USART" value="2"/>
</technology>
</technologies>
</device>
<device name="FDH20" package="SOT360">
<connects>
<connect gate="G$1" pin="!RESET!/PIO0_5" pad="4"/>
<connect gate="G$1" pin="PIO0_0/ACMP_I1/TDO" pad="19"/>
<connect gate="G$1" pin="PIO0_1/ACMP_I2/CLKIN/TDI" pad="12"/>
<connect gate="G$1" pin="PIO0_10" pad="9"/>
<connect gate="G$1" pin="PIO0_11" pad="8"/>
<connect gate="G$1" pin="PIO0_12" pad="3"/>
<connect gate="G$1" pin="PIO0_13" pad="2"/>
<connect gate="G$1" pin="PIO0_14" pad="20"/>
<connect gate="G$1" pin="PIO0_15" pad="11"/>
<connect gate="G$1" pin="PIO0_16" pad="10"/>
<connect gate="G$1" pin="PIO0_17" pad="1"/>
<connect gate="G$1" pin="PIO0_4/WAKEUP/!TRST!" pad="5"/>
<connect gate="G$1" pin="PIO0_6/VDDCMP" pad="18"/>
<connect gate="G$1" pin="PIO0_7" pad="17"/>
<connect gate="G$1" pin="PIO0_8/XTALIN" pad="14"/>
<connect gate="G$1" pin="PIO0_9/XTALOUT" pad="13"/>
<connect gate="G$1" pin="SWCLK/PIO0_3/TCK" pad="6"/>
<connect gate="G$1" pin="SWDIO/PIO0_2/TMS" pad="7"/>
<connect gate="G$1" pin="VDD" pad="15"/>
<connect gate="G$1" pin="VSS" pad="16"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMP" value="1"/>
<attribute name="FLASH" value="16k"/>
<attribute name="GPIO" value="18"/>
<attribute name="I2C" value="1"/>
<attribute name="SPI" value="2"/>
<attribute name="SRAM" value="4k"/>
<attribute name="USART" value="3"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LPC1347FBD64" prefix="IC">
<description>&lt;H2&gt;32-bit ARM Cortex-M3 microcontroller; up to 64  kB flash;        
up to 12 kB SRAM; USB device; USART; EEPROM&lt;/H2&gt;
The LPC1315/16/17/45/46/47 are ARM Cortex-M3 based microcontrollers for embedded 
applications featuring a high level of integration and low power consumption. The ARM 
Cortex-M3 is a next generation core that offers system enhancements such as enhanced 
debug features and a higher level of support block integration.
The LPC1315/16/17/45/46/47 operate at CPU frequencies of up to 72 MHz. The ARM 
Cortex-M3 CPU incorporates a 3-stage pipeline and uses a Harvard architecture with 
separate local instruction and data buses as well as a third bus for peripherals. The ARM 
Cortex-M3 CPU also includes an internal prefetch unit that supports speculative 
branching. 
Equipped with a highly flexible and configurable Full-Speed USB 2.0 device controller 
available on the LPC1345/46/47, this series brings unparalleled design flexibility and 
seamless integration to today’s demanding connectivity solutions.
The peripheral complement of the LPC1315/16/17/45/46/47 includes up to 64 kB of flash 
memory, 8 kB or 10 kB of SRAM data memory, one Fast-mode Plus I
2
C-bus interface, one 
RS-485/EIA-485 USART with support for synchronous mode and smart card interface, 
two SSP interfaces, four general purpose counter/timers, an 8-channel, 12-bit ADC, and 
up to 51 general purpose I/O pins.
&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt;
 &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="LPC1347FBD64"/>
</gates>
<devices>
<device name="" package="SOT314-2">
<connects>
<connect gate="G$1" pin="!RESET!/PIO0_0" pad="4"/>
<connect gate="G$1" pin="!TRST!/PIO0_14/AD3/CT32B1_MAT1" pad="46"/>
<connect gate="G$1" pin="PIO0_1/CLKOUT/CT32B0_MAT2/USB_FTOGGLE" pad="5"/>
<connect gate="G$1" pin="PIO0_16/AD5/CT32B1_MAT3/WAKEUP" pad="53"/>
<connect gate="G$1" pin="PIO0_17/!RTS!/CT32B0_CAP0/SCLK" pad="60"/>
<connect gate="G$1" pin="PIO0_18/RXD/CT32B0_MAT0" pad="61"/>
<connect gate="G$1" pin="PIO0_19/TXD/CT32B0_MAT1" pad="62"/>
<connect gate="G$1" pin="PIO0_2/SSEL0/CT16B0_CAP0" pad="13"/>
<connect gate="G$1" pin="PIO0_20/CT16B1_CAP0" pad="11"/>
<connect gate="G$1" pin="PIO0_21/CT16B1_MAT0/MOSI1" pad="22"/>
<connect gate="G$1" pin="PIO0_22/AD6/CT16B1_MAT1/MISO1" pad="40"/>
<connect gate="G$1" pin="PIO0_23/AD7" pad="56"/>
<connect gate="G$1" pin="PIO0_3/USB_VBUS" pad="19"/>
<connect gate="G$1" pin="PIO0_4/SCL" pad="20"/>
<connect gate="G$1" pin="PIO0_5/SDA" pad="21"/>
<connect gate="G$1" pin="PIO0_6/!USB_CONNECT!/SCK0" pad="29"/>
<connect gate="G$1" pin="PIO0_7/!CTS!" pad="30"/>
<connect gate="G$1" pin="PIO0_8/MISO0/CT16B0_MAT0" pad="36"/>
<connect gate="G$1" pin="PIO0_9/MOSI0/CT16B0_MAT1/SWO" pad="37"/>
<connect gate="G$1" pin="PIO1_0/CT32B1_MAT0" pad="1"/>
<connect gate="G$1" pin="PIO1_1/CT32B1_MAT1" pad="17"/>
<connect gate="G$1" pin="PIO1_10" pad="12"/>
<connect gate="G$1" pin="PIO1_11" pad="43"/>
<connect gate="G$1" pin="PIO1_13/!DTR!/CT16B0_MAT0/TXD" pad="47"/>
<connect gate="G$1" pin="PIO1_14/!DSR!/CT16B0_MAT1/RXD" pad="49"/>
<connect gate="G$1" pin="PIO1_15/!DCD!/CT16B0_MAT2/SCK1" pad="57"/>
<connect gate="G$1" pin="PIO1_16/!RI!/CT16B0_CAP0" pad="63"/>
<connect gate="G$1" pin="PIO1_17/CT16B0_CAP1/RXD" pad="23"/>
<connect gate="G$1" pin="PIO1_18/CT16B1_CAP1/TXD" pad="28"/>
<connect gate="G$1" pin="PIO1_19/!DTR!/SSEL1" pad="3"/>
<connect gate="G$1" pin="PIO1_2/CT32B1_MAT2" pad="34"/>
<connect gate="G$1" pin="PIO1_20/!DSR!/SCK1" pad="18"/>
<connect gate="G$1" pin="PIO1_21/!DCD!/MISO1" pad="35"/>
<connect gate="G$1" pin="PIO1_22/!RI!/MOSI1" pad="51"/>
<connect gate="G$1" pin="PIO1_23/CT16B1_MAT1/SSEL1" pad="24"/>
<connect gate="G$1" pin="PIO1_24/CT32B0_MAT0" pad="27"/>
<connect gate="G$1" pin="PIO1_25/CT32B0_MAT1" pad="2"/>
<connect gate="G$1" pin="PIO1_26/CT32B0_MAT2/RXD" pad="14"/>
<connect gate="G$1" pin="PIO1_27/CT32B0_MAT3/TXD" pad="15"/>
<connect gate="G$1" pin="PIO1_28/CT32B0_CAP0/SCLK" pad="31"/>
<connect gate="G$1" pin="PIO1_29/SCK0/CT32B0_CAP1" pad="41"/>
<connect gate="G$1" pin="PIO1_3/CT32B1_MAT3" pad="50"/>
<connect gate="G$1" pin="PIO1_4/CT32B1_CAP0" pad="16"/>
<connect gate="G$1" pin="PIO1_5/CT32B1_CAP1" pad="32"/>
<connect gate="G$1" pin="PIO1_7" pad="6"/>
<connect gate="G$1" pin="PIO1_8" pad="39"/>
<connect gate="G$1" pin="SWCLK/PIO0_10/SCK0/CT16B0_MAT2" pad="38"/>
<connect gate="G$1" pin="SWDIO/PIO0_15/AD4/CT32B1_MAT2" pad="52"/>
<connect gate="G$1" pin="TDI/PIO0_11/AD0/CT32B0_MAT3" pad="42"/>
<connect gate="G$1" pin="TDO/PIO0_13/AD2/CT32B1_MAT0" pad="45"/>
<connect gate="G$1" pin="TMS/PIO0_12/AD1/CT32B1_CAP0" pad="44"/>
<connect gate="G$1" pin="USB_DM" pad="25"/>
<connect gate="G$1" pin="USB_DP" pad="26"/>
<connect gate="G$1" pin="VDD" pad="10 33 58"/>
<connect gate="G$1" pin="VDDA" pad="59"/>
<connect gate="G$1" pin="VREFN" pad="48"/>
<connect gate="G$1" pin="VREFP" pad="64"/>
<connect gate="G$1" pin="VSS" pad="7 54"/>
<connect gate="G$1" pin="VSSA" pad="55"/>
<connect gate="G$1" pin="XTALIN" pad="8"/>
<connect gate="G$1" pin="XTALOUT" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="EEPROM" value="4kB"/>
<attribute name="FLASH" value="64kB"/>
<attribute name="GPIO" value="51"/>
<attribute name="SRAM0" value="8kB"/>
<attribute name="SRAM1" value="2kB"/>
<attribute name="SRAM_USB" value="2kB"/>
<attribute name="USB" value="yes"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LPC4088FET208" prefix="IC">
<description>&lt;H2&gt;32-bit ARM Cortex-M4 MCU; up to 512 kB flash, 96 kB SRAM; 
USB Device/Host/OTG; Ethernet; LCD; EMC; SPIFI&lt;/H2&gt;
The LPC408x/7x is an ARM Cortex-M4 based digital signal controller for embedded 
applications requiring a high level of integration and low power dissipation.
The ARM Cortex-M4 is a next generation core that offers system enhancements such as 
low power consumption, enhanced debug features, and a high level of support block 
integration. The ARM Cortex-M4 CPU incorporates a 3-stage pipeline, uses a Harvard 
architecture with separate local instruction and data buses as well as a third bus for 
peripherals, and includes an internal prefetch unit that supports speculative branching. 
The ARM Cortex-M4 supports single-cycle digital signal processing and SIMD 
instructions. A hardware floating-point processor is integrated in the core for several 
versions of the part. 
The LPC408x/7x adds a specialized flash memory accelerator to accomplish optimal 
performance when executing code from flash. The LPC408x/7x is targeted to operate at 
up to 120 MHz CPU frequency.
The peripheral complement of the LPC408x/7x includes up to 512 kB of flash program 
memory, up to 96 kB of SRAM data memory, up to 4032 byte of EEPROM data memory, 
External Memory controller (EMC), LCD, Ethernet, USB Device/Host/OTG, an SPI Flash 
Interface (SPIFI), a General Purpose DMA controller, five UARTs, three SSP controllers, 
three I
2
C-bus interfaces, a Quadrature Encoder Interface, four general purpose timers, 
two general purpose PWMs with six outputs each and one motor control PWM, an 
ultra-low power RTC with separate battery supply and event recorder, a windowed 
watchdog timer, a CRC calculation engine and up to 165 general purpose I/O pins. 
The analog peripherals include one eight-channel 12-bit ADC, two analog comparators, 
and a DAC.
The pinout of LPC408x/7x is intended to allow pin function compatibility with the 
LPC24xx/23xx as well as the LPC178x/7x families.
&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt;
 &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="LPC40X8FYY208"/>
</gates>
<devices>
<device name="" package="SOT950-1">
<connects>
<connect gate="G$1" pin="!RESET!" pad="M2"/>
<connect gate="G$1" pin="!RSTOUT!" pad="K3"/>
<connect gate="G$1" pin="JTAG_!TRST" pad="D1"/>
<connect gate="G$1" pin="JTAG_TCK/SWDCLK" pad="E2"/>
<connect gate="G$1" pin="JTAG_TDI" pad="C2"/>
<connect gate="G$1" pin="JTAG_TDO/SWO" pad="D3"/>
<connect gate="G$1" pin="JTAG_TMS/SWDIO" pad="E3"/>
<connect gate="G$1" pin="P0[0]" pad="U15"/>
<connect gate="G$1" pin="P0[10]" pad="T15"/>
<connect gate="G$1" pin="P0[11]" pad="R14"/>
<connect gate="G$1" pin="P0[12]" pad="R1"/>
<connect gate="G$1" pin="P0[13]" pad="R2"/>
<connect gate="G$1" pin="P0[14]" pad="T7"/>
<connect gate="G$1" pin="P0[15]" pad="J16"/>
<connect gate="G$1" pin="P0[16]" pad="J14"/>
<connect gate="G$1" pin="P0[17]" pad="K17"/>
<connect gate="G$1" pin="P0[18]" pad="K15"/>
<connect gate="G$1" pin="P0[19]" pad="L17"/>
<connect gate="G$1" pin="P0[1]" pad="T14"/>
<connect gate="G$1" pin="P0[20]" pad="M17"/>
<connect gate="G$1" pin="P0[21]" pad="M16"/>
<connect gate="G$1" pin="P0[22]" pad="N17"/>
<connect gate="G$1" pin="P0[23]" pad="H1"/>
<connect gate="G$1" pin="P0[24]" pad="G2"/>
<connect gate="G$1" pin="P0[25]" pad="F1"/>
<connect gate="G$1" pin="P0[26]" pad="E1"/>
<connect gate="G$1" pin="P0[27]" pad="T1"/>
<connect gate="G$1" pin="P0[28]" pad="R3"/>
<connect gate="G$1" pin="P0[29]" pad="U4"/>
<connect gate="G$1" pin="P0[2]" pad="C4"/>
<connect gate="G$1" pin="P0[30]" pad="R6"/>
<connect gate="G$1" pin="P0[31]" pad="T2"/>
<connect gate="G$1" pin="P0[3]" pad="D6"/>
<connect gate="G$1" pin="P0[4]" pad="B12"/>
<connect gate="G$1" pin="P0[5]" pad="C12"/>
<connect gate="G$1" pin="P0[6]" pad="D13"/>
<connect gate="G$1" pin="P0[7]" pad="C13"/>
<connect gate="G$1" pin="P0[8]" pad="A15"/>
<connect gate="G$1" pin="P0[9]" pad="C14"/>
<connect gate="G$1" pin="P1[0]" pad="A3"/>
<connect gate="G$1" pin="P1[10]" pad="C8"/>
<connect gate="G$1" pin="P1[11]" pad="A14"/>
<connect gate="G$1" pin="P1[12]" pad="A16"/>
<connect gate="G$1" pin="P1[13]" pad="D16"/>
<connect gate="G$1" pin="P1[14]" pad="A7"/>
<connect gate="G$1" pin="P1[15]" pad="A8"/>
<connect gate="G$1" pin="P1[16]" pad="D10"/>
<connect gate="G$1" pin="P1[17]" pad="A9"/>
<connect gate="G$1" pin="P1[18]" pad="P7"/>
<connect gate="G$1" pin="P1[19]" pad="U6"/>
<connect gate="G$1" pin="P1[1]" pad="B5"/>
<connect gate="G$1" pin="P1[20]" pad="U7"/>
<connect gate="G$1" pin="P1[21]" pad="R8"/>
<connect gate="G$1" pin="P1[22]" pad="U8"/>
<connect gate="G$1" pin="P1[23]" pad="P9"/>
<connect gate="G$1" pin="P1[24]" pad="T9"/>
<connect gate="G$1" pin="P1[25]" pad="T10"/>
<connect gate="G$1" pin="P1[26]" pad="R10"/>
<connect gate="G$1" pin="P1[27]" pad="T12"/>
<connect gate="G$1" pin="P1[28]" pad="T13"/>
<connect gate="G$1" pin="P1[29]" pad="U14"/>
<connect gate="G$1" pin="P1[2]" pad="D9"/>
<connect gate="G$1" pin="P1[30]" pad="P2"/>
<connect gate="G$1" pin="P1[31]" pad="P1"/>
<connect gate="G$1" pin="P1[3]" pad="A10"/>
<connect gate="G$1" pin="P1[4]" pad="A5"/>
<connect gate="G$1" pin="P1[5]" pad="A17"/>
<connect gate="G$1" pin="P1[6]" pad="B11"/>
<connect gate="G$1" pin="P1[7]" pad="D14"/>
<connect gate="G$1" pin="P1[8]" pad="C7"/>
<connect gate="G$1" pin="P1[9]" pad="A6"/>
<connect gate="G$1" pin="P2[0]" pad="B17"/>
<connect gate="G$1" pin="P2[10]" pad="N15"/>
<connect gate="G$1" pin="P2[11]" pad="T17"/>
<connect gate="G$1" pin="P2[12]" pad="N14"/>
<connect gate="G$1" pin="P2[13]" pad="T16"/>
<connect gate="G$1" pin="P2[14]" pad="R12"/>
<connect gate="G$1" pin="P2[15]" pad="P13"/>
<connect gate="G$1" pin="P2[16]" pad="R11"/>
<connect gate="G$1" pin="P2[17]" pad="R13"/>
<connect gate="G$1" pin="P2[18]" pad="U3"/>
<connect gate="G$1" pin="P2[19]" pad="R7"/>
<connect gate="G$1" pin="P2[1]" pad="E14"/>
<connect gate="G$1" pin="P2[20]" pad="T8"/>
<connect gate="G$1" pin="P2[21]" pad="U11"/>
<connect gate="G$1" pin="P2[22]" pad="U12"/>
<connect gate="G$1" pin="P2[23]" pad="U5"/>
<connect gate="G$1" pin="P2[24]" pad="P5"/>
<connect gate="G$1" pin="P2[25]" pad="R4"/>
<connect gate="G$1" pin="P2[26]" pad="T4"/>
<connect gate="G$1" pin="P2[27]" pad="P3"/>
<connect gate="G$1" pin="P2[28]" pad="P4"/>
<connect gate="G$1" pin="P2[29]" pad="N3"/>
<connect gate="G$1" pin="P2[2]" pad="D15"/>
<connect gate="G$1" pin="P2[30]" pad="L4"/>
<connect gate="G$1" pin="P2[31]" pad="N2"/>
<connect gate="G$1" pin="P2[3]" pad="E16"/>
<connect gate="G$1" pin="P2[4]" pad="D17"/>
<connect gate="G$1" pin="P2[5]" pad="F16"/>
<connect gate="G$1" pin="P2[6]" pad="E17"/>
<connect gate="G$1" pin="P2[7]" pad="G16"/>
<connect gate="G$1" pin="P2[8]" pad="H15"/>
<connect gate="G$1" pin="P2[9]" pad="H16"/>
<connect gate="G$1" pin="P3[0]" pad="B4"/>
<connect gate="G$1" pin="P3[10]" pad="B2"/>
<connect gate="G$1" pin="P3[11]" pad="D5"/>
<connect gate="G$1" pin="P3[12]" pad="D4"/>
<connect gate="G$1" pin="P3[13]" pad="C1"/>
<connect gate="G$1" pin="P3[14]" pad="H2"/>
<connect gate="G$1" pin="P3[15]" pad="M1"/>
<connect gate="G$1" pin="P3[16]" pad="F17"/>
<connect gate="G$1" pin="P3[17]" pad="F15"/>
<connect gate="G$1" pin="P3[18]" pad="C15"/>
<connect gate="G$1" pin="P3[19]" pad="B14"/>
<connect gate="G$1" pin="P3[1]" pad="B3"/>
<connect gate="G$1" pin="P3[20]" pad="A13"/>
<connect gate="G$1" pin="P3[21]" pad="C10"/>
<connect gate="G$1" pin="P3[22]" pad="C6"/>
<connect gate="G$1" pin="P3[23]" pad="T6"/>
<connect gate="G$1" pin="P3[24]" pad="R5"/>
<connect gate="G$1" pin="P3[25]" pad="U2"/>
<connect gate="G$1" pin="P3[26]" pad="T3"/>
<connect gate="G$1" pin="P3[27]" pad="A1"/>
<connect gate="G$1" pin="P3[28]" pad="D2"/>
<connect gate="G$1" pin="P3[29]" pad="F3"/>
<connect gate="G$1" pin="P3[2]" pad="B1"/>
<connect gate="G$1" pin="P3[30]" pad="H3"/>
<connect gate="G$1" pin="P3[31]" pad="J3"/>
<connect gate="G$1" pin="P3[3]" pad="E4"/>
<connect gate="G$1" pin="P3[4]" pad="F2"/>
<connect gate="G$1" pin="P3[5]" pad="G1"/>
<connect gate="G$1" pin="P3[6]" pad="J1"/>
<connect gate="G$1" pin="P3[7]" pad="L1"/>
<connect gate="G$1" pin="P3[8]" pad="D8"/>
<connect gate="G$1" pin="P3[9]" pad="C5"/>
<connect gate="G$1" pin="P4[0]" pad="U9"/>
<connect gate="G$1" pin="P4[10]" pad="G17"/>
<connect gate="G$1" pin="P4[11]" pad="F14"/>
<connect gate="G$1" pin="P4[12]" pad="C16"/>
<connect gate="G$1" pin="P4[13]" pad="B16"/>
<connect gate="G$1" pin="P4[14]" pad="B15"/>
<connect gate="G$1" pin="P4[15]" pad="A11"/>
<connect gate="G$1" pin="P4[16]" pad="U17"/>
<connect gate="G$1" pin="P4[17]" pad="P14"/>
<connect gate="G$1" pin="P4[18]" pad="P15"/>
<connect gate="G$1" pin="P4[19]" pad="P16"/>
<connect gate="G$1" pin="P4[1]" pad="U10"/>
<connect gate="G$1" pin="P4[20]" pad="R17"/>
<connect gate="G$1" pin="P4[21]" pad="M15"/>
<connect gate="G$1" pin="P4[22]" pad="K14"/>
<connect gate="G$1" pin="P4[23]" pad="J15"/>
<connect gate="G$1" pin="P4[24]" pad="B8"/>
<connect gate="G$1" pin="P4[25]" pad="B9"/>
<connect gate="G$1" pin="P4[26]" pad="L15"/>
<connect gate="G$1" pin="P4[27]" pad="G15"/>
<connect gate="G$1" pin="P4[28]" pad="C11"/>
<connect gate="G$1" pin="P4[29]" pad="B10"/>
<connect gate="G$1" pin="P4[2]" pad="T11"/>
<connect gate="G$1" pin="P4[30]" pad="B7"/>
<connect gate="G$1" pin="P4[31]" pad="A4"/>
<connect gate="G$1" pin="P4[3]" pad="U16"/>
<connect gate="G$1" pin="P4[4]" pad="R15"/>
<connect gate="G$1" pin="P4[5]" pad="R16"/>
<connect gate="G$1" pin="P4[6]" pad="M14"/>
<connect gate="G$1" pin="P4[7]" pad="L16"/>
<connect gate="G$1" pin="P4[8]" pad="J17"/>
<connect gate="G$1" pin="P4[9]" pad="H17"/>
<connect gate="G$1" pin="P5[0]" pad="F4"/>
<connect gate="G$1" pin="P5[1]" pad="J4"/>
<connect gate="G$1" pin="P5[2]" pad="L14"/>
<connect gate="G$1" pin="P5[3]" pad="G14"/>
<connect gate="G$1" pin="P5[4]" pad="C3"/>
<connect gate="G$1" pin="RTCX1" pad="K2"/>
<connect gate="G$1" pin="RTCX2" pad="L2"/>
<connect gate="G$1" pin="RTC_ALARM" pad="N1"/>
<connect gate="G$1" pin="USB_D-2" pad="U1"/>
<connect gate="G$1" pin="VBAT" pad="M3"/>
<connect gate="G$1" pin="VDD" pad="B13 C9 C17 D7 G3 K16 P6 P8 P17 U13"/>
<connect gate="G$1" pin="VDD(REG)(3V3)" pad="D11 H4 P11"/>
<connect gate="G$1" pin="VDDA" pad="G4"/>
<connect gate="G$1" pin="VREFP" pad="K1"/>
<connect gate="G$1" pin="VSS" pad="A2 A12 B6 E15 H14 L3 N16 P12 R9 T5"/>
<connect gate="G$1" pin="VSSA" pad="J2"/>
<connect gate="G$1" pin="VSSREG" pad="D12 K4 P10"/>
<connect gate="G$1" pin="XTAL1" pad="M4"/>
<connect gate="G$1" pin="XTAL2" pad="N4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LPC1114FN28" prefix="U">
<description>&lt;H2&gt;32-bit ARM Cortex-M0 microcontroller; up to 64 kB flash and 8 kB SRAM&lt;/H2&gt;
The LPC1110/11/12/13/14/15 are a ARM Cortex-M0 based, low-cost 32-bit MCU family, 
designed for 8/16-bit microcontroller applications, offering performance, low power, simple 
instruction set and memory addressing together with reduced code size compared to 
existing 8/16-bit architectures.
The LPC1110/11/12/13/14/15 operate at CPU frequencies of up to 50 MHz. 
The peripheral complement of the LPC1110/11/12/13/14/15 includes up to 64 kB of flash 
memory, up to 8 kB of data memory, one Fast-mode Plus I
2
C-bus interface, one 
RS-485/EIA-485 UART, up to two SPI interfaces with SSP features, four general purpose 
counter/timers, a 10-bit ADC, and up to 42 general purpose I/O pins.
Remark: The LPC111x series consists of the LPC1100 series (parts 
LPC111x/101/201/301), LPC1100L series (parts LPC111x/002/102/202/302), and the 
LPC1100XL series (parts LPC111x/103/203/303/323/333). The LPC1100L and 
LPC1100XL series include the power profiles, a windowed watchdog timer, and a 
configurable open-drain mode.
&lt;p&gt;&lt;author&gt;AAL Eindhoven MK&lt;/author&gt;&lt;hr&gt;&lt;p&gt;
 &lt;img src="http://www.nxp.com/img/NXP_logo.png"&gt;</description>
<gates>
<gate name="G$1" symbol="LPC1112FDH28"/>
</gates>
<devices>
<device name="" package="SOT117">
<connects>
<connect gate="G$1" pin="PIO0_1/CLKOUT/CT32B0_MAT2" pad="24"/>
<connect gate="G$1" pin="PIO0_2/SSEL/CT16B0_CAP0" pad="25"/>
<connect gate="G$1" pin="PIO0_3" pad="26"/>
<connect gate="G$1" pin="PIO0_4/SCL" pad="27"/>
<connect gate="G$1" pin="PIO0_5/SDA" pad="5"/>
<connect gate="G$1" pin="PIO0_6/SCK0" pad="6"/>
<connect gate="G$1" pin="PIO0_7/!CTS!" pad="28"/>
<connect gate="G$1" pin="PIO0_8/MISO0/CT16B0_MAT0" pad="1"/>
<connect gate="G$1" pin="PIO0_9/MOSI0/CT16B0_MAT1" pad="2"/>
<connect gate="G$1" pin="PIO1_4/AD5/CT32B1_MAT3/WAKEUP" pad="13"/>
<connect gate="G$1" pin="PIO1_5/!RTS!/CT32B0_CAP0" pad="14"/>
<connect gate="G$1" pin="PIO1_6/RXD/CT32B0_MAT0" pad="15"/>
<connect gate="G$1" pin="PIO1_7/TXD/CT32B0_MAT1" pad="16"/>
<connect gate="G$1" pin="PIO1_8/CT16B1_CAP0" pad="17"/>
<connect gate="G$1" pin="PIO1_9/CT16B1_MAT0" pad="18"/>
<connect gate="G$1" pin="RESET/PIO0_0" pad="23"/>
<connect gate="G$1" pin="SWCLK/PIO0_10/SCK0/CT16B0_MAT2" pad="3"/>
<connect gate="G$1" pin="SWDIO/PIO1_3/AD4/CT32B1_MAT2" pad="12"/>
<connect gate="G$1" pin="TDI/PIO0_11/AD0/CT32B0_MAT3" pad="4"/>
<connect gate="G$1" pin="TDO/PIO1_1/AD2/CT32B1_MAT0" pad="10"/>
<connect gate="G$1" pin="TMS/PIO1_0/AD1/CT32B1_CAP0" pad="9"/>
<connect gate="G$1" pin="TRST/PIO1_2/AD3/CT32B1_MAT1" pad="11"/>
<connect gate="G$1" pin="VDD" pad="21"/>
<connect gate="G$1" pin="VDDA" pad="7"/>
<connect gate="G$1" pin="VSS" pad="22"/>
<connect gate="G$1" pin="VSSA" pad="8"/>
<connect gate="G$1" pin="XTALIN" pad="20"/>
<connect gate="G$1" pin="XTALOUT" pad="19"/>
</connects>
<technologies>
<technology name="/102">
<attribute name="ADC" value="6"/>
<attribute name="FLASH" value="32kB"/>
<attribute name="GPIO" value="22"/>
<attribute name="PWR_PROFILES" value="yes"/>
<attribute name="SERIES" value="LPC1100L"/>
<attribute name="SPI" value="1"/>
<attribute name="SRAM" value="4kB"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IF-LPC11U35" prefix="IC" uservalue="yes">
<gates>
<gate name="G$1" symbol="IF-LPC11U35"/>
</gates>
<devices>
<device name="" package="HVQFN33">
<connects>
<connect gate="G$1" pin="IF_NRESET" pad="2"/>
<connect gate="G$1" pin="LED_HID" pad="12"/>
<connect gate="G$1" pin="LED_MSD" pad="7"/>
<connect gate="G$1" pin="LED_UART" pad="21"/>
<connect gate="G$1" pin="NC10" pad="28"/>
<connect gate="G$1" pin="NC11" pad="30"/>
<connect gate="G$1" pin="NC2" pad="10"/>
<connect gate="G$1" pin="NC3" pad="11"/>
<connect gate="G$1" pin="NC4" pad="19"/>
<connect gate="G$1" pin="NC5" pad="20"/>
<connect gate="G$1" pin="NC6" pad="22"/>
<connect gate="G$1" pin="NC7" pad="23"/>
<connect gate="G$1" pin="NC8" pad="24"/>
<connect gate="G$1" pin="NC9" pad="25"/>
<connect gate="G$1" pin="NRESET_FB_BL" pad="1"/>
<connect gate="G$1" pin="NRESET_FB_ISP" pad="3"/>
<connect gate="G$1" pin="SLEEP_NREQ" pad="27"/>
<connect gate="G$1" pin="TGT_NRESET" pad="8"/>
<connect gate="G$1" pin="TGT_RX" pad="32"/>
<connect gate="G$1" pin="TGT_SWCLK" pad="16"/>
<connect gate="G$1" pin="TGT_SWDIO" pad="17"/>
<connect gate="G$1" pin="TGT_SWO" pad="18"/>
<connect gate="G$1" pin="TGT_TX" pad="31"/>
<connect gate="G$1" pin="USB_D+" pad="14"/>
<connect gate="G$1" pin="USB_D-" pad="13"/>
<connect gate="G$1" pin="USB_SCON" pad="15"/>
<connect gate="G$1" pin="USB_VBUS" pad="9"/>
<connect gate="G$1" pin="VDD1" pad="6"/>
<connect gate="G$1" pin="VDD2" pad="29"/>
<connect gate="G$1" pin="VSS" pad="EXP"/>
<connect gate="G$1" pin="WAKE_NREQ" pad="26"/>
<connect gate="G$1" pin="XTALIN" pad="4"/>
<connect gate="G$1" pin="XTALOUT" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*125" prefix="IC">
<description>Quad bus &lt;b&gt;BUFFER&lt;/b&gt;, 3-state</description>
<gates>
<gate name="A" symbol="74125"/>
<gate name="B" symbol="74125"/>
<gate name="C" symbol="74125"/>
<gate name="D" symbol="74125"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL14">
<connects>
<connect gate="A" pin="I" pad="2"/>
<connect gate="A" pin="O" pad="3"/>
<connect gate="A" pin="OE" pad="1"/>
<connect gate="B" pin="I" pad="5"/>
<connect gate="B" pin="O" pad="6"/>
<connect gate="B" pin="OE" pad="4"/>
<connect gate="C" pin="I" pad="9"/>
<connect gate="C" pin="O" pad="8"/>
<connect gate="C" pin="OE" pad="10"/>
<connect gate="D" pin="I" pad="12"/>
<connect gate="D" pin="O" pad="11"/>
<connect gate="D" pin="OE" pad="13"/>
<connect gate="P" pin="GND" pad="7"/>
<connect gate="P" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name=""/>
<technology name="LS"/>
</technologies>
</device>
<device name="PW" package="TSSOP14">
<connects>
<connect gate="A" pin="I" pad="2"/>
<connect gate="A" pin="O" pad="3"/>
<connect gate="A" pin="OE" pad="1"/>
<connect gate="B" pin="I" pad="5"/>
<connect gate="B" pin="O" pad="6"/>
<connect gate="B" pin="OE" pad="4"/>
<connect gate="C" pin="I" pad="9"/>
<connect gate="C" pin="O" pad="8"/>
<connect gate="C" pin="OE" pad="10"/>
<connect gate="D" pin="I" pad="12"/>
<connect gate="D" pin="O" pad="11"/>
<connect gate="D" pin="OE" pad="13"/>
<connect gate="P" pin="GND" pad="7"/>
<connect gate="P" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name="ABT"/>
</technologies>
</device>
<device name="DB" package="SSOP14">
<connects>
<connect gate="A" pin="I" pad="2"/>
<connect gate="A" pin="O" pad="3"/>
<connect gate="A" pin="OE" pad="1"/>
<connect gate="B" pin="I" pad="5"/>
<connect gate="B" pin="O" pad="6"/>
<connect gate="B" pin="OE" pad="4"/>
<connect gate="C" pin="I" pad="9"/>
<connect gate="C" pin="O" pad="8"/>
<connect gate="C" pin="OE" pad="10"/>
<connect gate="D" pin="I" pad="12"/>
<connect gate="D" pin="O" pad="11"/>
<connect gate="D" pin="OE" pad="13"/>
<connect gate="P" pin="GND" pad="7"/>
<connect gate="P" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name="ABT"/>
</technologies>
</device>
<device name="BQ" package="DHVQFN14">
<connects>
<connect gate="A" pin="I" pad="2"/>
<connect gate="A" pin="O" pad="3"/>
<connect gate="A" pin="OE" pad="1"/>
<connect gate="B" pin="I" pad="5"/>
<connect gate="B" pin="O" pad="6"/>
<connect gate="B" pin="OE" pad="4"/>
<connect gate="C" pin="I" pad="9"/>
<connect gate="C" pin="O" pad="8"/>
<connect gate="C" pin="OE" pad="10"/>
<connect gate="D" pin="I" pad="12"/>
<connect gate="D" pin="O" pad="11"/>
<connect gate="D" pin="OE" pad="13"/>
<connect gate="P" pin="GND" pad="7"/>
<connect gate="P" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name="ABT"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="+3.3V">
<gates>
<gate name="G$1" symbol="+3.3V"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
