Main Page | Modules | Data Structures | File List | Data Fields | Globals | Related Pages

# binary_stream Struct Reference
[NPF structures and definitions]

A stream of X86 binary code. More...

`#include <jitter.h>`

## Data Fields
INT | cur_ip
| Current X86 instruction pointer.
INT | bpf_pc
| Current BPF instruction pointer, i.e. position in the BPF program reached by the jitter.
PCHAR | ibuf
| Instruction buffer, contains the X86 generated code.
PUINT | refs
| Jumps reference table.

## Detailed Description

A stream of X86 binary code.

Definition at line 68 of file jitter.h.

## Field Documentation

INT bpf_pc

| Current BPF instruction pointer, i.e. position in the BPF program reached by the jitter. Definition at line 70 of file jitter.h.

INT cur_ip

| Current X86 instruction pointer. Definition at line 69 of file jitter.h.

PCHAR ibuf

| Instruction buffer, contains the X86 generated code. Definition at line 71 of file jitter.h.

PUINT refs

| Jumps reference table. Definition at line 72 of file jitter.h.

The documentation for this struct was generated from the following file:

- jitter.h

documentation. Copyright (c) 2002-2005 Politecnico di Torino. Copyright (c) 2005 CACE technologies. All rights reserved.