Back to Release page
# Release Notes for STM32F7xx HAL Drivers Copyright 2016 STMicroelectronics
## Update History ### V1.2.0 / 30-December-2016 Main Changes Official release to add the support of STM32F722xx, STM32F723xx, STM32F732xx and STM32F733xx devices Add Low Layer drivers allowing performance and footprint optimization Low Layer drivers APIs provide register level programming: require deep knowledge of peripherals described in STM32F7xx Reference Manuals Low Layer drivers are available for: ADC, Cortex, CRC, DAC, DMA, DMA2D, EXTI, GPIO, I2C, IWDG, LPTIM, PWR, RCC, RNG, RTC, SPI, TIM, USART, WWDG peripherals and additionnal Low Level Bus, System and Utilities APIs. Low Layer drivers APIs are implemented as static inline function in new Inc/stm32f7xx_ll_ppp.h files for PPP peripherals, there is no configuration file and each stm32f7xx_ll_ppp.h file must be included in user code. General updates to fix known defects and enhancements implementation Add new HAL MMC and SMBUS drivers HAL Cortex update Move HAL_MPU_Disable() and HAL_MPU_Enable() from stm32f7xx_hal_cortex.h to stm32f7xx_hal_cortex.c Clear the whole MPU control register in HAL_MPU_Disable() API HAL CRYP update Add support of AES HAL DMA update Add a check on DMA stream instance in HAL_DMA_DeInit() API HAL ETH update Fix wrong definitions in driver header file stm32f7_hal_eth.h HAL FLASH update Support OTP program operation Add the support of PCROP feature Update the clearing of error flags HAL I2C update Align driver source code with other STM32 families HAL JPEG update Update the output data management when HAL_JPEG_Pause() is performed during the last data sending HAL RCC update Enable PWR only if necessary for LSE configuration in HAL_RCC_OscConfig() API Rename RCC_LPTIM1CLKSOURCE_PCLK define to RCC_LPTIM1CLKSOURCE_PCLK1 Rename RCC_DFSDM1CLKSOURCE_PCLK define to RCC_DFSDM1CLKSOURCE_PCLK2 HAL SPI update Clear RX FIFO at the end of each transaction HAL UART update Remove USART_CR2_LINEN bit clearing when initializing in synchronous mode HAL USB update Add support of embedded USB PHY Controller Add support of Battery Charging Detector (BCD) feature LL SDMMC update Add new SDMMC_CmdSDEraseStartAdd, SDMMC_CmdSDEraseEndAdd, SDMMC_CmdOpCondition and SDMMC_CmdSwitch functions LL USB update Update PENA bit clearing in OTG_HPRT0 register The following changes done on the HAL drivers require an update on the application code based on older HAL versions HAL SD update Overall rework of the driver for a more efficient implementation Modify initialization API and structures Modify Read / Write sequences: separate transfer process and SD Cards state management Adding interrupt mode for Read / Write operations Update the HAL_SD_IRQHandler function by optimizing the management of interrupt errors Refer to the following example to identify the changes: BSP example and USB_Device/MSC_Standalone application HAL TIM update Add new AutoReloadPreload field in TIM_Base_InitTypeDef structure Refer to the TIM examples to identify the changes HAL NAND update Modify NAND_AddressTypeDef, NAND_DeviceConfigTypeDef and NAND_HandleTypeDef structures fields Add new HAL_NAND_ConfigDevice API ### V1.1.1 / 01-July-2016 Main Changes HAL DMA update Update HAL_DMA_PollForTransfer() function implementation to avoid early TIMEOUT error. HAL JPEG update Update HAL_JPEG_ConfigEncoding() function to properly set the ImageHeight and ImageWidth HAL SPI update Update SPI_DMATransmitReceiveCplt() function to properly handle the CRC and avoid conditional statement duplication ### V1.1.0 / 22-April-2016 Main Changes Official release to add the support of STM32F765xx, STM32F767xx, STM32F768xx, STM32F769xx, STM32F777xx, STM32F778xx and STM32F779xx devices General updates to fix known defects and enhancements implementation Add new HAL drivers for DFSDM, DSI, JPEG and MDIOS peripherals Enhance HAL delay and timebase implementation Add new drivers stm32f7xx_hal_timebase_tim_template.c, stm32f7xx_hal_timebase_rtc_alarm_template.c and stm32f7xx_hal_timebase_rtc_wakeup_template.c which override the native HAL time base functions (defined as weak) to either use the TIM or the RTC as time base tick source. For more details about the usage of these drivers, please refer to HAL\HAL_TimeBase examples and FreeRTOS-based applications The following changes done on the HAL drivers require an update on the application code based on HAL V1.0.4 HAL UART, USART, IRDA, SMARTCARD, SPI, I2C, QSPI (referenced as PPP here below) drivers Add PPP error management during DMA process. This requires the following updates on user application: Configure and enable the PPP IRQ in HAL_PPP_MspInit() function In stm32f7xx_it.c file, PPP_IRQHandler() function: add a call to HAL_PPP_IRQHandler() function Add and customize the Error Callback API: HAL_PPP_ErrorCallback() HAL I2C (referenced as PPP here below) drivers: Update to avoid waiting on STOPF/BTF/AF flag under DMA ISR by using the PPP end of transfer interrupt in the DMA transfer process. This requires the following updates on user application: Configure and enable the PPP IRQ in HAL_PPP_MspInit() function In stm32f7xx_it.c file, PPP_IRQHandler() function: add a call to HAL_PPP_IRQHandler() function HAL IWDG driver: rework overall driver for better implementation Remove HAL_IWDG_Start(), HAL_IWDG_MspInit() and HAL_IWDG_GetState() APIs HAL WWDG driver: rework overall driver for better implementation Remove HAL_WWDG_Start(), HAL_WWDG_Start_IT(), HAL_WWDG_MspDeInit() and HAL_WWDG_GetState() APIs Update the HAL_WWDG_Refresh(WWDG_HandleTypeDef *hwwdg, uint32_t counter) function and API by removing the "counter" parameter HAL QSPI driver: Enhance the DMA transmit process by using PPP TC interrupt instead of waiting on TC flag under DMA ISR. This requires the following updates on user application: Configure and enable the QSPI IRQ in HAL_QSPI_MspInit() function In stm32f7xx_it.c file, QSPI_IRQHandler() function: add a call to HAL_QSPI_IRQHandler() function HAL CEC driver: Overall driver rework with compatibility break versus previous HAL version Remove HAL CEC polling Process functions: HAL_CEC_Transmit() and HAL_CEC_Receive() Remove HAL CEC receive interrupt process function HAL_CEC_Receive_IT() and enable the "receive" mode during the Init phase Rename HAL_CEC_GetReceivedFrameSize() funtion to HAL_CEC_GetLastReceivedFrameSize() Add new HAL APIs: HAL_CEC_SetDeviceAddress() and HAL_CEC_ChangeRxBuffer() Remove the 'InitiatorAddress' field from the CEC_InitTypeDef structure and manage it as a parameter in the HAL_CEC_Transmit_IT() function Add new parameter 'RxFrameSize' in HAL_CEC_RxCpltCallback() function Move CEC Rx buffer pointer from CEC_HandleTypeDef structure to CEC_InitTypeDef structure HAL CAN update Add the support of CAN3 HAL CEC update Overall driver rework with break of compatibility with HAL V1.0.4 Remove the HAL CEC polling Process: HAL_CEC_Transmit() and HAL_CEC_Receive() Remove the HAL CEC receive interrupt process (HAL_CEC_Receive_IT()) and manage the "Receive" mode enable within the Init phase Rename HAL_CEC_GetReceivedFrameSize() function to HAL_CEC_GetLastReceivedFrameSize() function Add new HAL APIs: HAL_CEC_SetDeviceAddress() and HAL_CEC_ChangeRxBuffer() Remove the 'InitiatorAddress' field from the CEC_InitTypeDef structure and manage it as a parameter in the HAL_CEC_Transmit_IT() function Add new parameter 'RxFrameSize' in HAL_CEC_RxCpltCallback() function Move CEC Rx buffer pointer from CEC_HandleTypeDef structure to CEC_InitTypeDef structure Update driver to implement the new CEC state machine: Add new "rxState" field in CEC_HandleTypeDef structure to provide the CEC state information related to Rx Operations Rename "state" field in CEC_HandleTypeDef structure to "gstate": CEC state information related to global Handle management and Tx Operations Update CEC process to manage the new CEC states. Update __HAL_CEC_RESET_HANDLE_STATE() macro to handle the new CEC state parameters (gState, rxState) HAL DMA update Add new APIs HAL_DMA_RegisterCallback() and HAL_DMA_UnRegisterCallback to register/unregister the different callbacks identified by the enum typedef HAL_DMA_CallbackIDTypeDef Add new API HAL_DMA_Abort_IT() to abort DMA transfer under interrupt context The new registered Abort callback is called when DMA transfer abortion is completed Add the check of compatibility between FIFO threshold level and size of the memory burst in the HAL_DMA_Init() API Add new Error Codes: HAL_DMA_ERROR_PARAM, HAL_DMA_ERROR_NO_XFER and HAL_DMA_ERROR_NOT_SUPPORTED Remove all DMA states related to MEM0/MEM1 in HAL_DMA_StateTypeDef HAL DMA2D update Update the HAL_DMA2D_DeInit() function to: Abort transfer in case of ongoing DMA2D transfer Reset DMA2D control registers Update HAL_DMA2D_Abort() to disable DMA2D interrupts after stopping transfer Optimize HAL_DMA2D_IRQHandler() by reading status registers only once Update HAL_DMA2D_ProgramLineEvent() function to: Return HAL error state in case of wrong line value Enable line interrupt after setting the line watermark configuration Add new HAL_DMA2D_CLUTLoad() and HAL_DMA2D_CLUTLoad_IT() functions to start DMA2D CLUT loading HAL_DMA2D_CLUTLoading_Abort() function to abort the DMA2D CLUT loading HAL_DMA2D_CLUTLoading_Suspend() function to suspend the DMA2D CLUT loading HAL_DMA2D_CLUTLoading_Resume() function to resume the DMA2D CLUT loading Add new DMA2D dead time management: HAL_DMA2D_EnableDeadTime() function to enable DMA2D dead time feature HAL_DMA2D_DisableDeadTime() function to disable DMA2D dead time feature HAL_DMA2D_ConfigDeadTime() function to configure dead time Update the name of DMA2D Input/Output color mode defines to be more clear for user (DMA2D_INPUT_XXX for input layers Colors, DMA2D_OUTPUT_XXX for output framebuffer Colors) HAL DCMI update Rename DCMI_DMAConvCplt to DCMI_DMAXferCplt Update HAL_DCMI_Start_DMA() function to Enable the DCMI peripheral Add new timeout implementation based on cpu cycles for DCMI stop Add HAL_DCMI_Suspend() function to suspend DCMI capture Add HAL_DCMI_Resume() function to resume capture after DCMI suspend Update lock mechanism for DCMI process Update HAL_DCMI_IRQHandler() function to: Add error management in case DMA errors through XferAbortCallback() and HAL_DMA_Abort_IT() Optimize code by using direct register read Move the content of the stm32f7xx_hal_dcmi_ex.c/.h files to common driver files (the extension files are kept empty for projects compatibility reason) HAL FLASH update Add the support of Dual BANK feature Add __HAL_FLASH_CALC_BOOT_BASE_ADR() macro to calculate the FLASH Boot Base Adress Move Flash total sector define to CMSIS header files HAL FMC update Update FMC_NORSRAM_Init() to remove the Burst access mode configuration Update FMC_SDRAM_Timing_Init() to fix initialization issue when configuring 2 SDRAM banks HAL HCD update Update HCD_Port_IRQHandler() to be compliant with new Time base implementation HAL I2C update Add the support of I2C fast mode plus (FM+) Update Polling management: The Timeout value must be estimated for the overall process duration: the Timeout measurement is cumulative Add the management of Abort service: Abort DMA transfer through interrupt In the case of Master Abort IT transfer usage: Add new user HAL_I2C_AbortCpltCallback() to inform user of the end of abort process A new abort state is defined in the HAL_I2C_StateTypeDef structure Add the management of I2C peripheral errors, ACK failure and STOP condition detection during DMA process. This requires the following updates on user application: Configure and enable the I2C IRQ in HAL_I2C_MspInit() function In stm32f7xx_it.c file, I2C_IRQHandler() function: add a call to HAL_I2C_IRQHandler() function Add and customize the Error Callback API: HAL_I2C_ErrorCallback() Refer to the I2C_EEPROM or I2C_TwoBoards_ComDMA project examples usage of the API Add the support of I2C repeated start feature: With the following new APIs HAL_I2C_Master_Sequential_Transmit_IT() HAL_I2C_Master_Sequential_Receive_IT() HAL_I2C_Master_Abort_IT() HAL_I2C_Slave_Sequential_Transmit_IT() HAL_I2C_Slave_Sequential_Receive_IT() HAL_I2C_EnableListen_IT() HAL_I2C_DisableListen_IT() Add new user callbacks: HAL_I2C_ListenCpltCallback() HAL_I2C_AddrCallback() Several updates on HAL I2C driver to implement the new I2C state machine: Add new API to get the I2C mode: HAL_I2C_GetMode() Update I2C process to manage the new I2C states HAL IWDG update Overall rework of the driver for a more efficient implementation Remove the following APIs: HAL_IWDG_Start() HAL_IWDG_MspInit() HAL_IWDG_GetState() Update implementation: HAL_IWDG_Init() : this function insures the configuration and the start of the IWDG counter HAL_IWDG_Refresh() : this function insures the reload of the IWDG counter Refer to the following example to identify the changes: IWDG_Example HAL LPTIM update Update HAL_LPTIM_TimeOut_Start_IT() and HAL_LPTIM_Counter_Start_IT( ) APIs to configure WakeUp Timer EXTI interrupt to be able to wakeup MCU from low power mode by pressing the EXTI line Update HAL_LPTIM_TimeOut_Stop_IT() and HAL_LPTIM_Counter_Stop_IT( ) APIs to disable WakeUp Timer EXTI interrupt HAL LTDC update Update HAL_LTDC_IRQHandler() to manage the case of reload interrupt Add LTDC extension driver needed with DSI Add HAL_LTDC_SetPitch() function for pitch reconfiguration Add new callback API HAL_LTDC_ReloadEventCallback() Add HAL_LTDC_Reload() to configure LTDC reload feature Add new No Reload LTDC variant APIs HAL_LTDC_ConfigLayer_NoReload() to configure the LTDC Layer according to the specified without reloading HAL_LTDC_SetWindowSize_NoReload() to set the LTDC window size without reloading HAL_LTDC_SetWindowPosition_NoReload() to set the LTDC window position without reloading HAL_LTDC_SetPixelFormat_NoReload() to reconfigure the pixel format without reloading HAL_LTDC_SetAlpha_NoReload() to reconfigure the layer alpha value without reloading HAL_LTDC_SetAddress_NoReload() to reconfigure the frame buffer Address without reloading HAL_LTDC_SetPitch_NoReload() to reconfigure the pitch for specific cases HAL_LTDC_ConfigColorKeying_NoReload() to configure the color keying without reloading HAL_LTDC_EnableColorKeying_NoReload() to enable the color keying without reloading HAL_LTDC_DisableColorKeying_NoReload() to disable the color keying without reloading HAL_LTDC_EnableCLUT_NoReload() to enable the color lookup table without reloading HAL_LTDC_DisableCLUT_NoReload() to disable the color lookup table without reloading Note: Variant functions with “_NoReload” post fix allows to set the LTDC configuration/settings without immediate reload. This is useful in case when the program requires to modify several LTDC settings (on one or both layers) then applying (reload) these settings in one shot by calling the function “HAL_LTDC_Reload” HAL NOR update Update NOR_ADDR_SHIFT macro implementation HAL PCD update Update HAL_PCD_IRQHandler() to get HCLK frequency before setting TRDT value HAL QSPI update Update to manage QSPI error management during DMA process Improve the DMA transmit process by using QSPI TC interrupt instead of waiting loop on TC flag under DMA ISR These two improvements require the following updates on user application: Configure and enable the QSPI IRQ in HAL_QSPI_MspInit() function In stm32f7xx_it.c file, QSPI_IRQHandler() function: add a call to HAL_QSPI_IRQHandler() function Add and customize the Error Callback API: HAL_QSPI_ErrorCallback() Add the management of non-blocking transfer abort service: HAL_QSPI_Abort_IT(). In this case the user must: Add new callback HAL_QSPI_AbortCpltCallback() to inform user at the end of abort process A new value of State in the HAL_QSPI_StateTypeDef provides the current state during the abort phase Polling management update: The Timeout value user must be estimated for the overall process duration: the Timeout measurement is cumulative. Refer to the following examples, which describe the changes: QSPI_ReadWrite_DMA QSPI_MemoryMapped QSPI_ExecuteInPlace Add two new APIs for the QSPI fifo threshold: HAL_QSPI_SetFifoThreshold(): configure the FIFO threshold of the QSPI HAL_QSPI_GetFifoThreshold(): give the current FIFO threshold Fix wrong data size management in HAL_QSPI_Receive_DMA() HAL RCC update Update HAL_RCC_PeriphCLKConfig() function to adjust the SystemCoreClock Optimize HAL_RCC_ClockConfig() function code Optimize internal oscillators and PLL startup times HAL RTC update Update HAL_RTC_GetTime() with proper 'SubSeconds' and 'SecondFraction' management HAL SAI update Update SAI state in case of TIMEOUT error within the HAL_SAI_Transmit() / HAL_SAI_Receive() Update HAL_SAI_IRQHandler: Add error management in case DMA errors through XferAbortCallback() and HAL_DMA_Abort_IT() Add error management in case of IT Move SAI_BlockSynchroConfig() and SAI_GetInputClock() functions to stm32f7xx_hal_sai.c/.h files (extension files are kept empty for projects compatibility reason) HAL SPDIFRX update Overall driver update for wait on flag management optimization HAL SPI update Overall driver optimization to improve performance in polling/interrupt mode to reach maximum peripheral frequency Polling mode: Replace the use of SPI_WaitOnFlagUnitTimeout() function by "if" statement to check on RXNE/TXE flage while transferring data Interrupt mode: Minimize access on SPI registers All modes: Add the USE_SPI_CRC switch to minimize the number of statements when CRC calculation is disabled Update timeout management to check on global processes Update error code management in all processes Update DMA process: Add the management of SPI peripheral errors during DMA process. This requires the following updates in the user application: Configure and enable the SPI IRQ in HAL_SPI_MspInit() function In stm32f7xx_it.c file, SPI_IRQHandler() function: add a call to HAL_SPI_IRQHandler() function Add and customize the Error Callback API: HAL_SPI_ErrorCallback() Refer to the following example which describe the changes: SPI_FullDuplex_ComDMA HAL TIM update Update HAL_TIM_ConfigOCrefClear() function for proper configuration of the SMCR register Add new function HAL_TIMEx_ConfigBreakInput() to configure the break input source HAL UART, USART, SMARTCARD and IRDA (referenced as PPP here below) update Update Polling management: The user Timeout value must be estimated for the overall process duration: the Timeout measurement is cumulative Update DMA process: Update the management of PPP peripheral errors during DMA process. This requires the following updates in user application: Configure and enable the PPP IRQ in HAL_PPP_MspInit() function In stm32f7xx_it.c file, PPP_IRQHandler() function: add a call to HAL_PPP_IRQHandler() function Add and customize the Error Callback API: HAL_PPP_ErrorCallback() HAL WWDG update Overall rework of the driver for more efficient implementation Remove the following APIs: HAL_WWDG_Start() HAL_WWDG_Start_IT() HAL_WWDG_MspDeInit() HAL_WWDG_GetState() Update implementation: HAL_WWDG_Init() A new parameter in the Init Structure: EWIMode HAL_WWDG_MspInit() HAL_WWDG_Refresh() This function insures the reload of the counter The "counter" parameter has been removed HAL_WWDG_IRQHandler() HAL_WWDG_EarlyWakeupCallback() is the new prototype of HAL_WWDG_WakeupCallback() Refer to the following example to identify the changes: WWDG_Example ### V1.0.4 / 09-December-2015 Main Changes HAL Generic update Update HAL weak empty callbacks to prevent unused argument compilation warnings with some compilers by calling the following line: UNUSED(hppp); HAL ETH update Update HAL_ETH_Init() function to add timeout on the Software reset management ### V1.0.3 / 13-November-2015 Main Changes General updates to fix known defects and enhancements implementation One change done on the HAL CRYP requires an update on the application code based on HAL V1.0.2 Update HAL_CRYP_DESECB_Decrypt() API to invert pPlainData and pCypherData parameters HAL Generic update Update HAL weak empty callbacks to prevent unused argument compilation warnings with some compilers by calling the following line: UNUSED(hppp); Remove references to STM32CubeMX and MicroXplorer from stm32f7xx_hal_msp_template.c file HAL ADC update Replace ADC_CHANNEL_TEMPSENSOR definition from ADC_CHANNEL_16 to ADC_CHANNEL_18 Update HAL ADC driver state machine for code efficiency Add new literal: ADC_INJECTED_SOFTWARE_START to be used as possible value for the ExternalTrigInjecConvEdge parameter in the ADC_InitTypeDef structure to select the ADC software trigger mode. HAL CORTEX update Remove duplication for __HAL_CORTEX_SYSTICKCLK_CONFIG() macro HAL CRYP update Update HAL_CRYP_DESECB_Decrypt() API to fix the inverted pPlainData and pCypherData parameters issue HAL FLASH update Update OB_IWDG_STOP_ACTIVE definition Update OB_RDP_LEVEL_x definition by proper values Update FLASH_MassErase() function to consider the voltage range parameter in the mass erase configuration HAL RCC update update values for LSE Drive capability defines update PLLN min value 50 instead of 100 add RCC_PLLI2SP_DIVx defines for PLLI2SP clock divider Update __HAL_RCC_USB_OTG_FS_CLK_DISABLE() macro to remove the disable of the SYSCFG Update HAL_RCCEx_GetPeriphCLKFreq() function for proper SAI clock configuration HAL SAI update update for proper management of the external synchronization input selection update of HAL_SAI_Init () funciton update definition of SAI_Block_SyncExt and SAI_Block_Synchronization groups update SAI_SLOTACTIVE_X defines values update HAL_SAI_Init() function for proper companding mode management update SAI_Transmit_ITxxBit() functions to add the check on transfer counter before writing new data to SAIx_DR registers update SAI_FillFifo() function to avoid issue when the number of data to transmit is smaller than the FIFO size update HAL_SAI_EnableRxMuteMode() function for proper mute management update SAI_InitPCM() function to support 24bits configuration HAL SD update update HAL_SD_Get_CardInfo() to properly support high capacity cards HAL SPDIFRX update update SPDIFRX_DMARxCplt() function implementation to check on circular mode before disabling the DMA HAL TIM update Update HAL_TIM_ConfigClockSource() function implementation for proper parameters check HAL UART update Update __HAL_UART_CLEAR_IT macro for proper functionning ll FMC update add FMC_PAGE_SIZE_512 define ll SDMMC update update SDMMC_SetSDMMCReadWaitMode() function for proper functionning ### V1.0.2 / 21-September-2015 Main Changes HAL Generic update stm32f7xx_hal.conf_template.h: update HSE_STARTUP_TIMEOUT stm32f7xx_hal_def.h: update the quotation marks used in #error"USE_RTOS should be 0 in the current HAL release" HAL DMA update Overall driver update for code optimization add StreamBaseAddress and StreamIndex new fields in the DMA_HandleTypeDef structure add DMA_Base_Registers private structure add static function DMA_CalcBaseAndBitshift() update HAL_DMA_Init() function to use the new added static function update HAL_DMA_DeInit() function to optimize clear flag operations update HAL_DMA_Start_IT() function to optimize interrupts enable update HAL_DMA_PollForTransfer() function to optimize check on flags update HAL_DMA_IRQHandler() function to optimize interrupt flag management HAL ETH update remove duplicated macro IS_ETH_RX_MODE() HAL GPIO update Rename GPIO_SPEED_LOW define to GPIO_SPEED_FREQ_LOW Rename GPIO_SPEED_MEDIUM define to GPIO_SPEED_FREQ_MEDIUM Rename GPIO_SPEED_FAST define to GPIO_SPEED_FREQ_HIGH Rename GPIO_SPEED_HIGH define to GPIO_SPEED_FREQ_VERY_HIGH HAL HASH update Rename HAL_HASH_STATETypeDef to HAL_HASH_StateTypeDef Rename HAL_HASH_PhaseTypeDef to HAL_HASHPhaseTypeDef HAL RCC update update values for LSE Drive capability defines update PLLN/PLLI2SN/PLLSAI VCO min value 100MHz instead of 192MHz add __HAL_RCC_MCO1_CONFIG() and __HAL_RCC_MCO2_CONFIG() macros update HAL_RCCEx_PeriphCLKConfig() function to reset the Backup domain only if the RTC Clock source selection is modified HAL TIM update update the implementation of __HAL_TIM_SET_COMPARE() macro remove useless assert() in HAL_TIM_PWM_ConfigChannel(), TIM_OC2_SetConfig() and HAL_TIM_PWM_ConfigChannel() functions HAL CAN update add the clear flag ERRI bit in HAL_CAN_IRQHandler() HAL I2S update update I2S HAL_I2S_Transmit() API to keep the check on busy flag only for the slave HAL QSPI update Add __HAL_QSPI_CLEAR_FLAG() before QSPI_Config() HAL UART update Remove enabling of ERR IT source and PE source from HAL_UART_Transmit_IT() and remove the corresponding disabling ERR/PE IT from UART_EndTransmit_IT() HAL PCD update Clean status phase received interrupt when DMA mode enabled HAL HCD update Update to use local variable in USB Host channel re-activation ll FMC update update the define FMC Write FIFO Disable/Enable: FMC_WRITE_FIFO_DISABLE and FMC_WRITE_FIFO_ENABLE remove return HAL_ERROR from FMC_SDRAM_SendCommand() function ### V1.0.1 / 25-June-2015 Main Changes General updates to fix known defects and enhancements implementation HAL CRC update update __HAL_CRC_SET_IDR() macro implementation to use WRITE_REG() instead of MODIFY_REG() HAL CEC update update timeout management in HAL_CEC_Transmit() and HAL_CEC_Receive() functions HAL Cortex update update HAL_MPU_ConfigRegion() function to be misra compliant HAL ETH update Remove duplicated IS_ETH_DUPLEX_MODE() and IS_ETH_RX_MODE() macros Remove illegal space ETH_MAC_READCONTROLLER_FLUSHING macro Update ETH_MAC_READCONTROLLER_XXX defined values (XXX can be IDLE, READING_DATA and READING_STATUS) HAL FLASH update update FLASH_OB_GetRDP() function to return uint8_t instead of FlagStatus update OB_RDP_LEVELx definition add __HAL_FLASH_GET_LATENCY() macro HAL HASH update update HASH_DMAXferCplt() and HASHEx_DMAXferCplt() functions to properly configure the number of valid bits in last word of the message update HAL_HASH_SHA1_Accumulate() function to check on the length of the input buffer update HAL_HASH_MODE_Start_IT() functions (Mode stands for MD5, SHA1, SHA224 and SHA256 ) to : Fix processing fail for small input buffers to unlock the process and call return HAL_OK at the end of HASH processing to avoid incorrect repeating software properly to manage the HashITCounter efficiency Update to call the HAL_HASH_InCpltCallback() at the end of the complete buffer instead of every each 512 bits update HASH_IT_DINI and HASH_IT_DCI definition update __HAL_HASH_GET_FLAG() macro definition HAL I2S update update HAL_I2S_Transmit() function to ensure the waiting on Busy flag in case of slave mode selection HAL RTC update update HAL_RTCEx_SetWakeUpTimer() and HAL_RTCEx_SetWakeUpTimer_IT() functions to properly check on WUTWF flag rename RTC_TIMESTAMPPIN_PI8 define to RTC_TIMESTAMPPIN_POS1 rename RTC_TIMESTAMPPIN_PC1 define to RTC_TIMESTAMPPIN_POS2 update __HAL_RTC_WAKEUPTIMER_CLEAR_FLAG() macro definition update __HAL_RTC_TAMPER_GET_IT() macro definition update __HAL_RTC_TAMPER_CLEAR_FLAG() macro definition update __HAL_RTC_TIMESTAMP_CLEAR_FLAG() macro definition update __HAL_RTC_TAMPER_TIMESTAMP_EXTI_GET_FLAG() macro definition add RTC_TAMPCR_TAMPXE and RTC_TAMPCR_TAMPXIE defines HAL SMARTCARD update add SMARTCARD_FLAG_IDLE, SMARTCARD_IT_IDLE and SMARTCARD_CLEAR_IDLEF defines HAL UART update update HAL_UART_DMAResume() function to clear overrun flag before resuming the Rx transfer update UART_FLAG_SBKF definition HAL USART update update HAL_USART_DMAResume() function to clear overrun flag before resuming the Rx transfer LL FMC update update NAND timing maximum values LL USB update USB_FlushTxFifo API: update to flush all Tx FIFO Update to use local variable in USB Host channel re-activation ### V1.0.0 / 12-May-2015 Main Changes First official release for STM32F756xx/746xx/745xx devices ## License Redistribution and use in source and binary forms, with or without modification, are permitted provided that the following conditions are met: Redistributions of source code must retain the above copyright notice, this list of conditions and the following disclaimer. Redistributions in binary form must reproduce the above copyright notice, this list of conditions and the following disclaimer in the documentation and/or other materials provided with the distribution. Neither the name of STMicroelectronics nor the names of its contributors may be used to endorse or promote products derived from this software without specific prior written permission. THIS SOFTWARE IS PROVIDED BY THE COPYRIGHT HOLDERS AND CONTRIBUTORS "AS IS" AND ANY EXPRESS OR IMPLIED WARRANTIES, INCLUDING, BUT NOT LIMITED TO, THE IMPLIED WARRANTIES OF MERCHANTABILITY AND FITNESS FOR A PARTICULAR PURPOSE ARE DISCLAIMED. IN NO EVENT SHALL THE COPYRIGHT HOLDER OR CONTRIBUTORS BE LIABLE FOR ANY DIRECT, INDIRECT, INCIDENTAL, SPECIAL, EXEMPLARY, OR CONSEQUENTIAL DAMAGES (INCLUDING, BUT NOT LIMITED TO, PROCUREMENT OF SUBSTITUTE GOODS OR SERVICES; LOSS OF USE, DATA, OR PROFITS; OR BUSINESS INTERRUPTION) HOWEVER CAUSED AND ON ANY THEORY OF LIABILITY, WHETHER IN CONTRACT, STRICT LIABILITY, OR TORT (INCLUDING NEGLIGENCE OR OTHERWISE) ARISING IN ANY WAY OUT OF THE USE OF THIS SOFTWARE, EVEN IF ADVISED OF THE POSSIBILITY OF SUCH DAMAGE. For complete documentation on STM32 Microcontrollers visit www.st.com/STM32