| Connectivity Middleware Utilities Library

Macros
generic middleware results/error codes
Common middleware utilities » Middleware utilities enumerated types

## General Description

List of all the generic result/error codes defined by the connectivity-utilities library.

## Macros
#define | CY_RSLT_MODULE_MW_ERR_CODE_START (0)
| Generic middleware error code start.
#define | CY_RSLT_MW_ERR_BASE CY_RSLT_CREATE(CY_RSLT_TYPE_ERROR, CY_RSLT_MODULE_MW_BASE, CY_RSLT_MODULE_MW_ERR_CODE_START)
| Generic middleware base error code.
#define | CY_RSLT_MW_ERROR ( CY_RSLT_MW_ERR_BASE + 1 )
| Generic middleware error.
#define | CY_RSLT_MW_TIMEOUT ( CY_RSLT_MW_ERR_BASE + 2 )
| Generic middleware timeout.
#define | CY_RSLT_MW_BADARG ( CY_RSLT_MW_ERR_BASE + 3 )
| Generic middleware bad argument.
#define | CY_RSLT_MW_OUT_OF_HEAP_SPACE ( CY_RSLT_MW_ERR_BASE + 4 )
| Generic middleware out of heap memory.
#define | CY_RSLT_MW_PENDNG ( CY_RSLT_MW_ERR_BASE + 5 )
| Generic middleware pending operation.
#define | CY_RSLT_MW_UNSUPPORTED ( CY_RSLT_MW_ERR_BASE + 6 )
| Generic middleware unsupported method.
#define | CY_RSLT_MW_BUFFER_UNAVAIL_TEMPORARILY ( CY_RSLT_MW_ERR_BASE + 7 )
| Generic middleware buffer unavailable.